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REVIEW OF MONITORING AND ASSESSMENT AT POETON CARDIFF 2016
This review is undertaken to comply with condition 4.2.2(a) of our environmental permit no. BP1772IZ. The review covers the past six years.
The review shows the increase in workforce, production, the hours the factory is open and the associated increase in water and energy use.  The increase in work has continued over the last year. The new extension has been built and the relocation of the paint shop and non-destructive testing (NDT) departments is nearly complete. The area that was occupied by aforementioned departments is being used to expand the anodising department and set up a cell for our Airbus work which is continuing to increase. 
Over the  year  we have again seen an increase the amount of work being processed which has led to an increase in the number of employees (Table 1) and in the number of hours the factory is open (Table 2).
To accommodate the increased demand for our services the number of employees has increased from 27 in 2010 to 83 in 2015 and to 94 in 2016. We are continuing to operate a 3 shift system in the week plus a weekend shift. The number of hours the factory operates annually has increased from 2160 hours in 2010 to 6143 hours in 2015 and to 6681 in 2016. 
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As a combination of increase in the amount of parts processed by an increased number of staff the energy usage has also risen (Table 3).
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The energy use increased in 2016 due to the extension being built and heated and also the new paint facility has internal temperature control to help with quality. As well as this we have installed 2 paint curing ovens and 2 de-embrittlement ovens to improve our ability to handle the increased work load.
 Water usage (Table 4) has increased over the last year. This is an area where we are trying to reduce consumption. The water meter allows us to monitor use better than before and we are introducing a monitoring system to ensure the flow restrictor valves are working satisfactorily. We are also making new operators aware of the importance of controlling water usage.  


[image: image5.png]WATER

2010

2011

2012 2013

JI”IIE

2014 2015 2016





Waste transferred from our site (Table 5) varies greatly from year to year as some of it is dependent on whether or not any of our tanks need to be completely emptied and changed (tank contents are removed by tanker lorry), as well as other variable factors such as production demands.  2016 waste levels return to more normal levels after the exceptionally high level of 2015. 
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 We already segregate our waste in to several different streams and we are always looking for ways to minimise waste, for example plastic drums that were previously sent to landfill are now sent for recycling. We already compress some of our waste and following a successful trial of a cardboard and plastics baler it is likely that we will invest in a permanent machine.
Discharge of cadmium (Table 6) has increased in 2016 due to increasing production.  The discharge figure is obtained from the analysis of the effluent and the total water used. As the analysis is close to detection limits the water usage has an effect on the final result.  Which is why we are working to reduce water consumption.
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Fugitive emissions did not alter in 2016. The relocation of the paint spray area has also entailed moving the discharge points and a further extraction point for the Liquid Penetrant Inspection (LPI) has been added. In line with the requirements of our revised permit the new and altered discharge points have been tested the results show the discharge is trivial. The results were sent to NWR
Chris Rochelle

Technical Manager

Feb 2017
4.2.2 Performance and activities report Poeton (Cardiff) Ltd
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