Maxibrite Ltd VP3132LJ – PC 4.2.1a

Annual Environmental Impact Review and Reporting Commitments For Calendar Year 2014 – Comparison With Original Environmental Impact Data Included In IPPC Permit Application 
[annual briquette production = 59,912 tonnes for calendar year 2014]

Report reviewing the results of the monitoring and assessment carried out in accordance with the permit against the relevant assumptions, parameters and results in the assessment of the impact of the emissions submitted with the application.

 Releases to Air

It is assumed that release points to air (other than A9 and A1) have not changed significantly since the permit application. A9 release point has shown average particulate release concentrations of 6.96mg/m3. This result is considerably less than the application assumption of 45mg/m3. Therefore, the environmental impact of the measured A9 emissions in 2014 was significantly less than the predicted impact included in the application.
Permit Release Point A1 (Main Stack)

When reviewing the main stack emissions data for the four quarters of 2014, it was found that the average emissions in mg/m3 for Particulate matter, SO2, NOx and ammonia for the year were significantly below the ‘worst case’ assumed concentrations in the ADMS modelling study included in the permit application. 
In addition, the average annual normalised main stack flow was significantly lower than the worst case flow figure used in the application assumptions. This confirms that the overall environmental impact for all main stack emissions in 2014 was considerably less than the predicted impact included in the original PPC permit application.

Releases to Water
Releases to the Mwyndy Brook Via W1

The environmental impact to the Brook will have reduced in 2014 when compared to the permit application assumptions, due to the installation of the new effluent filter press, along with the increased use of recycled water on site. The effluent filter press installation has reduced the overall suspended solids levels discharged, thereby lowering the environmental impact to the Brook. The new systems were not in place at the time of the original application, so the environmental impact to controlled waters must now be reduced in comparison to the original application systems. 
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