Permit Reference Number : BX3376IG




Operator : Continental UK Teves Limited
Installation : Continental UK Teves Limited




Form Number : S1
Reporting of Emissions to Sewer for the period from ……01-01-2014…………….to……31-12-2014
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Accreditation/ Certification [4]
	Uncertainty
[5]

	S1
	pH
	6-11
	N/A
	Plant & Lab Meters
	N/A
	N/A
	N/A

	S1
	Chromium and its compounds
	1mg/l
	N/A
	N/A Atomic Absorption
	N/A
	N/A
	N/A

	S1
	Zinc and its compounds
	2mg/l
	N/A
	N/A Atomic Absorption
	N/A
	N/A
	N/A

	S1
	Cadmium and its compounds
	0.01 mg/l
	0.01mg/l
	Yearly average/dilution
	1st Jan 2014 – 31st Dec 2014
	N/A
	N/A

	S1
	Mercury and its compounds
	0.005 mg/l
	0.001mg/l
	Yearly average/dilution
	1st Jan 2014 – 31st Dec 2014
	N/A
	N/A

	S1
	Cadmium and its compounds
	0.60 kg
	0.13kg
	Mass Balance Calculation
	1st Jan 2014 – 31st Dec 2014
	N/A
	N/A

	S1
	Mercury and its compounds
	0.12 kg
	0.0012kg
	Mass Balance Calculation
	1st Jan 2014 – 31st Dec 2014
	N/A
	N/A

	S1
	Total flow
	N/A
	 10,948 m3
	N/A Ultrasonic Flow Meter at Outfall
	1st Jan 2014 – 31st Dec 2014
	M/CERTS
	3.48%


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   
[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.
[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 
Signed …[image: image1.png]


…………………………….  

Date 21/01/2015……………..



(authorised to sign as representative of the Operator)                      
Permit Reference Number : BX3376IG




Operator : Continental UK Teves Limited
Installation : Continental UK Teves Limited




Form Number : E1
Reporting of Energy Usage for the year …2014……………………….
	Energy Source
	Energy Usage
	CO2
Produced
(tonnes)
	
	Trends in Energy Usage

	
	Quantity
	Primary Energy
(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy usage
	CO2
 produced

	
	
	
	
	
	
	
	

	
	
	
	
	
	2011
	2,280
	1,196

	Electricity *
	MWh
	3,566
	1,853
	
	2012
	2,768
	1,452

	Gas
	tonnes
	Nil
	Nil
	
	2013
	3,460
	1,815

	
	
	
	
	
	2014
	3,566
	1,853

	
	
	
	
	
	2015
	
	

	
	
	
	
	
	2016
	
	

	TOTAL
	-
	3,566
	1,853
	
	2017
	
	

	
	
	
	
	
	2018
	
	


* Conversion factor for delivered electricity to primary energy = 2.4
	Operator’s comments : 


Signed …[image: image2.png]


………………………….  

Date: …21/01/2015………..



(authorised to sign as representative of the Operator)
Permit Reference Number : BX3376IG




Operator : Continental UK Teves Limited
Installation : Continental UK Teves Limited




Form Number : R1
Reporting of Waste Disposal and Recovery for the year …2014…………………….
	Waste
Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes
	Tonnes
	
	Year
	Parameter

	
	
	
	
	
	
	Waste 1
	Waste 2
	Total Hazardous Waste (Tonnes)

	(1) Non-Filter Cake Waste
	External treatment/land fill
	24.223
	Nil
	
	2005
	266
	145.5
	411.5

	(2) Filter Cake
	Landfill
	59.6
	Nil
	
	2006
	273
	202
	475

	Total hazardous waste
	
	
	
	
	2007
	106.40
	141.78
	248.18

	
	
	
	
	
	2008
	30
	79
	109

	TOTAL WASTE
	-
	83.828
	
	
	2009
	45.16
	9.34
	54.5

	
	
	
	
	
	2010
	3.79
	36.56
	40.35

	
	
	
	
	
	2011
	51.86
	26.60
	78.46

	
	
	
	
	
	2012
	51.074
	42.040
	93.114

	
	
	
	
	
	2013
	35.14
	41.06
	76.2

	
	
	
	
	
	2014
	24.223
	59.5
	83.828

	
	
	
	
	
	2015
	
	
	


	Operator’s comments : 



Signed …[image: image3.png]


…………………………………….  

Date: 21/01/2015…………..



(authorised to sign as representative of the Operator)
Permit Reference Number : BX3376IG




Operator : Continental UK Teves Limited
Installation : Continental UK Teves Limited
Ebbw Vale



Form Number : WU1
Reporting of Water Usage for the year 2014……………………….
	Water Source
	Usage
(m3)
	
	
	
	
	Trends in Water Usage

	
	
	
	
	
	
	Year
	Parameter

	Mains Water supply
	   10,948        m3
	
	
	
	
	
	Named 
Water source
	Total 
Water usage
	Water per unit output

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	2005
	Mains water
	31002
	3.4 litres

	
	
	
	
	
	
	2006
	Mains water
	50244
	5.3 litres

	
	
	
	
	
	
	2007
	Mains water
	46543
	6 litres

	
	
	
	
	
	
	2008
	Mains water
	35557
	7 litres

	TOTAL WATER USAGE
	10,948       m3
	
	
	
	
	2009
	Mains water
	6475
	7 litres

	
	
	
	
	
	
	2010
	Mains water
	6337
	7 litres

	
	
	
	
	
	
	2011
	Mains water
	8,597
	8  litres

	
	
	
	
	
	
	2012
	Mains water
	8,427
	7 litres

	
	
	
	
	
	
	2013
	Mains water
	10,056
	7 litres

	
	
	
	
	
	
	2014
	Mains water
	10,948
	6.9 litres

	
	
	
	
	
	
	2015
	
	
	


	Operator’s comments : 


Signed …[image: image4.png]


………………………………….  

Date…21/01/2015………..



(authorised to sign as representative of the Operator)
Permit Reference Number : BX3376IG




Operator : Continental UK Teves Limited
Installation : Continental UK Teves Limited
Ebbw Vale

2014

Form Number : MR1
	Mass Release 
	
	Trends in Mass Release 

	Parameter
	Limit
	kg
	
	

	
	
	
	
	Year
	Parameter

	Cadmium and its compounds
	0.60 kg
	0.13kg
	
	
	Mercury
	Cadmium
	

	Mercury and its compounds
	0.12 kg
	0.0012kg
	
	2005
	0.014
	0.025
	

	
	
	
	
	2006
	0.085
	0.46
	

	
	
	
	
	2007
	0.055
	0.375
	

	
	
	
	
	2008
	0.04
	0.60
	

	
	
	
	
	2009
	0.013
	0.051
	

	
	
	
	
	2010
	0.013
	0.044
	

	
	
	
	
	2011
	0.013
	0.044
	

	
	
	
	
	2012
	0.013
	0.044
	

	
	
	
	
	2013
	0.02
	0.13
	

	
	
	
	
	2014
	0.0012
	0.13
	

	
	
	
	
	2015
	
	
	


	Operator’s comments : Results obtained via mass balance.



Signed ……[image: image5.png]


……………………………………………………….  

Date …21/01/2015……………..



(authorised to sign as representative of the Operator)
