Permit Number: 	EPR/EP3830GH			Operator: 		Liberty Steel UK Ltd

Facility:		Liberty Steel Newport		Form Number: 	 Air1 / 15/08/2016
Reporting of emissions to air for the period from 08/03/2016 to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	
Particulate Matter

	5 mg/m3
	Daily Average
	
	BS ISO 10155
	
	

	A1
	VOC as Total Organic Carbon (TOC)
	20 mg/m3
	1 hour period
	
	BS EN 12619
	
	

	A1
	Carbon  monoxide
	100 mg/m3
	Hourly Average
	
	ISO 12039
	
	

	
	
	
	
	
	
	
	

	A1
	Sulphur dioxide
	25 mg/m3
	15 minute average
	
	BS6069:Section 4.4:1993 (ISO 7935:1992)
	
	

	
	
	
	
	
	
	
	

	A1
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	25 mg/m3
	Spot sample
	
	ISO 10849
	
	

	
	
	
	
	
	
	
	

	A1
	PCDD/F
	0.1ng/m3
	6 – 8h random samples during steady state conditions

	
	BS EN 1948
	
	

	A1
	Mercury and its compounds

	0.05 mg/m3
	Spot samples for at least 4 hours
	
	BS EN 13649
	
	


	A1
	Metals
	
	

	
	USEPA method 29 or BS EN 14385
	
	

	A1 
	
PAH

	
	
	
	BS EN 1948
	
	

	A1
	
PCB

	
	
	
	BS EN 1948
	
	

	A2
	
Particulate Matter

	5 mg/m3
	Daily Average
	
	BS ISO 10155
	
	

	A2
	VOC as Total Organic Carbon (TOC)
	20 mg/m3
	1 hour period
	
	BS EN 12619
	
	

	A2
	
Carbon  monoxide
	100 mg/m3
	Hourly Average
	
	ISO 12039
	
	

	A2
	
Sulphur dioxide

	25 mg/m3
	15 minute average
	
	BS6069:Section 4.4:1993 (ISO 7935:1992)
	
	

	A2
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	25 mg/m3
	Spot sample
	
	ISO 10849
	
	

	A2
	PCDD/F
	0.1ng/m3
	6 – 8h random samples during steady state conditions

	
	BS EN 1948
	
	

	A2
	Mercury and its compounds

	0.05 mg/m3
	Spot samples for at least 4 hours
	
	BS EN 13649
	
	


	A2
	Metals
	
	

	
	USEPA method 29 or BS EN 14385
	
	

	A2 
	
PAH

	
	
	
	BS EN 1948
	
	

	A2
	
PCB

	
	
	
	BS EN 1948
	
	

	A5
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	400 mg/m3
	Spot
	
	ISO 10849
	
	




[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	

Permit Number: 	EPR/EP3830GH			Operator: 		Liberty Steel UK Ltd

Facility:		Liberty Steel Newport		Form Number: 	Water1 / 15/08/2016
Reporting of emissions to water (other than to sewer) and land for the period from 08/03/2016 to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1
	Total suspended solids
	20 mg/l
	Spot Sample
	
	BS EN 872:1996 or other ISO, BS or SCA blue book method as approved by Natural Resources Wales
	
	

	W1
	Total Hydrocarbons
	5 mg/l
	Spot Sample
	
	SCA blue book 77 ISBN 0117517283 2002 or other ISO, BS or SCA blue book method as approved by Natural Resources Wales
	
	

	W1
	pH
	6-10
	Spot Sample
	
	BS 6068-2.50:1995 (ISO 10523:1994)
	
	

	W1
	Lead
	0.1 mg/l
	Spot Sample
	
	BS 6068-2.60:1998, 
BS EN ISO 11885 1998
	
	

	W1
	Arsenic
	0.1 mg/l
	Spot Sample
	
	BS 6068-2.60:1998, 
BS EN ISO 11885 1998
	
	

	W1
	Cadmium
	0.05 mg/l
	Spot Sample
	
	BS 6068-2.60:1998, 
BS EN ISO 11885 1998
	
	

	W1
	Chromium
	0.2 mg/l
	Spot Sample
	
	BS 6068-2.60:1998, 
BS EN ISO 11885 1998
	
	

	W1
	Nickel
	0.1 mg/l
	Spot Sample
	
	BS 6068-2.60:1998, 
BS EN ISO 11885 1998
	
	

	W1
	Copper
	0.1 mg/l
	Spot Sample
	
	BS 6068-2.60:1998, 
BS EN ISO 11885 1998
	
	

	W1
	Mercury
	-
	Spot Sample
	
	BS 6068-2.60:1998, 
BS EN ISO 11885 1998
	
	

	W1
	Iron
	5 mg/l
	Spot Sample
	
	BS 6068-2.74:2002, 
BS EN ISO 13506:2002
	
	

	W1
	Zinc
	0.5 mg/l
	Spot Sample
	
	BS 6068-2.60:1998,
BS EN ISO 11885 1998
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] Metal include elements and compounds of Pb, As, Cd, Cr, Ni, Cu, Hg and Zn expressed as the metal and shall be individually reported


Signed …………………………………………………………….  		Date………………………..





Permit Number: 	EPR/EP3830GH			Operator: 		Liberty Steel UK Ltd

Facility:		Liberty Steel Newport		Form Number: 	WaterUsage1 / 15/08/2016

Reporting of Water Usage for the year 2016

	Water Source
	Usage
(m3/year)
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	Site borehole
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	
Permit Number: 	EPR/EP3830GH			Operator: 		Liberty Steel UK Ltd

Facility:		Liberty Steel Newport		Form Number: 	Energy1 / 15/08/2016

Reporting of Energy Usage for the year 2016

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	

Permit Number: 	EPR/EP3830GH			Operator: 		Liberty Steel UK Ltd

Facility:		Liberty Steel Newport		Form Number: 	Performance1 / 15/08/2016

Reporting of other performance indicators for the period 08/03/2016 to DD/MM/YYYY

	Parameter
	
	Quantity (tonnes)
	

	
	
	
	

	Total raw materials used 
	
	

	Total Product Produced
	
	

	Total Waste produced
	
	

	Total amount of SRF stored on-site
	
	

	Total amount of RDF stored on-site
	
	

	Total amount of ASR stored on-site
	
	

	Total amount of End of life tyres stored on-site
	
	

	Total amount of Scrap metal stored on-site
	
	

	Total amount of Waste plastics stored on-site
	
	

	
	
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	

Permit Number: 	EPR/EP3830GH			Operator: 		Liberty Steel UK Ltd

Facility:		Liberty Steel Newport		Form Number: 	 Particulate1 / 15/08/2016

Reporting of particulates for the period from 08/03/2016 to DD/MM/YYYY 

	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Particulate Matter
	 5 mg/m3
	
	
	BS EN 13284-1:2002
	
	

	
A2

	Particulate Matter
	 5 mg/m3
	
	
	BS EN 13284-1:2002
	
	




[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] [bookmark: _GoBack]For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
