Permit Reference Number: NP3030BJ
Operator: EnerSys Ltd
Installation: EnerSys Newport
Form Number: A1
Reporting of Emissions to Air for the period from …July 1st 2015………………………….to…September 30th 2015…………………………

	Emissions to Air

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value (Annual) [6]
	Spot Limit Values [6]
	Spot Result[1]
	Process run time
	Quarter Result [7]
	Test Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A1
	Lead
	1.0 mg/m3 
	1.0 mg/m3 
	N/R
	0
	N/R
	BS EN 14385:2004
	N/A
	MCERTS

UKAS 0934
	N/A

	Mill 1
	
	
	
	N/R
	0
	
	BS EN 14385:2004
	N/A
	MCERTS

UKAS 0934
	N/A

	
	
	
	
	N/R
	0
	
	BS EN 14385:2004
	N/A
	MCERTS

UKAS 0934
	N/A

	A2
	Lead  
	1.0 mg/m3 
	1.0 mg/m3
	0.04
	309
	0.064
	BS EN 14385:2004
	06/07/2015
13:10-13:58
	MCERTS

UKAS 0934
	<0.01

	Mill 2
	
	
	
	0.22
	507
	
	BS EN 14385:2004
	03/08/2015
12:25-13:01
	MCERTS

UKAS 0934
	+/-0.03

	
	
	
	
	0.03
	657
	
	BS EN 14385:2004
	22/09/2015
11:00-11:36
	MCERTS

UKAS 0934
	<0.01

	A3
	Lead
	1.0 mg/m3 
	1.0 mg/m3 
	0.14
	265
	0.178
	BS EN 14385:2004
	01/07/2015
11:30-12:10
	MCERTS

UKAS 0934
	+/-0.02

	Mill 3
	
	
	
	0.58
	528
	
	BS EN 14385:2004
	03/08/2015
11:05-11:45
	MCERTS

UKAS 0934
	+/-0.07

	
	
	
	
	0.27
	396
	
	BS EN 14385:2004
	01/09/2015
11:08-11:48
	MCERTS

UKAS 0934
	+/-0.03

	A63
	Lead
	1.0 mg/m3 
	1.0 mg/m3 
	0.32
	318
	0.100
	BS EN 14385:2004
	01/07/2015

12:35-13:18
	MCERTS

UKAS 0934
	+/-0.04

	Mill4
	
	
	
	0.02
	633
	
	BS EN 14385:2004
	04/08/2015
10:51-11:41
	MCERTS

UKAS 0934
	<0.01

	
	
	
	
	0.09
	593
	
	BS EN 14385:2004
	01/09/2015
12:12-13:00
	MCERTS

UKAS 0934
	+/-0.01


	Emission

Point
	Substance /

Parameter
	Emission

Limit Value (Annual) [6]
	Spot Limit Values [6]
	Spot Result[1]
	Process run time
	Quarter Result [7]
	Test Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A4
	Lead
	0.25 mg/m3 
	0.25 mg/m3
	0.22
	719
	0.072
	BS EN 14385:2004
	06/07/2015
15:20-16:00
	MCERTS

UKAS 0934
	+/-0.03

	A6
	Lead
	0.30 mg/m3 [6]
	1.5 mg/m3 
	0.10
	1526
	0.069
	BS EN 14385:2004
	02/07/2015
10:45-11:25
	MCERTS

UKAS 0934
	+/-0.01

	A8
	Lead
	0.20 mg/m3 [6]
	1.5 mg/m3]
	0.05
	1781
	0.040
	BS EN 14385:2004
	01/07/2015
15:20-16:00
	MCERTS

UKAS 0934
	<0.01

	A9
	Lead
	0.20 mg/m3 [6]
	0.75 mg/m3 
	0.02
	1701
	0.015
	BS EN 14385:2004
	06/07/2015
11:40-12:22
	MCERTS

UKAS 0934
	<0.01

	A10
	Lead
	0.20 mg/m3 [6]
	1.0 mg/m3 
	0.06
	1915
	0.052
	BS EN 14385:2004
	03/07/2015
14:00-14:54
	MCERTS

UKAS 0934
	<0.01

	A11
	Lead
	0.15mg/m3 (6)
	0.75mg/m3
	0.02
	1853
	0.017
	BS EN 14385:2004
	02/07/2015
12:10-12:52
	MCERTS

UKAS 4279
	<0.01

	A12
	Lead
	0.15 mg/m3 [6]
	0.75 mg/m3 
	0.09
	1662
	0.068
	BS EN 14385:2004
	02/07/2015
14:45-15:49
	MCERTS

UKAS 0934
	+/-0.01

	A13
	Lead
	0.4 mg/m3 [6]
	1.0 mg/m3
	0.05
	1897
	0.043
	BS EN 14385:2004
	03/07/2015
11:45-12:25
	MCERTS

UKAS 0934
	<0.01


 [1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

[6] The emission limit value is expressed as a maximum individual value and corrected to 273K, 101.3kPa.

[7] To be calculated pro rata according to run time.

Signed ………[image: image1.emf]

…(authorised to sign as representative of the Operator)…  

Date…23/10/2015……………..   


Permit Reference Number: NP3030BJ
Operator: Enersys Ltd
Installation: Enersys Newport
Form Number: A2

Reporting of Emissions to Air for the period from … July 1st 2015………………………….to…September 30th 2015…………………………
	Emissions to Air

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value (Annual) [6]
	Quarter 1 Average pro rata emission concentration
	Quarter 2 Average pro rata emission concentration
	Quarter 3 Average pro rata emission concentration
	Quarter 4 Average pro rata emission concentration
	Annual Emissions Concentration 

	A1
	Lead
	1.0 mg/m3 
	0.006
	0.022
	N/R
	
	

	A2
	Lead  
	1.0 mg/m3 
	0.058
	0.076
	0.064
	
	

	A3
	Lead
	1.0 mg/m3 
	0.096
	0.142
	0.178
	
	

	A63
	Lead
	1.0mg/m3
	0.034
	0.071
	0.100
	
	

	A4
	Lead
	0.25 mg/m3 
	0.129
	0.010
	0.072
	
	

	A6
	Lead
	0.30 mg/m3 
	0.018
	0.086
	0.069
	
	

	A8
	Lead
	0.20 mg/m3 
	0.020
	0.079
	0.040
	
	

	A9
	Lead
	0.20 mg/m3 
	0.124
	0.073
	0.015
	
	

	A10
	Lead
	0.20 mg/m3 
	0.009
	0.023
	0.052
	
	

	A11
	Lead
	0.20 mg/m3 
	0.009
	0.021
	0.017
	
	

	A12
	Lead
	0.15 mg/m3 
	0.017
	0.291
	0.068
	
	

	A13
	Lead
	0.4 mg/m3 
	0.018
	0.0225
	0.043
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

[6] The emission limit value is expressed as a maximum individual value and corrected to 273K, 101.3kPa.

 [7] To be Signed ………[image: image2.emf]

………………………………….  

Date…23/10/2015…


(authorised to sign as representative of the Operator)

Permit Reference Number: NP3030BJ
Operator: Enersys Ltd

Installation: Enersys Newport
Form Number: W1
Reporting of Emissions to Water (other than to Sewer) for the period from … July 1st 2015…………….to…September 30th 2015…………………………
	Emissions to Water

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/

Certification [4]
	Uncertainty

[5]

	W1
	Lead and its compounds
	2.0mg/l [6]
	0.400

0.056

0.340

0.082

0.430

0.390

0.057

0.039

0.051

0.120

0.084

0.290

0.420
0.220
	ISO/IEC 17025:2005
	1-Jul-15

8-Jul-15

15-Jul-15

22-Jul-15

29-Jul-15

5-Aug-15

12-Aug-15

19-Aug-15

26-Aug-15

2-Sep-15

9-Sep-15

16-Sep-15

23-Sep-15

30-Sep-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	W1
	Flow
	Not applicable
	
	
	
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values. Where the emission limit value is an annual mean, the result is given as the average measured value.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

[6] The emission limit values are expressed as a maximum individual value.  Limit  only applies from 1 July 2006.

Signed …………[image: image3.emf]

………….………………………………………….  

Date……23/10/2015…………………..




(authorised to sign as representative of the Operator)

Permit Reference Number: NP3030BJ
Operator: Enersys Ltd
Installation: Enersys Newport
Form Number: S1
Reporting of Emissions to Sewer for the period from … July 1st 2015………………………….to…September 30th 2015…………………………
	Emissions to Sewer

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/
Certification [4]
	Uncertainty

[5]

	S1
	Lead and its compounds.
	2mg/l [6]
	0.190
0.097

0.170

0.160

0.530

0.570

0.440

0.320

0.073

0.130

0.460

0.810

0.190
0.100
	ISO/IEC 17025:2005
	1-Jul-15

8-Jul-15

15-Jul-15

22-Jul-15

29-Jul-15

5-Aug-15

12-Aug-15

19-Aug-15

26-Aug-15

2-Sep-15

9-Sep-15

16-Sep-15

23-Sep-15

30-Sep-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	pH
	6-11 [7]
	6.10
6.70

7.10

6.90

7.50

6.80

7.10

7.20

7.20

7.00

7.10

6.80

7.60

7.10
	ISO/IEC 17025:2005
	1-Jul-15

8-Jul-15

15-Jul-15

22-Jul-15

29-Jul-15

5-Aug-15

12-Aug-15

19-Aug-15

26-Aug-15

2-Sep-15

9-Sep-15

16-Sep-15

23-Sep-15

30-Sep-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	Sulphates
	Not applicable
	47
240

260

210

270

370

240

290

220

250

250

310

390

330
	ISO/IEC 17025:2005
	1-Jul-15

8-Jul-15

15-Jul-15

22-Jul-15

29-Jul-15

5-Aug-15

12-Aug-15

19-Aug-15

26-Aug-15

2-Sep-15

9-Sep-15

16-Sep-15

23-Sep-15

30-Sep-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	Suspended solids
	Not applicable
	27
33

23

32

34

25

34

68

54

26

25

39

22

48
	ISO/IEC 17025:2005
	1-Jul-15

8-Jul-15

15-Jul-15

22-Jul-15

29-Jul-15

5-Aug-15

12-Aug-15

19-Aug-15

26-Aug-15

2-Sep-15

9-Sep-15

16-Sep-15

23-Sep-15

30-Sep-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	Flow
	150,000l/day * 92days =13,800,000 litres
	1026394
LITRES OVER THE QUARTER
	
	
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values. Where the emission limit value is an annual mean, the result is given as the average measured value.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

[6] The emission limit values are expressed as a maximum individual value.

[7] The emission limit values for pH are expressed as minimum and maximum individual values.

Signed ………[image: image4.emf]

……………………………………………….  

Date……23/10/2015…………………..



(authorised to sign as representative of the Operator)
Date created: 23/10/2015
23/10/2015 


