Permit Reference Number: NP3030BJ
Operator: EnerSys Ltd
Installation: EnerSys Newport
Form Number: A1
Reporting of Emissions to Air for the period from …April1st 2015………………………….to…June 30th 2015…………………………

	Emissions to Air

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value (Annual) [6]
	Spot Limit Values [6]
	Spot Result[1]
	Process run time
	Quarter Result [7]
	Test Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A1
	Lead
	1.0 mg/m3 
	1.0 mg/m3 
	0.03
	469
	0.022
	BS EN 14385:2004
	27/04/2015
13:10 - 14:10
	MCERTS

UKAS 0934
	<0.01

	Mill 1
	
	
	
	0.04
	715
	
	BS EN 14385:2004
	01/05/2015
10:52-11:40
	MCERTS

UKAS 0934
	<0.01

	
	
	
	
	0.04
	99
	
	BS EN 14385:2004
	01/06/2015
12:01-12:49
	MCERTS

UKAS 0934
	<0.01

	A2
	Lead  
	1.0 mg/m3 
	1.0 mg/m3
	0.05
	572
	0.066
	BS EN 14385:2004
	13/04/2015
10:57 – 11:45
	MCERTS

UKAS 0934
	+/-0.01

	Mill 2
	
	
	
	0.18
	642
	
	BS EN 14385:2004
	01/05/2015
12:00-12:48
	MCERTS

UKAS 0934
	+/-0.02

	
	
	
	
	0.02
	513
	
	BS EN 14385:2004
	01/06/2015
13:10-13:58
	MCERTS

UKAS 0934
	<0.01

	A3
	Lead
	1.0 mg/m3 
	1.0 mg/m3 
	0.27
	634
	0.121
	BS EN 14385:2004
	09/04/2015
12:15 – 12:55
	MCERTS

UKAS 0934
	+/-0.03

	Mill 3
	
	
	
	0.08
	581
	
	BS EN 14385:2004
	01/05/2015
13:25-14:25
	MCERTS

UKAS 0934
	+/-0.01

	
	
	
	
	0.09
	585
	
	BS EN 14385:2004
	09/06/2015
11:18-11:58
	MCERTS

UKAS 0934
	+/-0.01

	A63
	Lead
	1.0 mg/m3 
	1.0 mg/m3 
	0.20
	322
	0.057
	BS EN 14385:2004
	09/04/2015
14:20 – 15:08
	MCERTS

UKAS 0934
	+/-0.03

	Mill4
	
	
	
	0.05
	348
	
	BS EN 14385:2004
	05/05/2015
11:21-12:09
	MCERTS

UKAS 0934
	<0.01

	
	
	
	
	0.05
	569
	
	BS EN 14385:2004
	01/06/2015
14:35-15:23
	MCERTS

UKAS 0934
	<0.01


	Emission

Point
	Substance /

Parameter
	Emission

Limit Value (Annual) [6]
	Spot Limit Values [6]
	Spot Result[1]
	Process run time
	Quarter Result [7]
	Test Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A4
	Lead
	0.25 mg/m3 
	0.25 mg/m3
	0.02
	941
	0.009
	BS EN 14385:2004
	09/04/2015
11:10 – 11:50
	MCERTS

UKAS 0934
	<0.01

	A6
	Lead
	0.30 mg/m3 [6]
	1.5 mg/m3 
	0.08
	1985
	0.073
	BS EN 14385:2004
	10/04/2015
11:30 – 12:10
	MCERTS

UKAS 0934
	+/-0.01

	A8
	Lead
	0.20 mg/m3 [6]
	1.5 mg/m3]
	0.07
	2089
	0.067
	BS EN 14385:2004
	10/04/2015
14:10 – 14:50
	MCERTS

UKAS 0934
	+/-0.01

	A9
	Lead
	0.20 mg/m3 [6]
	0.75 mg/m3 
	0.07
	1929
	0.062
	BS EN 14385:2004
	13/04/2015
12:28 – 13:04
	MCERTS

UKAS 0934
	+/-0.01

	A10
	Lead
	0.20 mg/m3 [6]
	1.0 mg/m3 
	0.02
	2177
	0.020
	BS EN 14385:2004
	13/04/2015
14:15 – 15:09
	MCERTS

UKAS 0934
	<0.01

	A11
	Lead
	0.15mg/m3 (6)
	0.75mg/m3
	0.02
	1946
	0.018
	BS EN 14385:2004
	08/04/2015
11:20-12:20


	MCERTS

UKAS 4279
	<0.01

	A12
	Lead
	0.15 mg/m3 [6]
	0.75 mg/m3 
	0.26
	2082
	0.248
	BS EN 14385:2004
	27/04/2015
11:16 – 12:04
	MCERTS

UKAS 0934
	+/-0.03

	A13
	Lead
	0.4 mg/m3 [6]
	1.0 mg/m3
	0.02
	2102
	0.019
	BS EN 14385:2004
	08/04/2015
14:20 – 15:00
	MCERTS

UKAS 0934
	<0.01


 [1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

[6] The emission limit value is expressed as a maximum individual value and corrected to 273K, 101.3kPa.

[7] To be calculated pro rata according to run time.

Signed ………[image: image1.emf]

…(authorised to sign as representative of the Operator)…  

Date…30/07/2015……………..   


Permit Reference Number: NP3030BJ
Operator: Enersys Ltd
Installation: Enersys Newport
Form Number: A2

Reporting of Emissions to Air for the period from …April1st 2015………………………….to…June 30th 2015…………………………
	Emissions to Air

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value (Annual) [6]
	Quarter 1 Average pro rata emission concentration
	Quarter 2 Average pro rata emission concentration
	Quarter 3 Average pro rata emission concentration
	Quarter 4 Average pro rata emission concentration
	Annual Emissions Concentration 

	A1
	Lead
	1.0 mg/m3 
	0.006
	0.022
	
	
	

	A2
	Lead  
	1.0 mg/m3 
	0.058
	0.066
	
	
	

	A3
	Lead
	1.0 mg/m3 
	0.096
	0.121
	
	
	

	A63
	Lead
	1.0mg/m3
	0.034
	0.057
	
	
	

	A4
	Lead
	0.25 mg/m3 
	0.129
	0.009
	
	
	

	A6
	Lead
	0.30 mg/m3 
	0.018
	0.073
	
	
	

	A8
	Lead
	0.20 mg/m3 
	0.020
	0.067
	
	
	

	A9
	Lead
	0.20 mg/m3 
	0.124
	0.062
	
	
	

	A10
	Lead
	0.20 mg/m3 
	0.009
	0.020
	
	
	

	A11
	Lead
	0.20 mg/m3 
	0.009
	0.018
	
	
	

	A12
	Lead
	0.15 mg/m3 
	0.017
	0.248
	
	
	

	A13
	Lead
	0.4 mg/m3 
	0.018
	0.019
	
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

[6] The emission limit value is expressed as a maximum individual value and corrected to 273K, 101.3kPa.

 [7] To be Signed ………[image: image2.emf]

………………………………….  

Date…30/07/2015…


(authorised to sign as representative of the Operator)

Permit Reference Number: NP3030BJ
Operator: Enersys Ltd

Installation: Enersys Newport
Form Number: W1
Reporting of Emissions to Water (other than to Sewer) for the period from … April1st 2015 to June 30th 2015……………………………

	Emissions to Water

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/

Certification [4]
	Uncertainty

[5]

	W1
	Lead and its compounds
	2.0mg/l [6]
	0.530

0.240

0.270

0.290

0.360

0.240

0.280

0.770

0.400

0.093

0.870
0.340

0.047
	ISO/IEC 17025:2005
	1-Apr-15

8-Apr-15

15-Apr-15

22-Apr-15

29-Apr-15

6-May-15

13-May-15

20-May-15

27-May-15

4-Jun-15

10-Jun-15

17-Jun-15

24-Jun-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	W1
	Flow
	Not applicable
	
	
	
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values. Where the emission limit value is an annual mean, the result is given as the average measured value.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

[6] The emission limit values are expressed as a maximum individual value.  Limit  only applies from 1 July 2006.

Signed …………[image: image3.emf]

………….………………………………………….  

Date……30/07/2015…………………..




(authorised to sign as representative of the Operator)

Permit Reference Number: NP3030BJ
Operator: Enersys Ltd
Installation: Enersys Newport
Form Number: S1
Reporting of Emissions to Sewer for the period from … April1st 2015………………………….to…June 30th 2015……………………………

	Emissions to Sewer

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/
Certification [4]
	Uncertainty

[5]

	S1
	Lead and its compounds.
	2mg/l [6]
	0.130
0.080

0.039

0.230

0.180

0.097

0.750

0.540

0.320

1.500
0.770
0.260
0.390
	ISO/IEC 17025:2005
	1-Apr-15

8-Apr-15

15-Apr-15

22-Apr-15

29-Apr-15

6-May-15

13-May-15

20-May-15

27-May-15

4-Jun-15

10-Jun-15

17-Jun-15

24-Jun-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	pH
	6-11 [7]
	7.6
7.4

8.6

7.5

7.0

7.1

7.0

6.5

7.1

6.7

8.9
6.7
6.7
	ISO/IEC 17025:2005
	1-Apr-15

8-Apr-15

15-Apr-15

22-Apr-15

29-Apr-15

6-May-15

13-May-15

20-May-15

27-May-15

4-Jun-15

10-Jun-15

17-Jun-15

24-Jun-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	Sulphates
	Not applicable
	380
210

280

340

510

450

380

310

290

340

280
130
240
	ISO/IEC 17025:2005
	1-Apr-15

8-Apr-15

15-Apr-15

22-Apr-15

29-Apr-15

6-May-15

13-May-15

20-May-15

27-May-15

4-Jun-15

10-Jun-15

17-Jun-15

24-Jun-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	Suspended solids
	Not applicable
	56
44

5

49

98

21

41

23

20

33

38
120
110
	ISO/IEC 17025:2005
	1-Apr-15

8-Apr-15

15-Apr-15

22-Apr-15

29-Apr-15

6-May-15

13-May-15

20-May-15

27-May-15

4-Jun-15

10-Jun-15

17-Jun-15

24-Jun-15
	DERWENTSIDE ENVIRONMENTAL TESTING SERVICES LTD UKAS 2139
	

	S1
	Flow
	150,000l/day * 92days =13,800,000 litres
	851,793
LITRES OVER THE QUARTER
	
	
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values. Where the emission limit value is an annual mean, the result is given as the average measured value.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

[6] The emission limit values are expressed as a maximum individual value.

[7] The emission limit values for pH are expressed as minimum and maximum individual values.

Signed ………[image: image4.emf]

……………………………………………….  

Date……30/07/2015…………………..



(authorised to sign as representative of the Operator)
Date created: 06/08/2015
06/08/2015 


