Permit Reference Number: BL3986ID                






Operator: Tarmac Cement & Lime Ltd

Installation: Aberthaw Cement Works                                          




Form Number: Air 1 / 19/07/2016
Six-monthly Reporting of Emissions to Air from Emission Point A1 for the period from
to 
	Substance / Parameter
	Emission Limit Level
	Result (1)
	Test Method(2)
	Sample Date & Times(3)
	Accreditation/ Certification (4)
	Uncertainty

(5)

	
	
	First 6 Months
	Second 6 Months
	
	
	
	

	Hydrogen Fluoride
	1mg/Nm3 over minimum 1 hour period
	
	
	
	
	
	

	Cadmium & thallium and their compounds (total)
	0.05mg/Nm3 over minimum 30 min, max 8 hr period
	
	
	
	
	
	

	Mercury and its compounds
	0.05mg/Nm3 over minimum 30 min, max 8 hr period
	
	
	
	
	
	

	Sb, As, Pb, Cr, Co, Cu, Mn, Ni, and V and their compounds (total)
	0.5mg/Nm3 over minimum 30 min, max 8 hr period
	
	
	
	
	
	

	Dioxins / Furans (I-TEQ)6
	0.1ng/Nm3 over minimum 6hr, max 8 hr period
	
	
	
	
	
	

	Dioxins / Furans (WHO – TEQ Humans/ Mammals)6
	No Limit
	
	
	
	
	
	

	Dioxins / Furans (WHO – TEQ Fish)6
	No Limit
	
	
	
	
	
	

	Dioxins / Furans (WHO – TEQ Birds)6
	No Limit
	
	
	
	
	
	


1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reported period, expressed in the same terms as the emission limit value. Where the emission limit is expressed as a range, the result given as the minimum – maximum’ measured values. 

2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the agency is used then the appropriate identifier is given. In other cases the principal technique is stated e.g. gas chromatography

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.

4. The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis. 

5. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

6. The result to be reported as a range based on: All congeners less than the detection limit assumed to be zero as a minimum, and all congeners less than the detection limit assumed to be at the detection limit as a maximum. 

Signed ……………………………………………….        



Date………………………..      

(Authorised to sign as representative of Tarmac Cement & Lime Ltd)
