Schedule 6 – Notification
These pages outline the information that the operator must provide.
Units of measurement used in information supplied under Part A and B requirements shall be appropriate
to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions 

and authorized emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential 

information, supplied on a separate sheet and accompanied by an application for commercial confidentiality 

under the provisions of the PPC Regulations.

Part A
	Permit Number
	MP3038MP

	Name of operator
	Knauf Insulation

	Location of Installation
	Cwmbran

	Time and date of the detection
	25/11/2014          11:20 – 15:50


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	25th November 2014      11:20 – 15:50

	Reference or description of the location of the event
	A1

	Description of where any release into the environment took place
	To air in the Pontypool /Cwmbran area 

	Substance(s) potentially

released
	Oxides of Sulphur as SO2

	Best estimate of the quantity or rate of release of substance
	Average reading of the 4 samples - 190.1 mg/m3, (uncertainty of test +/- 23.1 mg/m3).

	Measures taken, or intended to be taken, to stop any emission
	N/A

	Description of the failure or accident
	Extractive test result is higher than permit temporary authorisation limit.


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	A1

	Parameter(s)
	Oxides of Sulphur as SO2

	Limit
	100 mg/m3 (Temporary Limit 150 mg/m3)

	Measured value and uncertainty
	190.1 mg/m3, (uncertainty of test +/- 23.1 mg/m3)

	Date and time of monitoring
	25th November 2014      11:20 – 15:50

	Measures taken, or intended to be taken, to stop the emission
	Extractive re-test to be undertaken January 2015.
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	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection 

	
	

	Substance(s) detected
	Oxides of Sulphur as SO2

	Concentrations of substances detected
	190.1 mg/m3, (uncertainty of test +/- 23.1 mg/m3)

	Date of monitoring/sampling
	25th November 2014      11:20 – 15:50


Part B – to be submitted as soon as practicable

	Any more accurate information on the matters for notification under Part A.
	Fluctuations in the SO2 levels are believed to be through poor quality bottled cullet being sent be the supplier during this sampling period.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	A re-sample of this parameter was undertaken and the average result was 37.9 mg/m3, (uncertainty of test +/- 4.6 mg/m3). 

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused be the emission
	Improved quality of bottled cullet is now being received from the supplier from a different location.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	28/05/13 – CEMS unit failure

28/06/13 – High COD from S1 discharge point
17/09/14 – EP Unit shut down due to failure


	Name*
	Warren Christy

	Post 
	HS&E Manager

	Signature
	                             [image: image1.emf]

	Date
	30/01/2015


* authorised to sign on behalf of Knauf Insulation Limited
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