Permit Number: 
BR8212IK




Operator: 

Knauf Insulation Ltd

Installation:

Knauf Insulation Ltd, Cwmbran

Form Number:
 Air1  

Reporting of emissions to air for the period from 

01/01/2015
to
30/06/2015
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	A0
	Particulate matter
	35 mg/m3

	Extractive sample 
	24.7
	BS EN 13284-1
	10:40 – 11:40
18/06/2015
	3.1

	A1
	Particulate matter
	20 mg/m3
	Daily average
	3.4
	MCerts Approved
	Jan – Jul  2015
99% Operational
	

	A1
	Particulate matter
	30 mg/m3
	Half hour maximum 
	15.3
	MCerts Approved
	Jan – Jul  2015
99% Operational
	

	A1
	Particulate matter
	30 mg/m3
	Extractive sample
	7.6
	BS EN 13284-1
	12:15 – 13:15
15/06/2015
	1.1

	A1
	Oxides of Nitrogen 

(NO and NO2 expressed as NO2) 
	300 mg/m3
	Daily average
	226
	MCerts Approved
	Jan – Jul  2015
99% Operational
	

	A1
	Oxides of Nitrogen 

(NO and NO2 expressed as NO2)
	450 mg/m3
	Half hour maximum 
	500
	MCerts Approved
	Jan – Jul  2015
99% Operational
	

	A1
	Oxides of Nitrogen 

(NO and NO2 expressed as NO2) 
	300 mg/m3
	Extractive sample 
	216.5
	BS EN 14792
	10:02 – 11:02
16/06/2015
	25

	A1
	Carbon monoxide
	200 mg/m3
	Extractive sample 
	1.6
	BS EN 15058
	10:02 – 11:02

16/06/2015
	11.6

	A1
	Oxides of sulphur (as SO2)
	150 mg/m3
(Temporary Limit)
	Extractive sample
	88.86
(5 sample average)
	BS EN14791
	09:45 – 15:05
16/06/2015
	10.78

	A1
	Gaseous fluorides (as HF)
	5 mg/m3
	Extractive sample 
	0.26
	ISO 15713
	15:10 – 16:10
16/06/2015
	0.03

	A1
	Gaseous Chlorides (as HCl)
	20 mg/m3
	Extractive sample
	4.4
	BS EN1911
	11:05 – 12:05
15/06/2015
	0.12

	A3
	Particulate matter
	35 mg/m3

	Extractive sample 
	35.2
	BS EN 13284-1
	11:55 – 12:55
17/06/2015
	0.8

	A3
	Phenol
	10 mg/m3
	Extractive sample
	<0.9
	BS EN 13649
	13:05 – 13:10
17/06/2015
	50%

	A3
	Formaldehyde
	5 mg/m3
	Extractive sample
	0.32
	USEPA 316
	10:38 – 11:38
17/06/2015
	0.05

	A3
	Ammonia
	50 mg/m3
	Extractive sample
	29.4
	BS EN 14791
	11:55 – 12:55

17/06/2015
	3.6

	A3
	Volatile organic compounds
	35 mg/m3
	Extractive sample
	18.0
	BS EN 12619
	11:10 – 12:10
17/06/2015
	7.5

	A4
	Particulate matter
	30 mg/m3

	Extractive sample 
	2.2
	BS EN 13284-1
	12:31 – 13:31
04/06/2015
	0.5


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the authority is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
Signed …………………[image: image1.emf]……………………………………….  

Date…27/07/2015……………………..   



(Authorised to sign as representative of Operator)

