Permit Number: 
BR8212IK




Operator: 

Knauf Insulation Ltd

Installation:

Knauf Insulation Ltd, Cwmbran

Form Number:
 Air2  

Reporting of emissions to air for the period from 

01/01/2018
to
30/06/2018
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	A0
	Particulate matter
	35 mg/Nm3
	Extractive sample 
	14.3
(3 spot sample average)
	BS EN 13284-1
	10:35 – 14:06
31/05/2018
	1.00

	A1
	Particulate matter
	20 mg/Nm3
	Daily average
	2.23

	MCerts Approved
	Jan – Jun 2018
95% Operational
	-

	A1
	Oxides of Nitrogen 

(NO and NO2 expressed as NO2) 
	300 mg/Nm3
	Daily average
	180.85


	MCerts Approved
	Jan – Jun 2018

95% Operational
	-

	A1
	Carbon Monoxide
	100 mg/Nm3
	Extractive sample 
	5.29
(3 spot sample average)
	BS EN 15058
	13:40 – 15:20
12/06/2018
	1.2

	A1
	Oxides of Sulphur (as SO2)
	150 mg/Nm3
	Extractive sample
	82.73
(3 spot sample average)
	BS EN14791
	13:53 – 16:00

12/06/2018
	6.57

	A1
	Gaseous Fluorides (as HF)
	5 mg/Nm3
	Extractive sample 
	0.637
(3 spot sample average)
	ISO 15713
	11:36 – 12:35

12/06/2018
	0.041

	A1
	Gaseous Chlorides (as HCl)
	10 mg/Nm3
	Extractive sample
	0.613
(3 spot sample average)
	BS EN1911
	09:13 – 11:18

12/06/2018
	0.039

	A1
	Group 1 Metals
	1 mg/Nm3
	Extractive sample
	0.036
(3 spot sample average)
	BS EN14385
	09:04 – 11:16

13/06/2018
	0.005

	A1
	Group 2 Metals
	2 mg/Nm3
	Extractive sample
	0.089
(3 spot sample average)
	BS EN14385
	09:04 – 11:16

13/06/2018
	0.013

	A3
	Particulate matter
	47 mg/Nm3

	Extractive sample 
	24.03
(3 spot sample average)
	BS EN 13284-1
	10:10 – 12:30

14/06/2018
	1.7

	A3
	Phenol
	9 mg/Nm3
	Extractive sample
	<0.15
(3 spot sample average)
	BS EN 13649
	12:30 – 15:40

14/06/2018
	0.061

	A3
	Formaldehyde
	5 mg/Nm3
	Extractive sample
	0.27
(3 spot sample average)
	USEPA M316
	13:03 – 15:10

14/06/2018
	0.04

	A3
	Ammonia
	60 mg/Nm3
	Extractive sample
	24.76
(3 spot sample average)
	BS EN 14791
	10:10 – 12:30

14/06/2018
	2.77

	A3
	Volatile organic compounds
	27 mg/Nm3
	Extractive sample
	12.07
(3 spot sample average)
	BS EN 12619
	10:20 – 12:00

14/06/2018
	0.51

	A3
	Amines
	3 mg/Nm3
	Extractive sample
	0.732
(3 spot sample average)
	CE/TS 13649
	09:50 – 13:05

31/05/2018
	0.432

	A4
	Particulate matter
	30 mg/Nm3

	Extractive sample 
	No longer emission point
	BS EN 13284-1
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the authority is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
Signed …………………[image: image1.emf]……………………………………….  

Date…31/07/2018……………………..   



(Authorised to sign as representative of Operator)

