
Permit Number: EPR/VP3339PD			Operator: 		Morganite Electrical Carbon Ltd

Facility:Electrical Carbon Swansea 		Form Number: 	 A1 
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A10
	Lead
	2 mg/Nm3
	Spot Sample
	
	BS EN 14385:2004
	
	

	A10
	Copper
	2 mg/Nm3
	Spot Sample
	
	BS EN 14385:2004
	
	

	A10
	Antimony
	2 mg/Nm3
	Spot Sample
	
	BS EN 14385:2004
	
	

	A10
	Total Particulate
	5 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002
	
	

	A15
	Total Particulate
	4 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002
	
	

	A15
	Benzo(a)pyrene (BaP)
	0.005 mg/Nm3
	Hourly Average
	
	
	
	

	
	
	
	
	
	
	
	

	A19
	Total Particulate
	5 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002
	
	

	
	
	
	
	
	
	
	

	A27
	Sulphur Dioxide
	2900 mg/Nm3
	24 Hourly Average
	
	BS ISO 7935:1992
	
	

	A27
	Oxides of Nitrogen (expressed as NO2)
	150 mg/Nm3
	24 Hourly Average
	
	BS ISO 10849:1996
	
	

	
	
	
	
	
	
	
	

	A27
	Total Particulate
	10 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002
	
	

	A27
	Benzo(a)pyrene (BaP)
	0.01 mg/Nm3
	Hourly Average
	
	
	
	


	A28
	Sulhpur Dioxide
	2900 mg/Nm3
	24 Hourly Average
	
	BS ISO 10849:1996
	
	

	A28
	[bookmark: _GoBack]Oxides of Nitrogen (expressed as NO2)
	150 mg/Nm3
	24 Hourly Average
	
	BS ISO 10849:1996
	
	

	A28
	Total Particulate
	10 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002
	
	

	A28
	Benzo(a)pyrene (BaP)
	0.01 mg/Nm3

	Hourly Average
	
	
	
	

	A61
	Sulphur Dioxide
	2900 mg/Nm3
	24 Hourly Average
	
	BS ISO 7935:1992
	
	

	A61
	Oxides of Nitrogen 
(expressed as NO2)
	150 mg/Nm3
	24 Hourly Average
	
	BS ISO 13284-1:2002
	
	

	A61
	Total Particulate
	10 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002
	
	

	A61
	Benzo(a)pyrene (BaP)
	0.01 mg/Nm3
	Hourly Average
	
	
	
	






[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

