Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…MAR15-SL…
Reporting of ……LEACHATE…… monitoring for the period for … March 2015…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL1


	Am Nitrogen


	1370 mg/l


	Mar - 15

	No Sample
	957
	29/03/15
	10.6



	SL1


	Cadmium


	0.1 mg/l


	Mar - 15

	No Sample
	34
	29/03/15
	7.83



	SL1


	Nickel


	0.1 mg/l


	Mar - 15

	No Sample
	34

	29/03/15
	8.82



	SL1


	Chloride
	13713 mg/l


	Mar - 15

	No Sample
	678
	29/03/15
	21.5



	SL1


	MP Xylene


	0.029 mg/l


	Mar - 15

	No Sample
	54
	29/03/15
	

	SL1


	Mecoprop


	0.032 mg/l


	Mar - 15

	No Sample
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL2
	Am Nitrogen


	1370 mg/l


	Mar - 15


	No Sample
	957
	29/03/15
	10.6



	SL2
	Cadmium


	0.1 mg/l


	Mar - 15


	No Sample
	34
	29/03/15
	7.83



	SL2
	Nickel


	0.1 mg/l


	Mar - 15


	No Sample
	34

	29/03/15
	8.82



	SL2
	Chloride


	13713 mg/l


	Mar - 15


	No Sample
	678
	29/03/15
	21.5



	SL2
	MP Xylene


	0.029 mg/l


	Mar - 15


	No Sample
	54
	29/03/15
	

	SL2
	Mecoprop


	0.032 mg/l


	Mar - 15


	No Sample
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL3
	Am Nitrogen


	1370 mg/l


	Mar - 15


	No Sample
	957
	29/03/15
	10.6



	SL3
	Cadmium


	0.1 mg/l


	Mar - 15


	No Sample
	34
	29/03/15
	7.83



	SL3
	Nickel


	0.1 mg/l


	Mar - 15


	No Sample
	34

	29/03/15
	8.82



	SL3
	Chloride


	13713 mg/l


	Mar - 15


	No Sample
	678
	29/03/15
	21.5



	SL3
	MP Xylene


	0.029 mg/l


	Mar - 15


	No Sample
	54
	29/03/15
	

	SL3
	Mecoprop


	0.032 mg/l


	Mar - 15


	No Sample
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL4
	Am Nitrogen


	1370 mg/l


	Mar - 15


	262
	957
	29/03/15
	10.6



	SL4
	Cadmium


	0.1 mg/l


	Mar - 15


	<1.00
	34
	29/03/15
	7.83



	SL4
	Nickel


	0.1 mg/l


	Mar - 15


	24.7
	34

	29/03/15
	8.82



	SL4
	Chloride


	13713 mg/l


	Mar - 15


	572
	678
	29/03/15
	21.5



	SL4
	MP Xylene


	0.029 mg/l


	Mar - 15


	0.130
	54
	29/03/15
	

	SL4
	Mecoprop


	0.032 mg/l


	Mar - 15


	10.7
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL5
	Am Nitrogen


	1370 mg/l


	Mar - 15


	197
	957
	29/03/15
	10.6



	SL5
	Cadmium


	0.1 mg/l


	Mar - 15


	<1.00
	34
	29/03/15
	7.83



	SL5
	Nickel


	0.1 mg/l


	Mar - 15


	20.9
	34

	29/03/15
	8.82



	SL5
	Chloride


	13713 mg/l


	Mar - 15


	716
	678
	29/03/15
	21.5



	SL5
	MP Xylene


	0.029 mg/l


	Mar - 15


	0.112
	54
	29/03/15
	

	SL5
	Mecoprop


	0.032 mg/l


	Mar - 15


	5.46
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL6
	Am Nitrogen


	1370 mg/l


	Mar - 15


	100
	957
	29/03/15
	10.6



	SL6
	Cadmium


	0.1 mg/l


	Mar - 15


	<1.00
	34
	29/03/15
	7.83



	SL6
	Nickel


	0.1 mg/l


	Mar - 15


	9.91
	34

	29/03/15
	8.82



	SL6
	Chloride


	13713 mg/l


	Mar - 15


	125
	678
	29/03/15
	21.5



	SL6
	MP Xylene


	0.029 mg/l


	Mar - 15


	0.678
	54
	29/03/15
	

	SL6
	Mecoprop


	0.032 mg/l


	Mar - 15


	<5
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL7
	Am Nitrogen


	1370 mg/l


	Mar - 15


	747
	957
	29/03/15
	10.6



	SL7
	Cadmium


	0.1 mg/l


	Mar - 15


	<1.00
	34
	29/03/15
	7.83



	SL7
	Nickel


	0.1 mg/l


	Mar - 15


	62.9
	34

	29/03/15
	8.82



	SL7
	Chloride


	13713 mg/l


	Mar - 15


	1220
	678
	29/03/15
	21.5



	SL7
	MP Xylene


	0.029 mg/l


	Mar - 15


	0.441
	54
	29/03/15
	

	SL7
	Mecoprop


	0.032 mg/l


	Mar - 15


	18.5
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL8
	Am Nitrogen


	1370 mg/l


	Mar - 15


	934
	957
	29/03/15
	10.6



	SL8
	Cadmium


	0.1 mg/l


	Mar - 15


	<1.00
	34
	29/03/15
	7.83



	SL8
	Nickel


	0.1 mg/l


	Mar - 15


	102
	34

	29/03/15
	8.82



	SL8
	Chloride


	13713 mg/l


	Mar - 15


	1530
	678
	29/03/15
	21.5



	SL8
	MP Xylene


	0.029 mg/l


	Mar - 15


	0.455
	54
	29/03/15
	

	SL8
	Mecoprop


	0.032 mg/l


	Mar - 15


	32.5
	1214

	29/03/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL9
	Am Nitrogen


	1370 mg/l


	Mar - 15


	1270
	957
	29/03/15
	10.6



	SL9
	Cadmium


	0.1 mg/l


	Mar - 15


	<1.00
	34
	29/03/15
	7.83



	SL9
	Nickel


	0.1 mg/l


	Mar - 15


	230
	34

	29/03/15
	8.82



	SL9
	Chloride


	13713 mg/l


	Mar - 15


	1750
	678
	29/03/15
	21.5



	SL9
	MP Xylene


	0.029 mg/l


	Mar - 15


	2.78
	54
	29/03/15
	

	SL9
	Mecoprop


	0.032 mg/l


	Mar - 15


	43.5
	1214

	29/03/15
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………..…………J G Ffoulkes………………………………….  

Date…………27/4/15……………..   



(Authorised to sign as representative of Operator)

