Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…FEB15-SL…
Reporting of ……LEACHATE…… monitoring for the period for … Febuary 2015…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL1


	Am Nitrogen


	1370 mg/l


	Feb - 15

	No Sample

	957
	28/02/15
	10.6



	SL1


	Cadmium


	0.1 mg/l


	Feb - 15

	No Sample


	34
	28/02/15
	7.83



	SL1


	Nickel


	0.1 mg/l


	Feb - 15

	No Sample


	34

	28/02/15
	8.82



	SL1


	Chloride
	13713 mg/l


	Feb - 15

	No Sample


	678
	28/02/15
	21.5



	SL1


	MP Xylene


	0.029 mg/l


	Feb - 15

	No Sample


	54
	28/02/15
	

	SL1


	Mecoprop


	0.032 mg/l


	Feb - 15

	No Sample


	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL2
	Am Nitrogen


	1370 mg/l


	Feb - 15


	No Sample


	957
	28/02/15
	10.6



	SL2
	Cadmium


	0.1 mg/l


	Feb - 15


	No Sample


	34
	28/02/15
	7.83



	SL2
	Nickel


	0.1 mg/l


	Feb - 15


	No Sample


	34

	28/02/15
	8.82



	SL2
	Chloride


	13713 mg/l


	Feb - 15


	No Sample


	678
	28/02/15
	21.5



	SL2
	MP Xylene


	0.029 mg/l


	Feb - 15


	No Sample


	54
	28/02/15
	

	SL2
	Mecoprop


	0.032 mg/l


	Feb - 15


	No Sample


	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL3
	Am Nitrogen


	1370 mg/l


	Feb - 15


	No Sample


	957
	28/02/15
	10.6



	SL3
	Cadmium


	0.1 mg/l


	Feb - 15


	No Sample


	34
	28/02/15
	7.83



	SL3
	Nickel


	0.1 mg/l


	Feb - 15


	No Sample


	34

	28/02/15
	8.82



	SL3
	Chloride


	13713 mg/l


	Feb - 15


	No Sample


	678
	28/02/15
	21.5



	SL3
	MP Xylene


	0.029 mg/l


	Feb - 15


	No Sample


	54
	28/02/15
	

	SL3
	Mecoprop


	0.032 mg/l


	Feb - 15


	No Sample


	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL4
	Am Nitrogen


	1370 mg/l


	Feb - 15


	1.7
	957
	28/02/15
	10.6



	SL4
	Cadmium


	0.1 mg/l


	Feb - 15


	<0.00020
	34
	28/02/15
	7.83



	SL4
	Nickel


	0.1 mg/l


	Feb - 15


	0.025
	34

	28/02/15
	8.82



	SL4
	Chloride


	13713 mg/l


	Feb - 15


	620
	678
	28/02/15
	21.5



	SL4
	MP Xylene


	0.029 mg/l


	Feb - 15


	14
	54
	28/02/15
	

	SL4
	Mecoprop


	0.032 mg/l


	Feb - 15


	7.9
	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL5
	Am Nitrogen


	1370 mg/l


	Feb - 15


	2.0
	957
	28/02/15
	10.6



	SL5
	Cadmium


	0.1 mg/l


	Feb - 15


	<0.00020
	34
	28/02/15
	7.83



	SL5
	Nickel


	0.1 mg/l


	Feb - 15


	0.046
	34

	28/02/15
	8.82



	SL5
	Chloride


	13713 mg/l


	Feb - 15


	810
	678
	28/02/15
	21.5



	SL5
	MP Xylene


	0.029 mg/l


	Feb - 15


	<1
	54
	28/02/15
	

	SL5
	Mecoprop


	0.032 mg/l


	Feb - 15


	6.3
	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL6
	Am Nitrogen


	1370 mg/l


	Feb - 15


	NO SAMPLE
	957
	28/02/15
	10.6



	SL6
	Cadmium


	0.1 mg/l


	Feb - 15


	NO SAMPLE
	34
	28/02/15
	7.83



	SL6
	Nickel


	0.1 mg/l


	Feb - 15


	NO SAMPLE
	34

	28/02/15
	8.82



	SL6
	Chloride


	13713 mg/l


	Feb - 15


	NO SAMPLE
	678
	28/02/15
	21.5



	SL6
	MP Xylene


	0.029 mg/l


	Feb - 15


	NO SAMPLE
	54
	28/02/15
	

	SL6
	Mecoprop


	0.032 mg/l


	Feb - 15


	NO SAMPLE
	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL7
	Am Nitrogen


	1370 mg/l


	Feb - 15


	890
	957
	28/02/15
	10.6



	SL7
	Cadmium


	0.1 mg/l


	Feb - 15


	<0.00050
	34
	28/02/15
	7.83



	SL7
	Nickel


	0.1 mg/l


	Feb - 15


	0.050
	34

	28/02/15
	8.82



	SL7
	Chloride


	13713 mg/l


	Feb - 15


	2000
	678
	28/02/15
	21.5



	SL7
	MP Xylene


	0.029 mg/l


	Feb - 15


	<1
	54
	28/02/15
	

	SL7
	Mecoprop


	0.032 mg/l


	Feb - 15


	13
	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL8
	Am Nitrogen


	1370 mg/l


	Feb - 15


	1200
	957
	28/02/15
	10.6



	SL8
	Cadmium


	0.1 mg/l


	Feb - 15


	<0.00050
	34
	28/02/15
	7.83



	SL8
	Nickel


	0.1 mg/l


	Feb - 15


	0.12
	34

	28/02/15
	8.82



	SL8
	Chloride


	13713 mg/l


	Feb - 15


	1500
	678
	28/02/15
	21.5



	SL8
	MP Xylene


	0.029 mg/l


	Feb - 15


	<1
	54
	28/02/15
	

	SL8
	Mecoprop


	0.032 mg/l


	Feb - 15


	16
	1214

	28/02/15
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL9
	Am Nitrogen


	1370 mg/l


	Feb - 15


	NO SAMPLE
	957
	28/02/15
	10.6



	SL9
	Cadmium


	0.1 mg/l


	Feb - 15


	NO SAMPLE
	34
	28/02/15
	7.83



	SL9
	Nickel


	0.1 mg/l


	Feb - 15


	NO SAMPLE
	34

	28/02/15
	8.82



	SL9
	Chloride


	13713 mg/l


	Feb - 15


	NO SAMPLE
	678
	28/02/15
	21.5



	SL9
	MP Xylene


	0.029 mg/l


	Feb - 15


	NO SAMPLE
	54
	28/02/15
	

	SL9
	Mecoprop


	0.032 mg/l


	Feb - 15


	NO SAMPLE
	1214

	28/02/15
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………..…………J G Ffoulkes………………………………….  

Date…………27/4/15……………..    



(Authorised to sign as representative of Operator)

