Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…DEC14-C…
Reporting of ……Ground Water…… monitoring for the period for … December  2014…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Dec - 14

	0.634
	25
	10 Dec 2014
	10.6



	C1


	Cadmium


	1 ug/l 
	Dec - 14

	<0.1
	34
	10 Dec 2014
	7.83



	C1


	Nickel


	0.22 ug/l


	Dec - 14

	1.38
	34
	10 Dec 2014
	8.82



	C1


	Chloride
	TBA


	Dec - 14

	175
	25
	10 Dec 2014
	21.5



	C1


	MP Xylene


	1 ug/l 
	Dec - 14

	<0.2
	54
	10 Dec 2014
	

	C1


	Mecoprop


	0.1 ug/l 
	Dec - 14

	0.013
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Dec - 14


	<0.0300
	25
	10 Dec 2014
	10.6



	C2
	Cadmium


	1 ug/l 
	Dec - 14


	0.738
	34
	10 Dec 2014
	7.83



	C2
	Nickel


	0.22 ug/l


	Dec - 14


	7.2
	34
	10 Dec 2014
	8.82



	C2
	Chloride


	TBA


	Dec - 14


	48.3
	25
	10 Dec 2014
	21.5



	C2
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C2
	Mecoprop


	0.1 ug/l 
	Dec - 14


	0.009
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Dec - 14


	<0.0300
	25
	10 Dec 2014
	10.6



	C3
	Cadmium


	1 ug/l 
	Dec - 14


	0.495
	34
	10 Dec 2014
	7.83



	C3
	Nickel


	0.22 ug/l


	Dec - 14


	7.43
	34
	10 Dec 2014
	8.82



	C3
	Chloride


	TBA


	Dec - 14


	46.6
	25
	10 Dec 2014
	21.5



	C3
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C3
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.005
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Dec - 14


	8.38
	25
	10 Dec 2014
	10.6



	C4
	Cadmium


	1 ug/l 
	Dec - 14


	<0.1
	34
	10 Dec 2014
	7.83



	C4
	Nickel


	0.22 ug/l


	Dec - 14


	3.69
	34
	10 Dec 2014
	8.82



	C4
	Chloride


	TBA


	Dec - 14


	2210
	25
	10 Dec 2014
	21.5



	C4
	MP Xylene


	1 ug/l 
	Dec - 14


	<1
	54
	10 Dec 2014
	

	C4
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.03
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Dec - 14


	9.24
	25
	10 Dec 2014
	10.6



	C5
	Cadmium


	1 ug/l 
	Dec - 14


	0.175
	34
	10 Dec 2014
	7.83



	C5
	Nickel


	0.22 ug/l


	Dec - 14


	15.1
	34
	10 Dec 2014
	8.82



	C5
	Chloride


	TBA


	Dec - 14


	3430
	25
	10 Dec 2014
	21.5



	C5
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C5
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.005
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Dec - 14


	0.684
	25
	10 Dec 2014
	10.6



	C6
	Cadmium


	1 ug/l 
	Dec - 14


	<0.1
	34
	10 Dec 2014
	7.83



	C6
	Nickel


	0.22 ug/l


	Dec - 14


	5.25
	34
	10 Dec 2014
	8.82



	C6
	Chloride


	TBA


	Dec - 14


	5210
	25
	10 Dec 2014
	21.5



	C6
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C6
	Mecoprop


	0.1 ug/l 
	Dec - 14


	0.057
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C7
	Am Nitrogen


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	10.6



	C7
	Cadmium


	1 ug/l 
	Dec - 14


	No Sample
	34
	10 Dec 2014
	7.83



	C7
	Nickel


	0.22 ug/l


	Dec - 14


	No Sample
	34
	10 Dec 2014
	8.82



	C7
	Chloride


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	21.5



	C7
	MP Xylene


	1 ug/l 
	Dec - 14


	No Sample
	54
	10 Dec 2014
	

	C7
	Mecoprop


	0.1 ug/l 
	Dec - 14


	No Sample
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Dec - 14


	5.52
	25
	10 Dec 2014
	10.6



	C8
	Cadmium


	1 ug/l 
	Dec - 14


	1.03
	34
	10 Dec 2014
	7.83



	C8
	Nickel


	0.22 ug/l


	Dec - 14


	41.1
	34
	10 Dec 2014
	8.82



	C8
	Chloride


	TBA


	Dec - 14


	6130
	25
	10 Dec 2014
	21.5



	C8
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C8
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.03
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C9
	Am Nitrogen


	TBA


	Dec - 14


	12.4
	25
	10 Dec 2014
	10.6



	C9
	Cadmium


	1 ug/l 
	Dec - 14


	<0.1
	34
	10 Dec 2014
	7.83



	C9
	Nickel


	0.22 ug/l


	Dec - 14


	1.74
	34
	10 Dec 2014
	8.82



	C9
	Chloride


	TBA


	Dec - 14


	5410
	25
	10 Dec 2014
	21.5



	C9
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C9
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.005
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Dec - 14


	17.4
	25
	10 Dec 2014
	10.6



	C10
	Cadmium


	1 ug/l 
	Dec - 14


	7.69
	34
	10 Dec 2014
	7.83



	C10
	Nickel


	0.22 ug/l


	Dec - 14


	12.1
	34
	10 Dec 2014
	8.82



	C10
	Chloride


	TBA


	Dec - 14


	3920
	25
	10 Dec 2014
	21.5



	C10
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C10
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.03
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C11
	Am Nitrogen


	TBA


	Dec - 14


	3.53
	25
	10 Dec 2014
	10.6



	C11
	Cadmium


	1 ug/l 
	Dec - 14


	0.267
	34
	10 Dec 2014
	7.83



	C11
	Nickel


	0.22 ug/l


	Dec - 14


	5.46
	34
	10 Dec 2014
	8.82



	C11
	Chloride


	TBA


	Dec - 14


	5930
	25
	10 Dec 2014
	21.5



	C11
	MP Xylene


	1 ug/l 
	Dec - 14


	<1
	54
	10 Dec 2014
	

	C11
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.03
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Dec - 14


	14.3
	25
	10 Dec 2014
	10.6



	C12
	Cadmium


	1 ug/l 
	Dec - 14


	0.742
	34
	10 Dec 2014
	7.83



	C12
	Nickel


	0.22 ug/l


	Dec - 14


	15.1
	34
	10 Dec 2014
	8.82



	C12
	Chloride


	TBA


	Dec - 14


	6000
	25
	10 Dec 2014
	21.5



	C12
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C12
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.005
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C13
	Am Nitrogen


	TBA


	Dec - 14


	8.06
	25
	10 Dec 2014
	10.6



	C13
	Cadmium


	1 ug/l 
	Dec - 14


	0.613
	34
	10 Dec 2014
	7.83



	C13
	Nickel


	0.22 ug/l


	Dec - 14


	40.6
	34
	10 Dec 2014
	8.82



	C13
	Chloride


	TBA


	Dec - 14


	4130
	25
	10 Dec 2014
	21.5



	C13
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C13
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.03
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	10.6



	C14
	Cadmium


	1 ug/l 
	Dec - 14


	No Sample
	34
	10 Dec 2014
	7.83



	C14
	Nickel


	0.22 ug/l


	Dec - 14


	No Sample
	34
	10 Dec 2014
	8.82



	C14
	Chloride


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	21.5



	C14
	MP Xylene


	1 ug/l 
	Dec - 14


	No Sample
	54
	10 Dec 2014
	

	C14
	Mecoprop


	0.1 ug/l 
	Dec - 14


	No Sample
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C15
	Am Nitrogen


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	10.6



	C15
	Cadmium


	1 ug/l 
	Dec - 14


	No Sample
	34
	10 Dec 2014
	7.83



	C15
	Nickel


	0.22 ug/l


	Dec - 14


	No Sample
	34
	10 Dec 2014
	8.82



	C15
	Chloride


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	21.5



	C15
	MP Xylene


	1 ug/l 
	Dec - 14


	No Sample
	54
	10 Dec 2014
	

	C15
	Mecoprop


	0.1 ug/l 
	Dec - 14


	No Sample
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Dec - 14


	1.11
	25
	10 Dec 2014
	10.6



	C16
	Cadmium


	1 ug/l 
	Dec - 14


	<1
	34
	10 Dec 2014
	7.83



	C16
	Nickel


	0.22 ug/l


	Dec - 14


	15.8
	34
	10 Dec 2014
	8.82



	C16
	Chloride


	TBA


	Dec - 14


	7180
	25
	10 Dec 2014
	21.5



	C16
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C16
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.03
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C17
	Am Nitrogen


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	10.6



	C17
	Cadmium


	1 ug/l 
	Dec - 14


	No Sample
	34
	10 Dec 2014
	7.83



	C17
	Nickel


	0.22 ug/l


	Dec - 14


	No Sample
	34
	10 Dec 2014
	8.82



	C17
	Chloride


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	21.5



	C17
	MP Xylene


	1 ug/l 
	Dec - 14


	No Sample
	54
	10 Dec 2014
	

	C17
	Mecoprop


	0.1 ug/l 
	Dec - 14


	No Sample
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Dec - 14


	14.4
	25
	10 Dec 2014
	10.6



	C18
	Cadmium


	1 ug/l 
	Dec - 14


	0.168
	34
	10 Dec 2014
	7.83



	C18
	Nickel


	0.22 ug/l


	Dec - 14


	4.85
	34
	10 Dec 2014
	8.82



	C18
	Chloride


	TBA


	Dec - 14


	4040
	25
	10 Dec 2014
	21.5



	C18
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C18
	Mecoprop


	0.1 ug/l 
	Dec - 14


	0.009
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Dec - 14


	3.96
	25
	10 Dec 2014
	10.6



	C19
	Cadmium


	1 ug/l 
	Dec - 14


	<0.1
	34
	10 Dec 2014
	7.83



	C19
	Nickel


	0.22 ug/l


	Dec - 14


	5.56
	34
	10 Dec 2014
	8.82



	C19
	Chloride


	TBA


	Dec - 14


	1980
	25
	10 Dec 2014
	21.5



	C19
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C19
	Mecoprop


	0.1 ug/l 
	Dec - 14


	0.007
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	10.6



	C20
	Cadmium


	1 ug/l 
	Dec - 14


	No Sample
	34
	10 Dec 2014
	7.83



	C20
	Nickel


	0.22 ug/l


	Dec - 14


	No Sample
	34
	10 Dec 2014
	8.82



	C20
	Chloride


	TBA


	Dec - 14


	No Sample
	25
	10 Dec 2014
	21.5



	C20
	MP Xylene


	1 ug/l 
	Dec - 14


	No Sample
	54
	10 Dec 2014
	

	C20
	Mecoprop


	0.1 ug/l 
	Dec - 14


	No Sample
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	TBA


	Dec - 14


	0.101
	25
	10 Dec 2014
	10.6



	C21
	Cadmium


	1 ug/l 
	Dec - 14


	0.261
	34
	10 Dec 2014
	7.83



	C21
	Nickel


	0.22 ug/l


	Dec - 14


	11.6
	34
	10 Dec 2014
	8.82



	C21
	Chloride


	TBA


	Dec - 14


	862
	25
	10 Dec 2014
	21.5



	C21
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C21
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.005
	1214
	10 Dec 2014
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Dec - 14


	3.94
	25
	10 Dec 2014
	10.6



	C22
	Cadmium


	1 ug/l 
	Dec - 14


	<0.1
	34
	10 Dec 2014
	7.83



	C22
	Nickel


	0.22 ug/l


	Dec - 14


	2.81
	34
	10 Dec 2014
	8.82



	C22
	Chloride


	TBA


	Dec - 14


	7750
	25
	10 Dec 2014
	21.5



	C22
	MP Xylene


	1 ug/l 
	Dec - 14


	<0.2
	54
	10 Dec 2014
	

	C22
	Mecoprop


	0.1 ug/l 
	Dec - 14


	<0.005
	1214
	10 Dec 2014
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………10 Dec 2014……………..  


(Authorised to sign as representative of Operator)

