Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…AUG15-C…
Reporting of ……Ground Water…… monitoring for the period for … August 2015…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Aug - 15

	0.553
	25
	31st Aug

	10.6



	C1


	Cadmium


	1 ug/l 
	Aug - 15

	
	34
	31st Aug


	7.83



	C1


	Nickel


	0.22 ug/l


	Aug - 15

	
	34
	31st Aug


	8.82



	C1


	Chloride
	TBA


	Aug - 15

	166
	25
	31st Aug


	21.5



	C1


	MP Xylene


	1 ug/l 
	Aug - 15

	
	54
	31st Aug


	

	C1


	Mecoprop


	0.1 ug/l 
	Aug - 15

	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Aug - 15


	2.87
	25
	31st Aug


	10.6



	C2
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C2
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C2
	Chloride


	TBA


	Aug - 15


	1170
	25
	31st Aug


	21.5



	C2
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C2
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Aug - 15


	3.63
	25
	31st Aug


	10.6



	C3
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C3
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C3
	Chloride


	TBA


	Aug - 15


	1180
	25
	31st Aug


	21.5



	C3
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C3
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Aug - 15


	2.47
	25
	31st Aug


	10.6



	C4
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C4
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C4
	Chloride


	TBA


	Aug - 15


	1180
	25
	31st Aug


	21.5



	C4
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C4
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Aug - 15


	4.84
	25
	31st Aug


	10.6



	C5
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C5
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C5
	Chloride


	TBA


	Aug - 15


	1190
	25
	31st Aug


	21.5



	C5
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C5
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Aug - 15


	No sample


	25
	31st Aug


	10.6



	C6
	Cadmium


	1 ug/l 
	Aug - 15


	No sample


	34
	31st Aug


	7.83



	C6
	Nickel


	0.22 ug/l


	Aug - 15


	No sample


	34
	31st Aug


	8.82



	C6
	Chloride


	TBA


	Aug - 15


	No sample


	25
	31st Aug


	21.5



	C6
	MP Xylene


	1 ug/l 
	Aug - 15


	No sample


	54
	31st Aug


	

	C6
	Mecoprop


	0.1 ug/l 
	Aug - 15


	No sample


	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C7
	Am Nitrogen


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	10.6



	C7
	Cadmium


	1 ug/l 
	Aug - 15


	NO SAMPLE
	34
	31st Aug


	7.83



	C7
	Nickel


	0.22 ug/l


	Aug - 15


	NO SAMPLE
	34
	31st Aug


	8.82



	C7
	Chloride


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	21.5



	C7
	MP Xylene


	1 ug/l 
	Aug - 15


	NO SAMPLE
	54
	31st Aug


	

	C7
	Mecoprop


	0.1 ug/l 
	Aug - 15


	NO SAMPLE
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Aug - 15


	1.21
	25
	31st Aug


	10.6



	C8
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C8
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C8
	Chloride


	TBA


	Aug - 15


	450
	25
	31st Aug


	21.5



	C8
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C8
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C9
	Am Nitrogen


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	10.6



	C9
	Cadmium


	1 ug/l 
	Aug - 15


	NO SAMPLE
	34
	31st Aug


	7.83



	C9
	Nickel


	0.22 ug/l


	Aug - 15


	NO SAMPLE
	34
	31st Aug


	8.82



	C9
	Chloride


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	21.5



	C9
	MP Xylene


	1 ug/l 
	Aug - 15


	NO SAMPLE
	54
	31st Aug


	

	C9
	Mecoprop


	0.1 ug/l 
	Aug - 15


	NO SAMPLE
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Aug - 15


	3.62
	25
	31st Aug


	10.6



	C10
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C10
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C10
	Chloride


	TBA


	Aug - 15


	451
	25
	31st Aug


	21.5



	C10
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C10
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C11
	Am Nitrogen


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	10.6



	C11
	Cadmium


	1 ug/l 
	Aug - 15


	NO SAMPLE
	34
	31st Aug


	7.83



	C11
	Nickel


	0.22 ug/l


	Aug - 15


	NO SAMPLE
	34
	31st Aug


	8.82



	C11
	Chloride


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	21.5



	C11
	MP Xylene


	1 ug/l 
	Aug - 15


	NO SAMPLE
	54
	31st Aug


	

	C11
	Mecoprop


	0.1 ug/l 
	Aug - 15


	NO SAMPLE
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Aug - 15


	0.442
	25
	31st Aug


	10.6



	C12
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C12
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C12
	Chloride


	TBA


	Aug - 15


	69.5
	25
	31st Aug


	21.5



	C12
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C12
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C13
	Am Nitrogen


	TBA


	Aug - 15


	0.402
	25
	31st Aug


	10.6



	C13
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C13
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C13
	Chloride


	TBA


	Aug - 15


	70.1
	25
	31st Aug


	21.5



	C13
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C13
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	TBA


	Aug - 15


	4.10
	25
	31st Aug


	10.6



	C14
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C14
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C14
	Chloride


	TBA


	Aug - 15


	75.4
	25
	31st Aug


	21.5



	C14
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C14
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C15
	Am Nitrogen


	TBA


	Aug - 15


	6.09
	25
	31st Aug


	10.6



	C15
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C15
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C15
	Chloride


	TBA


	Aug - 15


	78.2
	25
	31st Aug


	21.5



	C15
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C15
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Aug - 15


	0.524
	25
	31st Aug


	10.6



	C16
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C16
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C16
	Chloride


	TBA


	Aug - 15


	70.6
	25
	31st Aug


	21.5



	C16
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C16
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C17
	Am Nitrogen


	TBA


	Aug - 15


	
	25
	31st Aug


	10.6



	C17
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C17
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C17
	Chloride


	TBA


	Aug - 15


	
	25
	31st Aug


	21.5



	C17
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C17
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Aug - 15


	0.274
	25
	31st Aug


	10.6



	C18
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C18
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C18
	Chloride


	TBA


	Aug - 15


	61.9
	25
	31st Aug


	21.5



	C18
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C18
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Aug - 15


	0.288
	25
	31st Aug


	10.6



	C19
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C19
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C19
	Chloride


	TBA


	Aug - 15


	62.1
	25
	31st Aug


	21.5



	C19
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C19
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	10.6



	C20
	Cadmium


	1 ug/l 
	Aug - 15


	NO SAMPLE
	34
	31st Aug


	7.83



	C20
	Nickel


	0.22 ug/l


	Aug - 15


	NO SAMPLE
	34
	31st Aug


	8.82



	C20
	Chloride


	TBA


	Aug - 15


	NO SAMPLE
	25
	31st Aug


	21.5



	C20
	MP Xylene


	1 ug/l 
	Aug - 15


	NO SAMPLE
	54
	31st Aug


	

	C20
	Mecoprop


	0.1 ug/l 
	Aug - 15


	NO SAMPLE
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	TBA


	Aug - 15


	17.4
	25
	31st Aug


	10.6



	C21
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C21
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C21
	Chloride


	TBA


	Aug - 15


	85.9
	25
	31st Aug


	21.5



	C21
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C21
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Aug - 15


	0.388
	25
	31st Aug


	10.6



	C22
	Cadmium


	1 ug/l 
	Aug - 15


	
	34
	31st Aug


	7.83



	C22
	Nickel


	0.22 ug/l


	Aug - 15


	
	34
	31st Aug


	8.82



	C22
	Chloride


	TBA


	Aug - 15


	62.3
	25
	31st Aug


	21.5



	C22
	MP Xylene


	1 ug/l 
	Aug - 15


	
	54
	31st Aug


	

	C22
	Mecoprop


	0.1 ug/l 
	Aug - 15


	
	1214
	31st Aug


	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………Gareth Ffoulkes……………………….  

Date………30/10/15………………..   



(Authorised to sign as representative of Operator)

