Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…July16-C…
Reporting of ……Ground Water…… monitoring for the period for … July 2016…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Jul-16

	0.587
	25
	28 Jul 2016
	10.6



	C1


	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C1


	Nickel


	0.22 ug/l

	Jul-16

	
	34
	28 Jul 2016
	8.82



	C1


	Chloride
	TBA


	Jul-16

	157
	25
	28 Jul 2016
	21.5



	C1


	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C1


	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Jul-16

	<0.0300
	25
	28 Jul 2016
	10.6



	C2
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C2
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C2
	Chloride


	TBA


	Jul-16

	69.6
	25
	28 Jul 2016
	21.5



	C2
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C2
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Jul-16

	<0.0300
	25
	28 Jul 2016
	10.6



	C3
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C3
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C3
	Chloride


	TBA


	Jul-16

	69.9
	25
	28 Jul 2016
	21.5



	C3
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C3
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Jul-16

	12.0
	25
	28 Jul 2016
	10.6



	C4
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C4
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C4
	Chloride


	TBA


	Jul-16

	3190
	25
	28 Jul 2016
	21.5



	C4
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C4
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Jul-16

	12.0
	25
	28 Jul 2016
	10.6



	C5
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C5
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C5
	Chloride


	TBA


	Jul-16

	3170
	25
	28 Jul 2016
	21.5



	C5
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C5
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Jul-16

	<0.0300
	25
	28 Jul 2016
	10.6



	C6
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C6
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C6
	Chloride


	TBA


	Jul-16

	700
	25
	28 Jul 2016
	21.5



	C6
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C6
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Jul-16

	12.4
	25
	28 Jul 2016
	10.6



	C8
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C8
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C8
	Chloride


	TBA


	Jul-16

	5560
	25
	28 Jul 2016
	21.5



	C8
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C8
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Jul-16

	12.3
	25
	28 Jul 2016
	10.6



	C10
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C10
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C10
	Chloride


	TBA


	Jul-16

	3190
	25
	28 Jul 2016
	21.5



	C10
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C10
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Jul-16

	12.4
	25
	28 Jul 2016
	10.6



	C12
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C12
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C12
	Chloride


	TBA


	Jul-16

	3190
	25
	28 Jul 2016
	21.5



	C12
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C12
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C13
	Am Nitrogen


	TBA


	Jul-16

	12.0
	25
	28 Jul 2016
	10.6



	C13
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C13
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C13
	Chloride


	TBA


	Jul-16

	3210
	25
	28 Jul 2016
	21.5



	C13
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C13
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	TBA


	Jul-16

	11.9
	25
	28 Jul 2016
	10.6



	C14
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C14
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C14
	Chloride


	TBA


	Jul-16

	3180
	25
	28 Jul 2016
	21.5



	C14
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C14
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Jul-16

	0.0700
	25
	28 Jul 2016
	10.6



	C16
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C16
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C16
	Chloride


	TBA


	Jul-16

	102
	25
	28 Jul 2016
	21.5



	C16
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C16
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Jul-16

	0.114
	25
	28 Jul 2016
	10.6



	C18
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C18
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C18
	Chloride


	TBA


	Jul-16

	1010
	25
	28 Jul 2016
	21.5



	C18
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C18
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Jul-16

	<0.0300
	25
	28 Jul 2016
	10.6



	C19
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C19
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C19
	Chloride


	TBA


	Jul-16

	6890
	25
	28 Jul 2016
	21.5



	C19
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C19
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Jul-16

	0.0620
	25
	28 Jul 2016
	10.6



	C20
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C20
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C20
	Chloride


	TBA


	Jul-16

	1020
	25
	28 Jul 2016
	21.5



	C20
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C20
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Jul-16

	0.0760
	25
	28 Jul 2016
	10.6



	C22
	Cadmium


	1 ug/l 
	Jul-16

	
	34
	28 Jul 2016
	7.83



	C22
	Nickel


	0.22 ug/l


	Jul-16

	
	34
	28 Jul 2016
	8.82



	C22
	Chloride


	TBA


	Jul-16

	8670
	25
	28 Jul 2016
	21.5



	C22
	MP Xylene


	1 ug/l 
	Jul-16

	
	54
	28 Jul 2016
	

	C22
	Mecoprop


	0.1 ug/l 
	Jul-16

	
	1214
	28 Jul 2016
	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………Gareth Ffoulkes……………………….  

Date………28/11/16………………..   



(Authorised to sign as representative of Operator)

