Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…SEPT16-C…
Reporting of ……Ground Water…… monitoring for the period for … September  2016…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Sep - 16

	0.537
	25
	30 Sept 2016
	10.6



	C1


	Cadmium


	1 ug/l 
	Sep - 16

	4.65
	34
	30 Sept 2016
	7.83



	C1


	Nickel


	0.22 ug/l


	Sep - 16

	2.79
	34
	30 Sept 2016
	8.82



	C1


	Chloride
	TBA


	Sep - 16

	190
	25
	30 Sept 2016
	21.5



	C1


	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C1


	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.0273
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Sep - 16

	<0.0300
	25
	30 Sept 2016
	10.6



	C2
	Cadmium


	1 ug/l 
	Sep - 16

	0.330
	34
	30 Sept 2016
	7.83



	C2
	Nickel


	0.22 ug/l


	Sep - 16

	11.4
	34
	30 Sept 2016
	8.82



	C2
	Chloride


	TBA


	Sep - 16

	67.1
	25
	30 Sept 2016
	21.5



	C2
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C2
	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.0495
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Sep - 16

	<0.0300
	25
	30 Sept 2016
	10.6



	C3
	Cadmium


	1 ug/l 
	Sep - 16

	0.336
	34
	30 Sept 2016
	7.83



	C3
	Nickel


	0.22 ug/l


	Sep - 16

	11.9
	34
	30 Sept 2016
	8.82



	C3
	Chloride


	TBA


	Sep - 16

	66.3
	25
	30 Sept 2016
	21.5



	C3
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C3
	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.0515
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Sep - 16

	4.44
	25
	30 Sept 2016
	10.6



	C4
	Cadmium


	1 ug/l 
	Sep - 16

	0.527
	34
	30 Sept 2016
	7.83



	C4
	Nickel


	0.22 ug/l


	Sep - 16

	7.81
	34
	30 Sept 2016
	8.82



	C4
	Chloride


	TBA


	Sep - 16

	931
	25
	30 Sept 2016
	21.5



	C4
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C4
	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.593
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Sep - 16

	10.6
	25
	30 Sept 2016
	10.6



	C5
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C5
	Nickel


	0.22 ug/l


	Sep - 16

	39.7
	34
	30 Sept 2016
	8.82



	C5
	Chloride


	TBA


	Sep - 16

	3240
	25
	30 Sept 2016
	21.5



	C5
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C5
	Mecoprop


	0.1 ug/l 
	Sep - 16

	<0.005
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Sep - 16

	1.99
	25
	30 Sept 2016
	10.6



	C6
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C6
	Nickel


	0.22 ug/l


	Sep - 16

	8.48
	34
	30 Sept 2016
	8.82



	C6
	Chloride


	TBA


	Sep - 16

	5530
	25
	30 Sept 2016
	21.5



	C6
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C6
	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.181
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Sep - 16

	4.93
	25
	30 Sept 2016
	10.6



	C8
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C8
	Nickel


	0.22 ug/l


	Sep - 16

	14.7
	34
	30 Sept 2016
	8.82



	C8
	Chloride


	TBA


	Sep - 16

	24.0
	25
	30 Sept 2016
	21.5



	C8
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C8
	Mecoprop


	0.1 ug/l 
	Sep - 16

	<0.005
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Sep - 16

	8.63
	25
	30 Sept 2016
	10.6



	C10
	Cadmium


	1 ug/l 
	Sep - 16

	0.733
	34
	30 Sept 2016
	7.83



	C10
	Nickel


	0.22 ug/l


	Sep - 16

	8.38
	34
	30 Sept 2016
	8.82



	C10
	Chloride


	TBA


	Sep - 16

	1630
	25
	30 Sept 2016
	21.5



	C10
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C10
	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.623
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Sep - 16

	18.8
	25
	30 Sept 2016
	10.6



	C12
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C12
	Nickel


	0.22 ug/l


	Sep - 16

	9.67
	34
	30 Sept 2016
	8.82



	C12
	Chloride


	TBA


	Sep - 16

	168
	25
	30 Sept 2016
	21.5



	C12
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C12
	Mecoprop


	0.1 ug/l 
	Sep - 16

	<0.005
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	TBA


	Sep - 16

	7.62
	25
	30 Sept 2016
	10.6



	C14
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C14
	Nickel


	0.22 ug/l


	Sep - 16

	10.0
	34
	30 Sept 2016
	8.82



	C14
	Chloride


	TBA


	Sep - 16

	3850
	25
	30 Sept 2016
	21.5



	C14
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C14
	Mecoprop


	0.1 ug/l 
	Sep - 16

	<0.005
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Sep - 16

	1.59
	25
	30 Sept 2016
	10.6



	C16
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C16
	Nickel


	0.22 ug/l


	Sep - 16

	5.85
	34
	30 Sept 2016
	8.82



	C16
	Chloride


	TBA


	Sep - 16

	10400
	25
	30 Sept 2016
	21.5



	C16
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C16
	Mecoprop


	0.1 ug/l 
	Sep - 16

	<0.005
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C17
	Am Nitrogen


	TBA


	Sep - 16

	No Sample
	25
	30 Sept 2016
	10.6



	C17
	Cadmium


	1 ug/l 
	Sep - 16

	No Sample
	34
	30 Sept 2016
	7.83



	C17
	Nickel


	0.22 ug/l


	Sep - 16

	No Sample
	34
	30 Sept 2016
	8.82



	C17
	Chloride


	TBA


	Sep - 16

	No Sample
	25
	30 Sept 2016
	21.5



	C17
	MP Xylene


	1 ug/l 
	Sep - 16

	No Sample
	54
	30 Sept 2016
	

	C17
	Mecoprop


	0.1 ug/l 
	Sep - 16

	No Sample
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Sep - 16

	4.01
	25
	30 Sept 2016
	10.6



	C18
	Cadmium


	1 ug/l 
	Sep - 16

	0.181
	34
	30 Sept 2016
	7.83



	C18
	Nickel


	0.22 ug/l


	Sep - 16

	8.28
	34
	30 Sept 2016
	8.82



	C18
	Chloride


	TBA


	Sep - 16

	9120
	25
	30 Sept 2016
	21.5



	C18
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C18
	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.439
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Sep - 16

	<0.0300
	25
	30 Sept 2016
	10.6



	C19
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C19
	Nickel


	0.22 ug/l


	Sep - 16

	5.34
	34
	30 Sept 2016
	8.82



	C19
	Chloride


	TBA


	Sep - 16

	482
	25
	30 Sept 2016
	21.5



	C19
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C19
	Mecoprop


	0.1 ug/l 
	Sep - 16

	0.00773
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Sep - 16

	NO SAMPLE
	25
	30 Sept 2016
	10.6



	C20
	Cadmium


	1 ug/l 
	Sep - 16

	NO SAMPLE
	34
	30 Sept 2016
	7.83



	C20
	Nickel


	0.22 ug/l


	Sep - 16

	NO SAMPLE
	34
	30 Sept 2016
	8.82



	C20
	Chloride


	TBA


	Sep - 16

	NO SAMPLE
	25
	30 Sept 2016
	21.5



	C20
	MP Xylene


	1 ug/l 
	Sep - 16

	NO SAMPLE
	54
	30 Sept 2016
	

	C20
	Mecoprop


	0.1 ug/l 
	Sep - 16

	NO SAMPLE
	1214
	30 Sept 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Sep - 16

	0.399
	25
	30 Sept 2016
	10.6



	C22
	Cadmium


	1 ug/l 
	Sep - 16

	<0.1
	34
	30 Sept 2016
	7.83



	C22
	Nickel


	0.22 ug/l


	Sep - 16

	4.06
	34
	30 Sept 2016
	8.82



	C22
	Chloride


	TBA


	Sep - 16

	3950
	25
	30 Sept 2016
	21.5



	C22
	MP Xylene


	1 ug/l 
	Sep - 16

	<0.2
	54
	30 Sept 2016
	

	C22
	Mecoprop


	0.1 ug/l 
	Sep - 16

	<0.005
	1214
	30 Sept 2016
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………Gareth Ffoulkes……………………….  

Date………28/11/16………………..   



(Authorised to sign as representative of Operator)

