Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Carfiff

Installation:

Lamby Way Landfill Site

Form Number: 
…AUG16-L…
Reporting of ……LEACHATE…… monitoring for the period for … August 2016……..
	Monitoring

Point
	Substance /

Parameter
	Trigger level
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	L2
	Am Nitrogen
	904

	Aug - 16

	1150
	678
	31st Aug 2016
	10.6



	L2
	Cadmium
	0.05

	Aug - 16

	<2.00
	34
	31st Aug 2016
	7.83



	L2
	Nickel
	0.4

	Aug - 16

	262
	34
	31st Aug 2016
	8.82



	
	
	
	
	
	
	
	

	L2
	Chloride
	1306
	Aug - 16

	1330
	678
	31st Aug 2016
	21.5



	L2
	MP Xylene
	0.032
	Aug - 16

	3.49
	54
	31st Aug 2016
	

	
	
	
	
	
	
	
	

	
	MP Xylene


	
	
	
	
	
	

	L2
	Mecoprop
	0.024

	Aug - 16

	40.3
	1214
	31st Aug 2016
	14.6



	
	
	
	
	
	
	
	


	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	L4
	Am Nitrogen


	1370


	Aug - 16

	1140
	678
	31st Aug 2016
	10.6



	L4
	Cadmium


	0.1


	Aug - 16

	<2.00
	34
	31st Aug 2016
	7.83



	L4
	Nickel


	0.1


	Aug - 16

	261
	34
	31st Aug 2016
	8.82



	L4
	Chloride


	13713


	Aug - 16

	1300
	678
	31st Aug 2016
	21.5



	L4
	MP Xylene


	0.029


	Aug - 16

	5.30
	54
	31st Aug 2016
	

	L4
	Mecoprop


	0.032


	Aug - 16

	43.8
	1214
	31st Aug 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	L7
	Am Nitrogen


	1370


	Aug - 16

	1140
	678
	31st Aug 2016
	10.6



	L7
	Cadmium


	0.1


	Aug - 16

	<2.00
	34
	31st Aug 2016
	7.83



	L7
	Nickel


	0.1


	Aug - 16

	260
	34
	31st Aug 2016
	8.82



	L7
	Chloride


	13713


	Aug - 16

	1310
	678
	31st Aug 2016
	21.5



	L7
	MP Xylene


	0.029


	Aug - 16

	5.10
	54
	31st Aug 2016
	

	L7
	Mecoprop


	0.032


	Aug - 16

	43.8
	1214
	31st Aug 2016
	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………Gareth Ffoulkes……………………….  

Date………28/11/16………………..   



(Authorised to sign as representative of Operator)

