Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…DEC16-SL…
Reporting of ……LEACHATE…… monitoring for the period for …December 2016…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL1


	Am Nitrogen


	1370


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	10.6



	SL1


	Cadmium


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	7.83



	SL1


	Nickel


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	8.82



	SL1


	Chloride
	13713


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	21.5



	SL1


	MP Xylene


	0.029


	Dec -16

	NO SAMPLE
	T54
	10th Dec 2016
	

	SL1


	Mecoprop


	0.032


	Dec -16

	NO SAMPLE
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL2
	Am Nitrogen


	1370


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	10.6



	SL2
	Cadmium


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	7.83



	SL2
	Nickel


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	8.82



	SL2
	Chloride


	13713


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	21.5



	SL2
	MP Xylene


	0.029


	Dec -16

	NO SAMPLE
	T54
	10th Dec 2016
	

	SL2
	Mecoprop


	0.032


	Dec -16

	NO SAMPLE
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL3
	Am Nitrogen


	1370


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	10.6



	SL3
	Cadmium


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	7.83



	SL3
	Nickel


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	8.82



	SL3
	Chloride


	13713


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	21.5



	SL3
	MP Xylene


	0.029


	Dec -16

	NO SAMPLE
	T54
	10th Dec 2016
	

	SL3
	Mecoprop


	0.032


	Dec -16

	NO SAMPLE
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL4
	Am Nitrogen


	1370


	Dec -16

	390
	T686
	10th Dec 2016
	10.6



	SL4
	Cadmium


	0.1


	Dec -16

	<0.00050
	T301
	10th Dec 2016
	7.83



	SL4
	Nickel


	0.1


	Dec -16

	<0.025
	T301
	10th Dec 2016
	8.82



	SL4
	Chloride


	13713


	Dec -16

	670
	T686
	10th Dec 2016
	21.5



	SL4
	MP Xylene


	0.029


	Dec -16

	<1
	T54
	10th Dec 2016
	

	SL4
	Mecoprop


	0.032


	Dec -16

	6.1
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL5
	Am Nitrogen


	1370


	Dec -16

	620
	T686
	10th Dec 2016
	10.6



	SL5
	Cadmium


	0.1


	Dec -16

	<0.00050
	T301
	10th Dec 2016
	7.83



	SL5
	Nickel


	0.1


	Dec -16

	0.039
	T301
	10th Dec 2016
	8.82



	SL5
	Chloride


	13713


	Dec -16

	970
	T686
	10th Dec 2016
	21.5



	SL5
	MP Xylene


	0.029


	Dec -16

	<1
	T54
	10th Dec 2016
	

	SL5
	Mecoprop


	0.032


	Dec -16

	8.1
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL6
	Am Nitrogen


	1370


	Dec -16

	490
	T686
	10th Dec 2016
	10.6



	SL6
	Cadmium


	0.1


	Dec -16

	<0.00050
	T301
	10th Dec 2016
	7.83



	SL6
	Nickel


	0.1


	Dec -16

	0.037
	T301
	10th Dec 2016
	8.82



	SL6
	Chloride


	13713


	Dec -16

	550
	T686
	10th Dec 2016
	21.5



	SL6
	MP Xylene


	0.029


	Dec -16

	<1
	T54
	10th Dec 2016
	

	SL6
	Mecoprop


	0.032


	Dec -16

	6.7
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL7
	Am Nitrogen


	1370


	Dec -16

	1100
	T686
	10th Dec 2016
	10.6



	SL7
	Cadmium


	0.1


	Dec -16

	<0.00050
	T301
	10th Dec 2016
	7.83



	SL7
	Nickel


	0.1


	Dec -16

	0.030
	T301
	10th Dec 2016
	8.82



	SL7
	Chloride


	13713


	Dec -16

	1900
	T686
	10th Dec 2016
	21.5



	SL7
	MP Xylene


	0.029


	Dec -16

	1
	T54
	10th Dec 2016
	

	SL7
	Mecoprop


	0.032


	Dec -16

	3.3
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL8
	Am Nitrogen


	1370


	Dec -16

	1800
	T686
	10th Dec 2016
	10.6



	SL8
	Cadmium


	0.1


	Dec -16

	<0.00050
	T301
	10th Dec 2016
	7.83



	SL8
	Nickel


	0.1


	Dec -16

	0.18
	T301
	10th Dec 2016
	8.82



	SL8
	Chloride


	13713


	Dec -16

	1500
	T686
	10th Dec 2016
	21.5



	SL8
	MP Xylene


	0.029


	Dec -16

	1
	T54
	10th Dec 2016
	

	SL8
	Mecoprop


	0.032


	Dec -16

	2
	T16
	10th Dec 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL9
	Am Nitrogen


	1370


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	10.6



	SL9
	Cadmium


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	7.83



	SL9
	Nickel


	0.1


	Dec -16

	NO SAMPLE
	T301
	10th Dec 2016
	8.82



	SL9
	Chloride


	13713


	Dec -16

	NO SAMPLE
	T686
	10th Dec 2016
	21.5



	SL9
	MP Xylene


	0.029


	Dec -16

	NO SAMPLE
	T54
	10th Dec 2016
	

	SL9
	Mecoprop


	0.032


	Dec -16

	NO SAMPLE
	T16
	10th Dec 2016
	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………14/1/17…………..     



(Authorised to sign as representative of Operator)

