Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Oct16-C…
Reporting of ……Ground Water…… monitoring for the period for … October  2016…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	N/A
	Oct  - 16
	0.86
	T686
	25th Oct 2016
	10.6



	C1


	Cadmium


	1 ug/l 
	Oct  - 16

	0.00012
	T301
	25th Oct 2016
	7.83



	C1


	Nickel


	0.22 ug/l


	Oct  - 16

	0.006
	T301
	25th Oct 2016
	8.82



	C1


	Chloride
	TBA


	Oct  - 16

	153
	T686
	25th Oct 2016
	21.5



	C1


	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C1


	Mecoprop


	0.1 ug/l 
	Oct  - 16

	0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	2.09 mg/l

	Oct  - 16
	<0.05
	T686
	25th Oct 2016
	10.6



	C2
	Cadmium


	1 ug/l 
	Oct  - 16

	0.00010
	T301
	25th Oct 2016
	7.83



	C2
	Nickel


	0.22 ug/l


	Oct  - 16

	0.006
	T301
	25th Oct 2016
	8.82



	C2
	Chloride


	TBA


	Oct  - 16

	43.3
	T686
	25th Oct 2016
	21.5



	C2
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C2
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	8.94 mg/l

	Oct  - 16
	3.1
	T686
	25th Oct 2016
	10.6



	C3
	Cadmium


	1 ug/l 
	Oct  - 16

	0.00094
	T301
	25th Oct 2016
	7.83



	C3
	Nickel


	0.22 ug/l


	Oct  - 16

	0.014
	T301
	25th Oct 2016
	8.82



	C3
	Chloride


	TBA


	Oct  - 16

	35.3
	T686
	25th Oct 2016
	21.5



	C3
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C3
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	11.4 mg/l
	Oct  - 16
	5.3
	T686
	25th Oct 2016
	10.6



	C4
	Cadmium


	1 ug/l 
	Oct  - 16

	<0.00020
	T301
	25th Oct 2016
	7.83



	C4
	Nickel


	0.22 ug/l


	Oct  - 16

	0.024
	T301
	25th Oct 2016
	8.82



	C4
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C4
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C4
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	20.87 mg/l
	Oct  - 16
	10
	T686
	25th Oct 2016
	10.6



	C5
	Cadmium


	1 ug/l 
	Oct  - 16

	0.00082
	T301
	25th Oct 2016
	7.83



	C5
	Nickel


	0.22 ug/l


	Oct  - 16

	0.008
	T301
	25th Oct 2016
	8.82



	C5
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C5
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C5
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	5.02 mg/l
	Oct  - 16
	1.7
	T686
	25th Oct 2016
	10.6



	C6
	Cadmium


	1 ug/l 
	Oct  - 16

	<0.00020
	T301
	25th Oct 2016
	7.83



	C6
	Nickel


	0.22 ug/l


	Oct  - 16

	0.016
	T301
	25th Oct 2016
	8.82



	C6
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C6
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C6
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	0.3
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	12.07 mg/l
	Oct  - 16
	6.3
	T686
	25th Oct 2016
	10.6



	C8
	Cadmium


	1 ug/l 
	Oct  - 16

	<0.00020
	T301
	25th Oct 2016
	7.83



	C8
	Nickel


	0.22 ug/l


	Oct  - 16

	0.025
	T301
	25th Oct 2016
	8.82



	C8
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C8
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C8
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	22.62 mg/l

	Oct  - 16
	5.3
	T686
	25th Oct 2016
	10.6



	C10
	Cadmium


	1 ug/l 
	Oct  - 16

	0.00027
	T301
	25th Oct 2016
	7.83



	C10
	Nickel


	0.22 ug/l


	Oct  - 16

	0.022
	T301
	25th Oct 2016
	8.82



	C10
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C10
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C10
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	19.49 mg/l
	Oct  - 16
	NO SAMPLE
	T686
	25th Oct 2016
	10.6



	C12
	Cadmium


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	7.83



	C12
	Nickel


	0.22 ug/l


	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	8.82



	C12
	Chloride


	TBA


	Oct  - 16

	NO SAMPLE
	T686
	25th Oct 2016
	21.5



	C12
	MP Xylene


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T54
	25th Oct 2016
	

	C12
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	NO SAMPLE
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	25.88 mg/l

	Oct  - 16
	NO SAMPLE
	T686
	25th Oct 2016
	10.6



	C14
	Cadmium


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	7.83



	C14
	Nickel


	0.22 ug/l


	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	8.82



	C14
	Chloride


	TBA


	Oct  - 16

	NO SAMPLE
	T686
	25th Oct 2016
	21.5



	C14
	MP Xylene


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T54
	25th Oct 2016
	

	C14
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	NO SAMPLE
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	12.62 mg/l
	Oct  - 16
	NO SAMPLE
	T686
	25th Oct 2016
	10.6



	C16
	Cadmium


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	7.83



	C16
	Nickel


	0.22 ug/l


	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	8.82



	C16
	Chloride


	TBA


	Oct  - 16

	NO SAMPLE
	T686
	25th Oct 2016
	21.5



	C16
	MP Xylene


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T54
	25th Oct 2016
	

	C16
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	NO SAMPLE
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	18.39 mg/l
	Oct  - 16
	5.3
	T686
	25th Oct 2016
	10.6



	C18
	Cadmium


	1 ug/l 
	Oct  - 16

	0.00027
	T301
	25th Oct 2016
	7.83



	C18
	Nickel


	0.22 ug/l


	Oct  - 16

	0.022
	T301
	25th Oct 2016
	8.82



	C18
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C18
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C18
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	0.4
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	19.03 mg/l
	Oct  - 16
	0.08
	T686
	25th Oct 2016
	10.6



	C19
	Cadmium


	1 ug/l 
	Oct  - 16

	<0.00010
	T301
	25th Oct 2016
	7.83



	C19
	Nickel


	0.22 ug/l


	Oct  - 16

	0.016
	T301
	25th Oct 2016
	8.82



	C19
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C19
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C19
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	15.4 mg/l

	Oct  - 16
	NO SAMPLE
	T686
	25th Oct 2016
	10.6



	C20
	Cadmium


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	7.83



	C20
	Nickel


	0.22 ug/l


	Oct  - 16

	NO SAMPLE
	T301
	25th Oct 2016
	8.82



	C20
	Chloride


	TBA


	Oct  - 16

	NO SAMPLE
	T686
	25th Oct 2016
	21.5



	C20
	MP Xylene


	1 ug/l 
	Oct  - 16

	NO SAMPLE
	T54
	25th Oct 2016
	

	C20
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	NO SAMPLE
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	9.65 mg/l
	Oct  - 16
	0.31
	T686
	25th Oct 2016
	10.6



	C21
	Cadmium


	1 ug/l 
	Oct  - 16

	0.00022
	T301
	25th Oct 2016
	7.83



	C21
	Nickel


	0.22 ug/l


	Oct  - 16

	0.021
	T301
	25th Oct 2016
	8.82



	C21
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C21
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C21
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	12.10 mg/l
	Oct  - 16
	5.0
	T686
	25th Oct 2016
	10.6



	C22
	Cadmium


	1 ug/l 
	Oct  - 16

	<0.00020
	T301
	25th Oct 2016
	7.83



	C22
	Nickel


	0.22 ug/l


	Oct  - 16

	0.022
	T301
	25th Oct 2016
	8.82



	C22
	Chloride


	TBA


	Oct  - 16

	
	T686
	25th Oct 2016
	21.5



	C22
	MP Xylene


	1 ug/l 
	Oct  - 16

	<1
	T54
	25th Oct 2016
	

	C22
	Mecoprop


	0.1 ug/l 
	Oct  - 16

	<0.1
	T16
	25th Oct 2016
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………14/1/17…………..     



(Authorised to sign as representative of Operator)
