Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…JUNE17-C…
Reporting of ……Ground Water…… monitoring for the period for … June 2017…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	June - 17

	0.50
	T686
	28th June


	10.6



	C1


	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C1


	Nickel


	0.22 ug/l


	June - 17

	<2
	T301
	28th June


	8.82



	C1


	Chloride
	TBA


	June - 17

	189
	T686
	28th June


	21.5



	C1


	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C1


	Mecoprop


	0.1 ug/l 
	June - 17

	0.0355
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	2.09 mg/l


	June - 17

	<0.0300
	T686
	28th June


	10.6



	C2
	Cadmium


	1 ug/l 
	June - 17

	0.568
	T301
	28th June


	7.83



	C2
	Nickel


	0.22 ug/l


	June - 17

	3.12
	T301
	28th June


	8.82



	C2
	Chloride


	TBA


	June - 17

	48.3
	T686
	28th June


	21.5



	C2
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C2
	Mecoprop


	0.1 ug/l 
	June - 17

	0.0351
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	8.94 mg/l


	June - 17

	3.46
	T686
	28th June


	10.6



	C3
	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C3
	Nickel


	0.22 ug/l


	June - 17

	3.37
	T301
	28th June


	8.82



	C3
	Chloride


	TBA


	June - 17

	1070
	T686
	28th June


	21.5



	C3
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C3
	Mecoprop


	0.1 ug/l 
	June - 17

	0.0309
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	11.4 mg/l 
	June - 17

	7.53
	T686
	28th June


	10.6



	C4
	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C4
	Nickel


	0.22 ug/l


	June - 17

	2.29
	T301
	28th June


	8.82



	C4
	Chloride


	TBA


	June - 17

	2110
	T686
	28th June


	21.5



	C4
	MP Xylene


	1 ug/l 
	June - 17

	<0.001
	T54
	28th June


	

	C4
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	20.87 mg/l 
	June - 17

	11.8
	T686
	28th June


	10.6



	C5
	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C5
	Nickel


	0.22 ug/l


	June - 17

	10.5
	T301
	28th June


	8.82



	C5
	Chloride


	TBA


	June - 17

	3410
	T686
	28th June


	21.5



	C5
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C5
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	5.02 mg/l 
	June - 17

	1.22
	T686
	28th June


	10.6



	C6
	Cadmium


	1 ug/l 
	June - 17

	<1
	T301
	28th June


	7.83



	C6
	Nickel


	0.22 ug/l


	June - 17

	<10
	T301
	28th June


	8.82



	C6
	Chloride


	TBA


	June - 17

	5480
	T686
	28th June


	21.5



	C6
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C6
	Mecoprop


	0.1 ug/l 
	June - 17

	0.201
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	12.07 mg/l 
	June - 17

	5.66
	T686
	28th June


	10.6



	C8
	Cadmium


	1 ug/l 
	June - 17

	<1
	T301
	28th June


	7.83



	C8
	Nickel


	0.22 ug/l


	June - 17

	<10
	T301
	28th June


	8.82



	C8
	Chloride


	TBA


	June - 17

	6560
	T686
	28th June


	21.5



	C8
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C8
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	22.62 mg/l


	June - 17

	19.1
	T686
	28th June


	10.6



	C10
	Cadmium


	1 ug/l 
	June - 17

	1.45
	T301
	28th June


	7.83



	C10
	Nickel


	0.22 ug/l


	June - 17

	7.44
	T301
	28th June


	8.82



	C10
	Chloride


	TBA


	June - 17

	3780
	T686
	28th June


	21.5



	C10
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C10
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	19.49 mg/l 
	June - 17

	19.0 
	T686
	28th June


	10.6



	C12
	Cadmium


	1 ug/l 
	June - 17

	<1
	T301
	28th June


	7.83



	C12
	Nickel


	0.22 ug/l


	June - 17

	18.2
	T301
	28th June


	8.82



	C12
	Chloride


	TBA


	June - 17

	5670
	T686
	28th June


	21.5



	C12
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C12
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	25.88 mg/l


	June - 17

	6.01
	T686
	28th June


	10.6



	C14
	Cadmium


	1 ug/l 
	June - 17

	1.69
	T301
	28th June


	7.83



	C14
	Nickel


	0.22 ug/l


	June - 17

	60.5
	T301
	28th June


	8.82



	C14
	Chloride


	TBA


	June - 17

	65100
	T686
	28th June


	21.5



	C14
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C14
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	12.62 mg/l 
	June - 17

	5.07
	T686
	28th June


	10.6



	C16
	Cadmium


	1 ug/l 
	June - 17

	1.62
	T301
	28th June


	7.83



	C16
	Nickel


	0.22 ug/l


	June - 17

	<5
	T301
	28th June


	8.82



	C16
	Chloride


	TBA


	June - 17

	7310
	T686
	28th June


	21.5



	C16
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C16
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	18.39 mg/l 
	June - 17

	21.1
	T686
	28th June


	10.6



	C18
	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C18
	Nickel


	0.22 ug/l


	June - 17

	4.45
	T301
	28th June


	8.82



	C18
	Chloride


	TBA


	June - 17

	5320
	T686
	28th June


	21.5



	C18
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C18
	Mecoprop


	0.1 ug/l 
	June - 17

	0.0170
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	19.03 mg/l 
	June - 17

	0.0900
	T686
	28th June


	10.6



	C19
	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C19
	Nickel


	0.22 ug/l


	June - 17

	4.35
	T301
	28th June


	8.82



	C19
	Chloride


	TBA


	June - 17

	691
	T686
	28th June


	21.5



	C19
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C19
	Mecoprop


	0.1 ug/l 
	June - 17

	0.0198
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	15.4 mg/l


	June - 17

	<0.0300
	T686
	28th June


	10.6



	C20
	Cadmium


	1 ug/l 
	June - 17

	0.551
	T301
	28th June


	7.83



	C20
	Nickel


	0.22 ug/l


	June - 17

	5.97
	T301
	28th June


	8.82



	C20
	Chloride


	TBA


	June - 17

	46.8
	T686
	28th June


	21.5



	C20
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C20
	Mecoprop


	0.1 ug/l 
	June - 17

	0.0187
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	9.65 mg/l 
	June - 17

	0.561
	T686
	28th June


	10.6



	C21
	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C21
	Nickel


	0.22 ug/l


	June - 17

	4.56
	T301
	28th June


	8.82



	C21
	Chloride


	TBA


	June - 17

	5530
	T686
	28th June


	21.5



	C21
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C21
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	12.10 mg/l 
	June - 17

	4.04
	T686
	28th June


	10.6



	C22
	Cadmium


	1 ug/l 
	June - 17

	<0.1
	T301
	28th June


	7.83



	C22
	Nickel


	0.22 ug/l


	June - 17

	<5
	T301
	28th June


	8.82



	C22
	Chloride


	TBA


	June - 17

	8310
	T686
	28th June


	21.5



	C22
	MP Xylene


	1 ug/l 
	June - 17

	<0.2
	T54
	28th June


	

	C22
	Mecoprop


	0.1 ug/l 
	June - 17

	<0.005
	T16
	28th June


	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………Gareth Ffoulkes…………………………………….  

Date…………21/8/17……………..   



(Authorised to sign as representative of Operator)

