Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Carfiff

Installation:

Lamby Way Landfill Site

Form Number: 
…AUG17-L…
Reporting of ……LEACHATE…… monitoring for the period for … August 2017……..
	Monitoring

Point
	Substance /

Parameter
	Trigger level
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	L2
	Am Nitrogen
	1370 mg/l


	Aug - 17

	1150
	INORG-L12
	31st Aug 2017
	10.6



	L2
	Cadmium
	0.1 ug/l


	Aug - 17

	<2.00
	1450
	31st Aug 2017
	7.83



	L2
	Nickel
	0.1 ug/l


	Aug - 17

	262
	METALS-L
	31st Aug 2017
	8.82



	
	
	
	
	
	
	
	

	L2
	Chloride
	13713 ug/l
	Aug - 17

	1330
	INORG-L13
	31st Aug 2017
	21.5



	L2
	MP Xylene
	0.032 ug/l


	Aug - 17

	3.49
	1760
	31st Aug 2017
	

	
	
	
	
	
	
	
	

	
	MP Xylene


	
	
	
	
	
	

	L2
	Mecoprop
	0.024 ug/l

	Aug - 17

	40.3
	ORL-L17
	31st Aug 2017
	14.6



	
	
	
	
	
	
	
	


	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	L4
	Am Nitrogen


	1370 mg/l


	Aug - 17

	1140
	INORG-L12
	31st Aug 2017
	10.6



	L4
	Cadmium


	0.1 ug/l


	Aug - 17

	<2.00
	1450
	31st Aug 2017
	7.83



	L4
	Nickel


	0.1 ug/l


	Aug - 17

	261
	METALS-L
	31st Aug 2017
	8.82



	L4
	Chloride


	13713 mg/l 
	Aug - 17

	1300
	INORG-L13
	31st Aug 2017
	21.5



	L4
	MP Xylene


	0.029 ug/l 
	Aug - 17

	5.30
	1760
	31st Aug 2017
	

	L4
	Mecoprop


	0.032 ug/l


	Aug - 17

	43.8
	ORL-L17
	31st Aug 2017
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	L7
	Am Nitrogen


	1370 mg/l


	Aug - 17

	1140
	INORG-L12
	31st Aug 2017
	10.6



	L7
	Cadmium


	0.1 ug/l


	Aug - 17

	<2.00
	1450
	31st Aug 2017
	7.83



	L7
	Nickel


	0.1 ug/l


	Aug - 17

	260
	METALS-L
	31st Aug 2017
	8.82



	L7
	Chloride


	13713 mg/l 
	Aug - 17

	1310
	INORG-L13
	31st Aug 2017
	21.5



	L7
	MP Xylene


	0.029 ug/l 
	Aug - 17

	5.10
	1760
	31st Aug 2017
	

	L7
	Mecoprop


	0.032 ug/l


	Aug - 17

	43.8
	ORL-L17
	31st Aug 2017
	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………Gareth Ffoulkes……………………….  

Date………20/11/17………………..   



(Authorised to sign as representative of Operator)

