Permit Reference Number: DP3430LX



Operator: TRW Limited 

Installation: TRW Automotive




Form Number: S1

[image: image4.emf]Reporting of Emissions to Sewer for the period from …………01/07/14………………….to………31/12/14……………………

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/ Certification [4]
	Uncertainty

[5]

	S1
	Zinc
	5.0mg/l
	6.2
	WAS-049
	10/12/14 @ 10:55
	UKAS
	6.3 – 10.1 %

	S1
	Nickel
	2.0mg/l
	0.1
	WAS-049
	All readings
	UKAS
	7.1 – 8.9 %

	S1
	Chromium
	4.0mg/l
	0.1
	WAS-049
	All readings
	UKAS
	-

	S1
	Copper
	2.0mg/l
	0.1
	WAS-049
	All readings
	UKAS
	8 – 10.4 %

	S1
	pH
	6 – 11 [6]
	7.8 Max

7.2 Min
	WAS-049
	20/11/14 @ 13:44

28/08/14 @ 11:05
	UKAS
	-


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – The basis of any other uncertainty figure needs to be stated. Where no figure is available Natural Resources Wales will need to agree an appropriate uncertainty value. 

[6] The emission limit values for {pH} are expressed as minimum and maximum individual values.

Signed …………………………………………………………….  

Date………28/01/15………………..




(Authorised to sign as representative of TRW Limited)

Permit Reference Number: DP3430LX



Operator: TRW Limited 

Installation: TRW Automotive




Form Number: R1

Reporting of Waste Disposal and Recovery for the year ………2014…………………….

	Waste

Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes
	Tonnes
	
	Year
	Parameter

	
	
	
	
	
	
	Named 

Waste
	Total 

Waste

	1a) Hazardous Wastes - Solid
	Landfill
	27.825
	6.21

	
	2013
	644.28
	644.28

	1b) Hazardous Wastes - Liquids
	Chemical Treatment
	851.24
	
	
	2014
	885.275
	885.275

	2) Non-Hazardous Wastes
	
	
	
	
	2015
	
	

	
	
	
	
	
	
	
	

	TOTAL WASTE
	-
	879.065
	6.21
	
	
	
	


	Operator’s comments :




Signed …[image: image1.png]


…………………………………………….  

Date……28/01/15…………………..




(Authorised to sign as representative of TRW Limited)

Permit Reference Number: DP3430LX



Operator: TRW Limited 

Installation: TRW Automotive




Form Number: WU1

Reporting of Water Usage for the year ………2014…………………….
	Water Source
	Usage

(m3)
	Specific Usage 

(m3/t)
	
	Trends in Water Usage

	
	
	
	
	Year
	Parameter

	
	
	
	
	
	Named 

Water source
	Total 

Water usage

	Mains water
	46302
	
	
	
	
	

	
	
	
	
	2013
	Town’s Mains
	39385

	
	
	
	
	2014
	Town’s Mains
	46302

	TOTAL WATER USAGE
	46302
	
	
	2015
	
	


	Operator’s comments :

The increase in water usage in 2014 id due to the increased production on the newly installed Zinc Nickel Plating process



Signed …[image: image2.png]


…………………………………………….  

Date……28/01/15…………………..




(Authorised to sign as representative of TRW Limited)

Permit Reference Number: DP3430LX



Operator: TRW Limited 

Installation: TRW Automotive




Form Number: E1

Reporting of Energy Usage for the year ………2014……………………..

	Energy Source
	Energy Usage
	CO2
Produced

(tonnes)
	
	Trends in Energy Usage

	
	Quantity
	Primary Energy

(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy usage
	CO2

 produced

	
	
	
	
	
	
	
	

	
	
	
	
	
	2013
	4.938 MWh
	0.820 Tonnes

	Electricity *
	MWh
	8.17
	1.356
	
	2014
	9.57 MWh
	1.622 Tonnes

	Natural Gas
	tonnes
	1.4
	0.266
	
	2015
	
	

	Gas Oil
	tonnes
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	TOTAL
	-
	9.57
	1.622
	
	
	
	

	
	
	
	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4
	Operator’s comments :

The conversion factors used to calculate the Co2 produced were taken from the sector guidance H2 section 3.1 and were 190 for natural Gas and 166 for electricity.
Due to the fact that we have no direct measurement meters on the process plants themselves the Electrical figures are best estimates.
Increased usage figures due to the installation of the new Zn Ni process in 2014 which uses electric dryers as opposed to gas and increased production volumes.


Signed …………[image: image3.png]


………………………………………………….  

Date……28/01/15…………….
(Authorised to sign as representative of TRW Limited)

�








Date of form: 05/12/2013
Date of form: 05/12/2013
Date of form: 05/12/2013

