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Operator: 

Castle Waste Services Limited
Facility:

Roath Dock Transfer Station

Form Number: 
Sewer1 / 30/04/18
Reporting of emissions to sewer for the period from 01/01/2018 to 31/03/2018
	Emission

Point
	Substance /

Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	S1
	Effluent Flow m3/day


	No limit set 
	24-hour flow proportional sample


	78
	BS EN 135006
	22/03/2018
	N/A

	S1
	Zinc, as Zn mg/l
	No limit set
	daily average from composite sample taken over 24 hours
	1.781
	BS 6068-2.29:1987,

ISO 8288-1986
	19/02/2018
	+/- 0.610%

	S1
	Copper, as Cu mg/l
	No limit set
	daily average from composite sample taken over 24 hours
	1.248
	BS 6068-2.29:1987

ISO 8288-1986
	15/02/2018
	+/- 1.07%

	S1
	Lead, as Pb mg/l
	No limit set
	daily average from composite sample taken over 24 hours
	1.517
	BS 6068-2.29:1987


ISO 8288-1986

	22/03/2018
	+/- 8.62%

	S1
	Chromium, as Cr mg/l
	No limit set
	daily average from composite sample taken over 24 hours
	1.673
	BS EN 1233:1997,

BS 6068-2.38:1997
	06/01/2018
	+/- 7.61%

	S1
	Nickel, as Ni mg/l
	No limit set
	daily average from composite sample taken over 24 hours
	1.80
	BS 6068-2.29:1987

ISO 8288-1986
	23/01/2018
	+/- 3.26%


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Environment Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …M.Buffery……………………
Date……30/04/ 2018………..


(Authorised to sign as representative of Operator

