Permit Number: 	EPR/BV8024IW			Operator: 		Glanbia Cheese Limited

Facility:		Llangefni Dairy	                      Form Number: 	Sewer1 / 04/02/2022
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Chemical oxygen demand (mg/l)
	No limit set
	Spot sample comprising of a minimum of 4 composite samples taken in any 24 hour period
	
	BS 6068-2.34 or ISO 6060
	
	

	
	Total effluent flow
	No limit set
	Instantaneous (Continuous)
	
	Continuous flow meter
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	EPR/BV8024IW			Operator: 		Glanbia Cheese Limited

Facility:		Llangefni Dairy                             	Form Number: 	Water1 / 04/02/2022
Reporting of emissions to water for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W2
	Biochemical oxygen demand
	6 mg/l
	Instantaneous (spot sample)
	
	BS EN 1899-1
	
	

	
	Suspended solids
	30 mg/l
	Instantaneous (spot sample)
	
	BS EN 872
	
	

	
	Oil and grease
	10 mg/l
	Instantaneous (spot sample)
	
	SCA, the determination of hydrocarbon oils in waters by solvent extraction IR absorption and gravimetry
	
	

	
	pH 
	6-9
	Instantaneous (spot sample)
	
	SCA, the measurement of electric conductivity and the determination of pH
	
	

	
	Bromine 
	Not detectable
	Instantaneous (spot sample)
	
	SCA Blue Book 218
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
