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1.
 INTRODUCTION, SITE, LICENCE & WORKING PLAN

1.1
Site Location
The site is located off the roundabout for the A474/A48 in Briton Ferry Neath
1.2
Site Development

The Briton Ferry HWRC and Transfer Station have been designed to provide a public waste disposal centre for Neath & Port Talbot residents.  

This Working Plan is aimed towards the facilities which will be supplied by the current site operations, however, as the development progresses this working plan will be updated to accommodate any changes over those specified here.

1.3
Site Permit
The site permit area comprises the site entrance, vehicle parking and movement area and storage bays/areas for keeping waste.

The weighbridge is used for trade waste inputs and all waste exports is located within the Transfer Station
1.4
Working Plan


The working plan is a comprehensive document to detail the principles, infrastructure, operational activities, methods and environmental controls for the site.  It contains guidelines and procedures for the site management and operatives to ensure that the site is run in a safe and effective manner in accordance with a Quality Management System.


The Working Plan incorporates detail required for the issue and regulation of a Waste Management Licence issued by Natural Resources Wales (NRW) to prevent harm to human health, pollution of the environment and avoid serious detriment to local amenity.  It is designed to offer flexibility of operation whilst the above objectives are met.

1.5
Changes to the Working Plan

The site operational procedures will be under constant review and the Working Plan will be amended in agreement or with the prior knowledge of the NRW.  Any proposed changes will be issued in draft form for consultation, comments and agreement before final issue.  

 
Up to date copies of the Working Plan will be located at the Briton Ferry site office.

2.
SPECIFIED WASTE MANAGEMENT OPERATIONS

The types of waste management operations that can be carried out on site are detailed in Table 1.1 of the Waste Management licence and for ease of reference are summarised in Table 2.1 below.

	Table 2.1  Specified Waste Management Operations

	Specified Waste Management Operation reference
	Specified Waste Management Operation summary
	Permitted Waste Types
	Limits

	D13 
	Blending or mixing of wastes prior to storage. This does not apply to the mixing of wastes to achieve a more dilute waste in order to come under a threshold.
	All solid non-hazardous wastes as listed in Appendix A to the licence.
	 

	D15 
	Storage of waste pending disposal and another licensed facility.
	All waste types listed in Appendix A to Licence
	

	R13
	Storage of waste pending recycling / recovery at another licensed facility.
	All waste types listed in Appendix A to Licence
	

	D9
	Physio-chemical treatment of waste.
	All solid non-haz wastes in Appendix A
	 

	R2
	Recycling or reclamation of organic substances.
	
	

	R3
	Recycling or reclamation of metals
	
	

	R4
	Recycling or reclamation of in organic solvents
	
	


3.
PERMITTED WASTE TYPES AND QUANTITIES

The site will accept household only in the HWRC, household, commercial and industrial wastes at the Transfer Station
 The annual tonnage of waste permitted at the site is <25,000 tonnes.

Of the above categories only specific waste types are permitted by the Permit
3.1
Waste Acceptance List

	European Waste Catalogue Number
	Maximum Permitted Quantities

Annual: 25,000 tonnes

	03
	Wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing, food preparation and processing

	03 01
	Wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing
	

	03 01 01
	waste bark and cork
	

	03 01 05
	waste bark and cork sawdust, shavings, cuttings, wood, particle board and veneer other than those mentioned in 03 01 04
	

	13
	Oil wastes and wastes of liquid fuels (except edible oils, and those in chapters 05,12 & 19)

	13 02
	Waste engine, gear and lubricating oils
	 

	13 02 04*
	mineral-based chlorinated engine, gear and lubricating oils
	

	13 02 05*
	mineral-based non-chlorinated engine, gear and lubricating oils
	

	13 02 06*
	synthetic engine, gear and lubricating oils
	

	13 02 08*
	other engine, gear and lubricating oils
	

	15
	Waste packaging; absorbents, wiping cloths, filter materials and protective clothing not otherwise listed

	15 01
	Packaging (including separately collected municipal packaging waste)
	

	15 01 01
	Paper and cardboard packaging
	

	15 01 02
	Plastic packaging
	

	15 01 03
	Wooden packaging
	

	15 01 04
	Metallic packaging
	

	15 01 05
	Composite packaging
	

	15 01 06
	Mixed packaging
	

	15 01 07
	Glass packaging
	

	15 01 09
	Textile packaging
	

	16
	Wastes not otherwise specified in the list

	16 01
	End-of-life vehicles from different means of transport (including off-road machinery) and wastes from
	

	16 01 03
	End-of-life tyres
	

	16 01 07*
	oil filters
	

	16 02
	Wastes from electrical and electronic equipment
	

	16 02 11*
	Discarded equipment containing chlorofluorocarbons, HCFC, HFC
	

	16 02 16
	Components removed from the discarded equipment other than those mentioned in 16 02 15 (16 02 15; hazardous components removed from discarded equipment)
	

	16 06
	Batteries and accumulators
	

	16 06 01*
	Lead batteries
	

	16 06 02*
	Ni-Cd batteries
	

	16 06 04
	Alkaline batteries (except 16 06 03* mercury containing batteries)
	

	16 06 05
	Other batteries and accumulators
	

	17
	Construction And Demolition Wastes (Including Excavated Soil From Contaminated Sites)

	17 01
	Concrete, bricks, tiles and ceramics
	 

	17 01 01
	Concrete
	

	17 01 02
	Bricks
	

	17 01 03
	Tiles and ceramics
	

	17 01 07
	Mixtures of concrete, bricks, tiles and ceramics other than those mentioned in 17 01 06*  (17 01 06* = mixtures of, or separate fraction of concrete, bricks, tiles, and ceramics containing dangerous substances)
	

	17 02
	Wood, glass and plastic
	

	17 02 01
	Wood
	

	17 02 02
	Glass
	

	17 02 03
	Plastic
	

	17 04
	Metals (including their alloys)
	

	17 04 01
	Copper, bronze, brass
	

	17 04 02
	Aluminium
	

	17 04 03
	Lead
	

	17 04 04
	Zinc 
	

	17 04 05
	Iron and steel
	

	17 04 06
	Tin
	

	17 04 07
	Mixed metals
	

	17 04 11
	Cables other than those mentioned in 17 04 10*  (17 04 10* = cable containing oil, coal tar and other dangerous substances)
	

	17 05
	Soil (including excavated soil from contaminated sites), stones and dredging spoil
	

	17 05 04
	Soil and stones other than those mentioned in

17 05 03*
	

	17 06
	Insulation materials and asbestos-containing construction materials
	

	17 06 01*
	Insulation materials containing asbestos
	

	17 06 03*
	Other insulation materials consisting of or containing dangerous substances
	

	17 06 04
	Insulation materials other than those mentioned in 17 06 01* (insulation materials containing asbestos) and 17 06 03* (other insulation materials consisting of or containing dangerous substances)
	

	17 06 05*
	Construction materials containing asbestos
	

	17 08
	Gypsum based construction material
	

	17 08 02
	Gypsum-based construction materials other than those mentioned in 17 06 03* ( 17 08 01* = gypsum-based construction materials contaminated with dangerous substances)
	

	17 09 04
	Mixed construction and demolition wastes other than those mentioned in 17 09 01, 7 09 02* and 17 09 03*
	

	19
	Wastes From Waste Management Facilities, Off-Site Waste Water Treatment Plants And Preparation Of Water Intended For Human Consumption / Industrial Use

	19 12
	Wastes from the mechanical treatment of waste (for example sorting, crushing, compacting)
	

	19 12 01
	Paper and cardboard
	

	19 12 02
	Ferrous metal
	

	19 12 03
	Non-ferrous metal
	

	19 12 04
	Plastic and rubber
	

	19 12 05
	Glass
	

	19 12 07
	wood other than that mentioned in 19 12 06* (19 12 06* = wood containing dangerous substances)
	

	19 12 08
	Textiles
	

	19 12 09
	Minerals (for example sand, stones)
	

	19 12 12
	Other wastes (including mixtures of materials) from mechanical treatment of wastes other than those mentioned in 19 12 11* (19 12 11* = other wastes (including mixtures of materials) from mechanical treatment of waste containing dangerous substances)
	

	20
	Municipal Wastes (Household Waste And Similar Commercial, Industrial And Institutional Wastes)

	20 01
	Separately collected fractions (except 15 01)
	 .

	20 01 01
	Paper and cardboard
	

	20 01 02
	Glass
	

	20 01 10
	Clothes
	

	20 01 11
	Textiles
	

	20 01 13*
	Solvents
	

	20 01 19*
	pesticides
	

	20 01 21*
	Fluorescent tubes
	

	20 01 23*
	Discarded equipment containing chlorofluorocarbons 
	

	20 01 25
	Edible oils and fat
	

	20 01 27*
	Paint, inks, adhesives, and resins containing dangerous substances
	

	20 01 28
	Paints, inks, adhesives and resins other than those mentioned in 20 01 27*
	

	20 01 33*
	Batteries and accumulators included in 

16 06 01,  16 06 02 or 16 06 03 and unsorted batteries and batteries and accumulators containing these batteries
	

	20 01 34
	Batteries and accumulators
	

	20 01 35*
	Discarded electrical and electronic equipment other than those mentioned in 20 01 21* and 20 01 23* containing hazardous components
	

	20 01 36
	Discarded electrical and electronic equipment 
	

	20 01 37*
	Wood containing dangerous substances
	

	20 01 38
	Wood other than that mentioned in 20 01 37*
	

	20 01 39
	Batteries and accumulators plastics other than those mentioned in 20 01 33*
	

	20 01 40
	Metals
	

	20 02 
	Garden and park waste (including cemetery waste)
	

	20 02 01
	Biodegradable waste
	

	20 02 02
	Soil and stones
	

	20 02 03
	Other non-biodegradable wastes
	

	20 03
	Other municipal wastes
	

	20 03 01
	Mixed municipal waste
	

	20 03 02
	Waste from markets
	

	20 03 03
	Street-cleaning residues
	

	20 03 07
	Bulky waste
	


3.2
Waste Acceptance in Emergencies

Other waste not included in Waste Acceptance List shall only be accepted at the site with the permission of NRW.  Such requests are likely to be in the case of emergencies where a more suitable Waste Management Facility is not open to receive that waste.

All waste received in an ‘emergency’ will be assessed for it’s compatibility with other wastes on site, its risk to the environment and human health and shall be stored in a position and container (if required to be sealed) suitable to the risk posed.


Details of the type of waste, the list of risks shall be written into the site diary.  The diary will also contain the resultant storage container type (if applicable) and the place where the waste is stored.  The time that the waste is stored on site will be recorded in the site diary.

At all times no incompatible wastes will be accepted at the site, which in combination with other materials could give rise to harm or pollution to those outside the site.

4.0
Hours of Operation

The site will operate within the following hours of operation 
HWRC :-

            Operational hours
7 Days per week
08:30 to 17:00

Christmas day

Closed

Boxing day
Closed


New Years day
Closed

            Transfer station :-        Monday to Friday         07:30 to 16:30





Saturday & Sunday
07:30 to 12:30
                                                  Christmas day

Closed
Emergency waste operations will take place outside the specified hours with prior permission of NRW (24 hours) and the Local Authority if contactable in advance (standard office hours).

5.
SITE INFRASTRUCTURE


The layout of the site is shown in the Site Layout Drg
5.1
Site Security
The site perimeter and gates are constructed of steel palisade fencing and in addition the access and egress road that operates on a one-way system is enclosed by steel palisade fencing and gates. FCC vehicles go against the flow of traffic to access containers, whilst this is done there is a SWP in place 

The Permit area security will be visually checked once per day, formally inspected once per week within the weekly inspection schedule and repaired as necessary to ensure security is maintained.

CCTV is in operation 24hrs a day and the site is manned by a security company out of hours
5.2
Site Signs
Full details required by the site licence are displayed at the entrance. The Site Waste Management sign will include Permit numbers, site name, address and telephone number, emergency contact numbers, head office address and telephone numbers, hours of opening and the name, address and telephone number of NRW
Further signage indicating the storage areas for waste types will be displayed, where it is deemed appropriate to assist in ensuring the correct waste type is stored or deposited there.  Some waste bays may be flexible with regards to the waste type stored and therefore signage will be movable.  

5.3
Access

The site is accessed via a dedicated entrance off the main road.  All visitors are required to sign in at the site office.


A visitor's book, site diary and accident book will be located in the site office.  The logbook will be used to record any significant event, weather conditions, visits by NRW personnel, engineering dates and any other important information.

5.4
Storage

Diesel fuel stored in a bunded tank.
5.5
Weighbridge

There is one Weighbridge provided, which is located in the Transfer Station Permitted area.  The two sites are operated by FCC Environment under the same permit number and the weighbridge and office facilities are shared.

The weighbridge(s) is calibrated and will be inspected for compliance with weights and measures when required.  A maintenance contractor will certify the inspection and any necessary repair.

The weighbridge is linked to the computer system, which accurately records weights of the vehicles, and calculates and records all waste outputs from the site.   The computer is linked by modem to Head Office where all waste records and statistics are generated.
6.0
SITE ENGINEERING AND DRAINAGE SYSTEM

6.1
Engineering Specification – Impermeable Surface

The site is constructed of hard wearing impermeable base for the effective keeping and mechanical movement of waste.  

The site construction means that all waste containers identified for are deposited, sorted, stored and loaded on an impermeable concrete pavement.  
The specification of the impermeable surface will be retained.  All major repair work to the engineered impermeable surface will be carried out to the same or higher specification.  Details of any higher specification work will be stored with a map showing the areas laid to this specification.  The qualifications and experience of the contractor carrying out the work will be recorded and submitted to NRW.
6.2
Engineered Specification - Drainage

All the drainage from the site is collected via drains and passed through a bypass separator and then discharged to public sewer
7.
SITE MANAGEMENT and OPERATIONAL PROCEDURES

In additional to this Working Plan, the site Management and Operatives are given operational instructions by the company health and safety manual, and specific written instructions issued separately. 


Updates in training will be as necessary or when the waste management licence or site working plan brings a change to the duties or expectations of personnel.

7.1

Technically Competent Management
The site requires a Technically Competent Management (TCM) with a minimum Certificate of Technical Competence of TS4.

	Table 7.1  Technically Competent Management

	Name
	COTC level
	Date assigned to TCM

	Darren Hemming
	4MTSH
	07/11/2016

	 
	 
	 

	
	
	


7.2
Operations Staff

A minimum of four personnel will be on site at all times during working hours  to assist with the deposits of waste, inspecting waste to ensure compliance with licence conditions, ensuring waste is deposited in the correct locations and responding to queries.


Additional persons will be brought to the site as necessary to assist during busier time, plant maintenance, personnel training, compliance audits, and any other duties necessary to ensure health and safety and environmental protection.

7.3
Staff Training

The FCC Environment Training Procedures, in accordance with the Environmental Management System will be followed.  All staff will receive adequate instruction and training to effectively and efficiently carry out their job function.  Personnel will receive any necessary formal training with outside agencies, which will be documented.  In-house training will be given and documented, in all aspects of operational procedures, site licence requirements in relation to operations and the environment, health and safety and general requirements of the working plan.  Training will take place in head-office, on site and on similar sites within the Group, with specific computer and record-keeping instruction given to all weighbridge personnel.  The Group Training Manager is responsible for ensuring training for health and safety purposes and achieving the WAMITAB qualification.  The Technically Competent Manager is responsible for giving induction training and instruction.

8.0
INCOMING AND OUTGOING WASTES AND WASTE RECORDING
8.1
Health and Safety Instruction


All trade vehicles entering the site must stop on the weighbridge and report to the operator.  First time trade visitors to the site are asked to read the displayed notice giving instructions on health and safety and site procedures.  Visitors other than customers/public bringing waste to the site must sign the Visitors Book before proceeding onto the site, and sign out prior to leaving.

8.2
Duty of Care 

8.2.1
Trade waste


Trade customers must wait on the weighbridge to have the gross weight of the vehicle recorded on the computerised system.  The driver of the vehicle must provide a document detailing the source location and description of the waste they are carrying for Duty of Care purposes.  These details are recorded on the computer system along with the vehicle registration number.  Annual duty of care notes are provided by some customers for inputs where the producer, description of waste, approximate quantity and carrier does not vary.  A copy of these notes is held at the weighbridge office and Head Office.
8.2.2
Household waste


The Public binging in ‘household’ waste are not required to produce a waste transfer note in accordance the Duty of Care requirements.  However when the waste is transferred out the site, the transfer will need to comply with the Duty of Care Regulations as in 8.2.1 above.

8.3
Carrier Registration
8.3.1
Trade waste

The operator of the weighbridge will check that the trade customer is a Registered Waste Carrier by referring to the detail on the computer system maintained by Head Office.  If the customer details on the computer show there not to be a valid carriers registration the customer will be asked for proof of registration in the form of a validated Carriers Certificate.


If the customer is not a Registered Waste Carrier the customer will be advised that on the first occasion the waste will be accepted into the site but that the customer should then contact the NRW to ensure registration before attempting to enter the site again.


The only exemptions to this are local authorities and customers carrying their own wastes (if not construction and demolition material).  The Compliance Manager should be contacted if any clarification is needed.
8.3.2
Household waste


The Public binging in ‘household’ waste is not required to be a registered waste carrier if carrying/transporting their own ‘household’ waste.

8.4
Waste Acceptance and Rejection

8.4.1
Trade waste


The site operatives will question the trade waste driver if unsure about the waste description to ensure it complies with the requirements of the waste management licence for the site.  A visual check, whenever possible, will be made to ensure an adequate description has been provided.

If the waste is acceptable in accordance with the Waste Acceptance and Rejection Procedure, the customer will be directed to the tipping area or the relevant recycling area as indicated in the Site Layout Drawing.  


If either the waste description or the content of the incoming load is not satisfactory the load will be checked thoroughly and a decision will be made on its acceptability, if necessary requesting help from the Area Manager, Operations Director or the Compliance Manager.


If the waste is not acceptable under the terms of the waste management licence, entry to the site will be refused and the registration number of the vehicle recorded separately in the site diary.  The technically competent manager or Compliance Manager will be informed.


8.4.2
Household waste


The Public can bring all ‘household’ waste to the site 


The site operatives must be available to manage the delivery of household waste in order to ensure it is placed in the correct areas and that any possibly non-compatible or unidentifiable wastes can be identified early, especially by the person delivering the waste.  If the operative is uncertain of the nature of a ‘household’ waste it must be isolated away from other wastes, labelled as ‘isolated’ and identification of it sought through the Technically Competent Manager and the Group resources.  A suitable place for disposal/recycling can be identified.

8.5
Outgoing Vehicles


8.5.1
Trade waste
              All vehicles removing waste materials shall comply with the Duty Of Care Regulations (Section 34 of the Waste Management Licensing Regulations 1994). 


Outgoing vehicles must stop at the weighbridge before leaving the site.  A duty of care transfer note will be issued and signed showing waste type and vehicle destination.  The driver must also sign the note to agree the transfer.  A copy of this is issued to the driver and a copy is held on site.

In the event of Computer/Weighbridge failure notes will be issued manually.


All outgoing vehicles carrying bulk waste materials or materials destined for recycling re-processors will be sheeted before leaving the site.


All weighbridge records are collated at Head Office to ascertain waste inputs by weight and type on a monthly basis.


8.5.2
Household waste


The Public will not take waste out of the site unless it is identified as unacceptable or a more suitable method of disposal/recycling has been advised under section 8.4.  No Duty of Care requirements are applicable.
8.6
Waste Records
NRW require a summary of waste received and removed (tonnage, type and district of origin) at the end of every quarter year.  The information will be sent to NRW on the standard Waste Return format and will be completed by the Site Manager/Admin
Records referring to the Duty of Care for waste (delivered and removed waste) will be kept for a minimum of 2 years.

All data will be kept either in electronic form with back ups or in paper format.

9.0
Processes: Waste Storage and Handling.
9.1
Waste Storage

Wastes will be stored according to the Site Layout. 

The storage of waste materials in dedicated bins/containers will not exceed the full capacity of the bin/container.


All wastes will be handled in accordance with this section.  
            9.1.1   Treatment of black bag waste.
            Domestic household black bag waste to be treated will be taken to the dedicated treatment area. The treatment will take place on the sites existing impermeable site drainage system within the sites waste storage area.

            A workstation, suitable for two staff, will be used for hand sorting of the waste only with recyclable items being placed into dedicated wheelie bins.  The bins will be moved when full and placed into the existing containers for these recyclable materials.  The site will have 3 wheelie bins for recyclable materials next to the workstation and a 4th bin will be used for the non-recycle waste remaining, which will be moved to the appropriate container on site when full.

            Any materials found requiring special handling such as “needles” or “household chemicals” will be placed within clinical boxes and/or chemsafe where necessary.

            The working area will be cleared of any loose waste or litter at the end of the working day

            Only suitable and selected black bag waste will be treated, with up to 100 bags a day going through the process.  The treatment operations will only take place under suitable weather conditions to ensure there is no excessive windblown litter or where the recycling materials could be adversely affected.

            Safe working procedures are in place with appropriate PPE being used for the hand sorting process.


9.1.2
Acceptable, compatible and identifiable waste

Wastes will be inspected by the Site Operative for compliance with Site Permit.  Site Operatives will assist the public in identifying the correct waste disposal area and will ensure that trade waste depositors are directed to the correct area from the weighbridge.

General waste not identified for separate collection will be collected in open top containers and some compaction will be applied to the waste.  

Items identified for separate collections are provided with suitable storage containers or areas, such as bottle banks for glass, paper containers for paper etc.


All open top containers will be sheeted before leaving the site, except for those transporting waste directly to the adjacent site via the weighbridge.

 9.1.3
Non-acceptable, non-compatible & non-identifiable waste

This section details issues that may arise from non-acceptable, non-compatible waste considered dangerous for one reason or more reasons.

Trade wastes that are considered ‘dangerous’ on their own or in combination with other waste are not acceptable at the site.  Not with standing this, the Technically Competent Manager and site operatives will be aware of the procedure for handling substances considered dangerous to handle.

Household wastes that are considered ‘dangerous’ on their own or in combination with other waste are to be treated in accordance with the Procedure for the Control of Dangerous Substances. 

All trade non-acceptable wastes will be rejected and directed to a suitable waste management facility in the vicinity.  However substances identified on site, once delivered will be isolated and stored in a suitable container or area.  The risk the waste causes will be identified and appropriate action taken.

All household non-compatible and non-identifiable wastes will be isolated and stored in a suitable container or area.  The risk the waste causes will be identified and appropriate action taken. 

A chemical giving off fumes will require the site to be evacuated, whilst a contained substance will require isolation prior to removal off site.

On identification of a non-acceptable waste that is considered to be ‘dangerous’, NRW will be notified immediately or as soon as practical, which shall not be later than the end of the working day.  Other Agencies will be notified if required, in accordance with the FCC Safety, Health and Environmental System.


9.1.4 Accidental Leaks and Spillages of Waste

The site will accept some wastes which may contain potentially polluting or harmful liquids, sludges or powders.  Should any accidental leaks occur they will be treated in the following manner:-

· Any further leaks or spillages will be prevented from occurring;
· All reasonable endeavours will be made to prevent harmful liquids, sludges or powders from entering any surface water drainage system, by the application of absorbent granules or immediate sweeping.  Contaminated granules and sweepings will be placed in an appropriate container and disposed of at a suitably licensed facility as soon as is reasonably practicable.

· Waste types comprising of substances that have the potential to leak, such as acid- 
containing batteries, will be stored appropriately:

· Batteries will be stored undercover or within a container which is impermeable to the 
battery contents and which is able to withhold 110% of the capacity of the volume of 
the batteries contained therein.  Batteries will be stored away from any surface water 
drains and on a concreted area with a sealed drainage system.  If used, the storage 
container will be fitted with a cover which should be replaced each time the 
container is used, so as to prevent rainwater ingress.  

· All asbestos arriving at the site will be stored within a purpose designed lockable 
skip      and will be within a sealed drainage system.  

· Fluorescent tubes will be stored within an impermeable, covered, labelled container, 
located away from any surface water drains and on a concreted area with a sealed 
drainage system  
· Gas bottles will be stored securely in an upright position within a lockable cage 
which will be located away from buildings and positioned to avoid accidental impact 
from moving plant or vehicles.  The gas bottles cage will be stored away from 
potential sources of heat, potentially flammable waste types and the quarantine area. 
Gas bottled will be stored away from any surface water drains and on an 
impermeable surface with a sealed drainage system.  

· It is the Site Supervisor’s responsibility to ensure that either or both the shut off 
valves on the two drainage systems are closed in the event of an accidental spillage, 
when deemed necessary.

· Should any harmful liquid, sludge or powder enter the interceptor, it is the Site 
Supervisors responsibility to ensure that the outlet valve on the interceptor unit is 
closed and provision is made for the interceptors contents to be pumped out and 
removed from site to a suitably licensed facility as soon as is reasonably practicable.

· Spilt material will be removed and all areas that are affected by any spillage, 
including plant and machinery as soon as is reasonably practicable.

10.
ENVIRONMENTAL CONTROLS

10.1
Environmental Risk Assessment
A risk assessment on the environmental impacts of each stage in the Waste Disposal and Recycling Centre operations has been completed in order to identify the control measures needed to manage the site with regards to the environment.  The risk assessment is detailed in 
IMS File 3
The risk assessment has identified the requirement to control environmental impacts, for example, dust and odour.  In assessing the potential of each environmental impact to have an effect the following summary of receptors has been considered.
	Key receptor
	Direction
	Distance from facility boundary (metres)

	Industrial
	SW
	100 metres

	Residential 
	NW/NE
	100 Metres

	M4
	N
	100 Metres

	A48
	S
	100 Meters


11.0
Control of Environmental Impacts

11.1
Dust Control


The site surface is fully concreted which serves to keep dust generation to a minimum.  The site surface will be regularly swept to prevent dust build up.  


Site roads, and other areas, will be damped down using a hose if necessary.  Any operation or activity generating dust in excess of that being capable of control using the control systems will be stopped.


A daily visual inspection of the site be carried out by the site operatives and all inspections and actions will be recorded in the site diary.

11.2
Litter Control


The site is surrounded by fencing that will serve to collect windblown litter, however, should litter be blown off site, the site operatives will organise its collection and take action on site to prevent of further litter escape.  In the event of severe litter blow, litter pickers will be employed or hired in as necessary to keep the site and its surrounds tidy.  Priority will be given to off-site areas with the tidiness of the site attended to once those are clear.


Bulk vehicles will sheet up before leaving the site.

11.3
Noise Control

The impact of reverse bleepers has been identified as a potential source of noise and will be monitored for impact outside the site when operations are undertaken by FCC.
Monitoring of noise levels will be carried out.

11.4
Odour Control


Strong odours are unlikely to be generated at such a facility during normal operations.  Nevertheless any incoming wastes generating strong odour will be loaded into the first available bulk lorry departing the site as specified.
            There are odour checks done twice daily and recorded on the daily site check sheet.
11.5
Pests


A contract has been set up with a pest control company who inspect the site on a regular basis.  Records of visits and any action taken are held in the site office.  This contract will be maintained.

The rapid turnaround of general wastes at the site means that the risk of pest development - mainly flies and other insects - on site are minimised.  There is however a risk that customers may inadvertently bring loads of wastes into the site with flies, wasps and other insect pests already developed.  In this event the waste load will be treated with insecticide.  The customer will be informed of the need to carry out such treatment at the site of production to ensure that future loads do not give rise to similar problems.


Birds are unlikely to be attracted to the site due to the continual use of the site. 

11.6
Mud


The hard surface of the whole of the site means the ability to generate mud is minimal.  There is a possibility of debris being picked up on vehicle wheels from the tipping areas.  To minimise this the areas will be kept clean by sweeping.  


All bulk lorries collecting waste for onward recycling or disposal will be sheeted or netted before leaving the site. This will ensure that no debris is deposited on site or outside the site.  In the event of any deposition, site surfaces and outside highway will be cleaned or picked immediately.  


Vehicles will be visually inspected by site staff before they leave the site and advice given to drivers if there is a need to clean mud or debris before leaving. 

11.7
Spillages

Spillage's of liquid will be dealt with by use of appropriate absorbent materials.  A supply of absorbent granules is kept dry and available on site.  The residual waste may be stored on site before being loaded directly to a bulk container pending off-site disposal to a suitably licensed site.


In the event of any spillage of a major pollutant (most notably of oils and fuel) anywhere in the Waste Management Licensed area, the spillage will then be soaked up using the granules and disposed to a suitably licensed site.
The site will accept some potentially polluting hazardous wastes.  Should any accidental leaks occur they will be treated in the following manner:-

· Any further leaks or spillages will be prevented from occurring;
· All reasonable endeavours will be made to prevent harmful liquids, sludges or powders from entering any surface water drainage system, by the application of absorbent granules or immediate sweeping.  Contaminated granules and sweepings will be placed in an appropriate container and disposed of at a suitably licensed facility as soon as is reasonably practicable.

· Waste types comprising of substances that have the potential to leak, such as acid- 
containing batteries, will be stored appropriately:

· Batteries will be stored undercover or within a container which is impermeable to the 
battery contents and which is able to withhold 110% of the capacity of the volume of 
the batteries contained therein.  Batteries will be stored away from any surface water 
drains and on a concreted area with a sealed drainage system.  If used, the storage 
container will be fitted with a cover which should be replaced each time the 
container is used, so as to prevent rainwater ingress.  

· All asbestos arriving at the site will be stored within a purpose designed lockable 
skip located on the southern edge of the concreted hard standing to the south east of 
the waste transfer building   The waste be within a sealed drainage system
· Fluorescent tubes will be stored within an impermeable, covered, labelled container, 
located away from any surface water drains and on a concreted area with a sealed   

                         drainage system.
· Gas bottles will be stored securely in an upright position within a lockable cage 
which will be located away from buildings and positioned to avoid accidental impact 
from moving plant or vehicles.  The gas bottles cage will be stored away from 
potential sources of heat, potentially flammable waste types and the quarantine area. 
Gas bottled will be stored away from any surface water drains and on an 
impermeable surface with a sealed drainage system.  

· It is the Site Supervisor’s responsibility to ensure that either or both the shut off 
valves on the two drainage systems are closed in the event of an accidental spillage, 
when deemed necessary.

· Should any harmful liquid, sludge or powder enter the interceptor, it is the Site 
Supervisors responsibility to ensure that the outlet valve on the interceptor unit is 
closed and provision is made for the interceptors contents to be pumped out and 
removed from site to a suitably licensed facility as soon as is reasonably practicable.

· Spilt material will be removed and all areas that are affected by any spillage, 
including plant and machinery as soon as is reasonably practicable.

11.8
Fire

 
A work instruction and fire emergency plan is drawn up and displayed in the office for operators to be aware of in case of outbreak of fire.  

The risk of fire is minimised by the division of waste materials on site and the no smoking policy.  Part of the waste checks is to ensure that all incoming wastes will be inspected on deposit to check for burning, smouldering or smoking wastes.


In the event of a small fire, fire extinguishers are located in the weighbridge office.  


The fire equipment will be visually checked on a weekly basis to ensure readiness for use.  An annual certification check will be carried out and recorded by an external professional on all fire equipment to ensure full compliance with fire requirements.


Advice to all operatives on fire procedures will be recorded on the Induction Training Checklist and Record.  At least twice per year a fire drill will be carried out under the direction of the Technically Competent Manager.  This will ensure all site staff are aware of the procedures, and of locations and methods of use of fire equipment. Records of these events will be kept in the site diary.  Any improvements needed to procedures, equipment or training will be reported at the next Operations Meeting.  


Any residues from a fire will be first checked to see if completely extinguished.  They will then be loaded into bulk collection vehicles for onward disposal at a suitably licensed landfill site.
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