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Notice of variation and consolidation with introductory note
The Environmental Permitting (England & Wales) Regulations 2016	

Dŵr Cymru Cyfyngedig

Storm Overflow at The Llandarcy 36” Outfall
Side of Bridge House
Pen-Y-Heol (B4290)
Llandarcy
Neath
SA10 6LQ

Variation application number
PAN-017074
Permit number
BP0064319	




	





Storm Overflow at The Llandarcy 36” Outfall
Permit Number BP0064319
Introductory note
This introductory note does not form a part of the permit
The following notice gives notice of the variation and consolidation of an environmental permit.

This variation removes the sewage pumping station activity from the permit. This activity was incorrectly labelled Activity 3 on the previous permit. The sewage pumping station is at another site and is regulated under BP0255601 (Dynevor PS CSO & EO). 

The permit has been varied to include event duration monitoring as part of the AMP environmental improvement programme.

The schedules specify the changes made to the permit.

The status log of the permit sets out the permitting history, including any changes to the permit reference number. It is not backdated before 6 April 2010.

	Status Log of the permit

	Detail
	Date
	Comments

	Application BP0064319/V002
(variation and consolidation)
	Duly made
06/08/2014
	Application to vary and update the permit to modern conditions and remove 1, 2, Dichloroethane.

	Variation Issued
BP0064319 
	16/12/2015
	Varied and consolidated permit issued in modern condition format.

	Variation Issued
BP0064319
	01/04/2018
	Admin variation to amend error on oil & grease and to correct NGRs.

	Regulator-initiated variation
Application PAN-017074
	Duly Made
01/05/2020
	AMP programme EDM variation and removal of pumping station activity.

	Variation Issued
BP0064319
	09/03/2022
	Varied permit issued to Dŵr Cymru Cyfyngedig.



End of Introductory Note

	[bookmark: _Toc77056945]
Notice of variation and consolidation 


The Environmental Permitting (England and Wales) Regulations 2016
[bookmark: _Hlt13295849]
The Natural Resources Body for Wales (“Natural Resources Wales”) in exercise of its powers under regulation 20 of the Environmental Permitting (England and Wales) Regulations 2016 varies and consolidates

Permit number
BP0064319

[bookmark: _Hlk13917238]Issued to
Dŵr Cymru Cyfyngedig (“the operator”)

[bookmark: InstallationAddress21]whose registered office is
[bookmark: _Hlk72241007]Linea 
Fortran Road 
St Mellons 
Cardiff 
CF3 0LT

company registration number 02366777

to operate a water discharge activity at
Storm Overflow at The Llandarcy 36” Outfall
Side of Bridge House
Pen-Y-Heol (B4290)
Llandarcy
Neath
SA10 6LQ

to the extent set out in the schedules.

The notice shall take effect from 09/03/2022.

	Name
	Date

	Emma Jones
	09/03/2022



Authorised on behalf of Natural Resources Wales

Schedule 1
All the conditions have been varied as a result of a regulator-initiated variation.

Schedule 2 – consolidated permit


Consolidated permit issued as a separate document. 
Variation application:
PAN-017074	Page iv
	
Permit


The Environmental Permitting (England and Wales) Regulations 2016

Permit number
BP0064319

This is the consolidated permit referred to in the variation and consolidation notice for application PAN-017074 authorising

Dŵr Cymru Cyfyngedig (“the operator”)

whose registered office is
Linea 
Fortran Road 
St Mellons 
Cardiff 
CF3 0LT

company registration number 02366777

to operate a water discharge activity at
Storm Overflow at The Llandarcy 36” Outfall
Side of Bridge House
Pen-Y-Heol (B4290)
Llandarcy
Neath
SA10 6LQ

to the extent authorised by and subject to the conditions of this permit.

	Name
	Date

	Emma Jones
	09/03/2022


Authorised on behalf of Natural Resources Wales


Conditions
Management
0. [bookmark: _Ref373938749]General management
[bookmark: _Ref373938830]The operator shall manage and operate the activity:
in accordance with a written management system that identifies and minimises risks of pollution so far as is reasonably practicable, including those risks arising from operations, maintenance, accidents, incidents, non-conformances and those drawn to the attention of the operator as a result of complaints; and
using sufficient competent persons and resources.
Records demonstrating compliance with condition 1.1.1 shall be maintained. 
1.1.3   Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of the permit.
Operations
Permitted activities
2.1.1   The only activity authorised by the permit is the activity specified in schedule 1 table S1.1.
The site 
The discharge activity shall take place at the discharge point marked on the site plan at schedule 7 to this permit, and as listed in table S3.2.
Operating techniques
For the discharge specified in table S3.3:
The discharge shall only occur when and only for as long as either:
(i)  the flow passed forward is equal to or greater than the overflow setting indicated due to rainfall and/or snow melt or
                                  (ii)  the hydraulic capacity of the sewer network downstream of the combined sewer overflow is reached due to rainfall and/or snow melt and the level of storm sewage in the sewer at the combined sewer overflow is greater than the weir level of the overflow structure which is specified as an overflow setting in table S3.3. 

The capacity of the sewer network downstream of the combined sewer overflow shall not be altered in any way which would lead to a significant increase in the frequency or volume of the discharge. 
The discharge shall not be comminuted or macerated and shall have passed through screens as specified and shall not contain a significant quantity of solid matter with a particle size greater than any indicated. All screenings shall be removed from the discharge. 
Where a mechanically cleaned screen is installed, a telemetry alarm system shall be installed and maintained, as far as reasonably practicable, so as to give the operator immediate notification of a failure of the screen cleaning mechanism, unless otherwise agreed in writing by Natural Resources Wales. The operator shall take all appropriate measures to return the screen cleaning mechanism to normal operation as soon as reasonably practicable after receipt of notification of the failure. 
Emissions and monitoring
[bookmark: _Hlk96092587][bookmark: _Hlk70518089]Emissions to water
The limits given in schedule 3 table S3.1 shall not be exceeded.
Emissions of substances not controlled by emission limits
Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.
Monitoring 
The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring specified in the following tables in schedule 3 to this permit:
point source emissions specified in tables S3.1 and S3.4.
The operator shall maintain records of all monitoring required by this permit.
An accessible monitoring point shall be provided and maintained to enable the emissions monitoring programme to be carried out at the monitoring point specified in table S3.4 of schedule 3 and shown marked on the site plan in schedule 7. 
The operator shall take appropriate measures to ensure that the event recorder remains fully operational at all times within the reference period specified in table S3.1. Any failures shall be remedied as soon as reasonably practicable.
Information
Records
All records required to be made by schedule 3, 4 and 5 to this permit shall:
be legible;
be made as soon as reasonably practicable;
if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 10 years from the date when the records were made. 
The operator shall maintain convenient access, in either electronic or hard copy, to the records, plan and management system required to be maintained by this permit. 
Reporting
The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
Within the time period after the end of the reporting period specified in schedule 4 table S4.1 the operator shall, unless otherwise agreed in writing by Natural Resources Wales, submit reports of the monitoring and assessment carried out in accordance with the conditions of this permit, as follows:
in respect of the parameters and monitoring points specified in schedule 4 table S4.1;
for the reporting periods specified in schedule 4 table S4.1 and using the forms specified in schedule 4 table S4.2; and
giving the information from such results and assessments as may be required by the forms specified in those tables.
Notifications
Natural Resources Wales shall be notified as soon as reasonably practicable following detection, within the site of the regulated facility of any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution. Any other significant adverse environmental effects, which may have been caused by the activity, shall also be notified to Natural Resources Wales as soon as reasonably practicable following detection.
The information provided under condition 4.3.1 shall be supported by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules:
Where the operator is a registered company:
any change in the operator’s trading name, registered name or registered office address; and
any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and
any steps taken with a view to the dissolution of the operator.
0.0.2 For the activities referenced in schedule 1, table S1.1 where the operator proposes to make a change in the nature of the activity by increasing the concentration of, or the addition of, or allowing the introduction of, a substance to the activity to an extent that the operator considers could have a significant adverse environmental effect on the receiving waters, and the change is not permitted by emission limits specified within schedule 3 table S3.1 or the subject of an application for approval under the EP Regulations or under the terms of this permit:
(a) Natural Resources Wales shall be notified in writing at least 14 days before the increase or addition or allowing the introduction; and
(b) the notification shall contain a description of the proposed change.

Interpretation
In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “as soon as reasonably practicable”, in which case it may be provided by telephone.

Schedule 1 – Operations 
	Table S1.1 Activities

	Activity reference
	Description of activity
	Limits of specified activity

	A1
	Trade effluent consisting of site drainage via POINT OF DISCHARGE
	Only include Coed Darcy site drainage previously controlled by permit BP0064319 01

	A2
	Discharge of storm sewage via POINT OF DISCHARGE
	N/A





Schedule 2 – Waste types, raw materials and fuels
Schedule 2 not in use.



Schedule 3 – Emissions and monitoring
	Table S3.1 Point Source emissions to water (other than sewer) – emission limits and monitoring requirements

	Effluent and discharge point
	Parameter  
	Limit (including unit)
	Reference Period
	Limit of effective range
	Monitoring frequency
	Compliance Statistic

	A1 Trade effluent consisting of site drainage via POINT OF DISCHARGE
	Maximum rate of discharge
	957 litres per second
	Instantaneous (spot sample)
	N/A
	Continuous
	Maximum

	
	Suspended solids (measured after drying at 105oC)
	100 mg/l
	Instantaneous (spot sample)
	N/A
	N/A
	Maximum

	
	Visible oil or grease
	No significant trace present so far as is reasonably practicable
	Instantaneous (visual examination )
	N/A
	N/A
	No significant trace


	
	pH
	6 to 9
	Instantaneous (spot sample)
	N/A
	N/A
	Minimum and maximum

	A2 Storm sewage via POINT OF DISCHARGE


	Discharge start and end times 
	N/A


	N/A


	N/A


	Whenever a discharge occurs
	N/A



	
	Block-counted spills 
	N/A
	1st January to 31st December inclusive 
	N/A
	15 minutes
	N/A

	
	Event recorder status operational 
	N/A
	N/A
	N/A
	15 minutes
	N/A


 
	Table S3.2 Discharge points

	Effluent Name
	Discharge Point
	Discharge point NGR
	Receiving water/Environment

	A1 Trade effluent
	POINT OF DISCHARGE
	SS 72990 96379
	Estuarial Waters of the River Neath, via surface water sewer

	A2 Storm sewage
	POINT OF DISCHARGE
	SS 72990 96379
	



	Table S3.3 Storm sewage discharge settings

	Effluent and discharge point 
	Description of discharge
	Overflow setting l/s
	Maximum size of solid matter
	Screen aperture size

	Storm sewage via POINT OF DISCHARGE
	Storm sewage
	360
	No greater than 6 mm in more than 1 dimension
	6 mm x 6 mm mesh screen



	Table S3.4 Monitoring points

	Effluent and discharge point
	Monitoring type
	Monitoring point NGR
	Monitoring point reference

	A1 Trade effluent consisting of site drainage via POINT OF DISCHARGE
	Effluent sampling
	SS 72005 96203
	POINT OF OVERFLOW

	A2 Storm sewage via POINT OF DISCHARGE
	Effluent sampling 
	SS 72005 96203
	POINT OF OVERFLOW

	
	Event duration monitoring 
	SS 72005 96203
	





Schedule 4 – Reporting
Parameters, for which reports shall be made, in accordance with conditions of this permit, are listed below.
	Table S4.1 Reporting of monitoring data

	Activity reference
	Parameter
	Monitoring point reference
	Reporting period
	Period begins

	A1
	Dry Weather Flow (daily flows total)
	POINT OF OVERFLOW
	Annually
Report to be submitted within 2 months of the end of the calendar year
	1 January

	
	Operator Self Monitoring - suspended solids (measured after drying at 105oC)
	
	Quarterly
Report to be submitted within 2 months
	1st of month

	A2
	Event recorder status operational
	POINT OF OVERFLOW
	Annually
Report to be submitted within 2 months
	1st January

	
	CSO performance, including total number of block-counted spills 
	
	Annually
Report to be submitted within 2 months
	1st January

	
	Duration of total spills
	
	Annually
Report to be submitted within 2 months
	1st January

	
	Storm sewage discharge start and end times
	
	Reports to be provided to Natural Resources Wales upon request 
	As specified by Natural Resources Wales



	Table S4.2 Reporting forms

	Activity reference
	Parameter
	Reporting format

	A1
	Dry Weather Flow (daily flows total)
	WISKI electronic format specified by Natural Resources Wales

	
	OSM - suspended solids (measured after drying at 105oC)
	Quarterly - Electronic format specified by Natural Resources Wales

	A2
	Combined sewer overflow performance including number and duration of block-counted spills 
	Annual summary report or other form as agreed in writing by Natural Resources Wales


	
	Storm sewage discharge start and end times 
	Form as agreed in writing by Natural Resources Wales 

	
	Event recorder status

	Annual summary report or other form as agreed in writing by Natural Resources Wales
Percentage of time in the recording period that event duration monitoring equipment is operational

	
	Investigation into the operation of the overflow 
	Electronic format as agreed in writing by Natural Resources Wales. 




Schedule 5 – Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A
	Permit Number
	BP0064319

	Name of operator
	Dŵr Cymru Cyfyngedig

	Location of Facility
	Storm Overflow at The Llandarcy 36” Outfall, Side of Bridge House, Pen-Y-Heol (B4290), Llandarcy, Neath, SA10 6LQ

	Time and date of the detection 
	



	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 7 days of detection unless otherwise agreed in writing by Natural Resources Wales

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released/type or nature of sewage released
	

	Best estimate of the quantity or rate of release of substances and/or duration of discharge
	

	Best estimate of the environmental impact of the discharge
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



Part B – to be submitted as soon as reasonably practicable unless otherwise agreed in writing by Natural Resources Wales
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident/breach/exceedance
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator


Schedule 6 – Interpretation 
“accident” means an accident that may result in pollution.
“annually” means once every year.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“block-counted spill” one or more overflow events within a period of 12 hours or less will be considered to be one spill, one or more overflow events extending over a period of greater than 12 hours up to 36 hours will be considered to be 2 spills. Each subsequent 24-hour duration counts as 1 additional spill and the whole of the 24-hour block is included. 
“event recorder” a recorder which records the start time and end time of individual overflow events 
“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the permitted activities, which are not controlled by an emission limit.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.1154 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“minimum screen capacity flow” means the minimum flow passed through the screens to the outfall when the screen bypass operates. 
“monitoring frequency” as used in Table S3.1 in the context of event duration monitoring is the temporal interval at which a change in state between no discharge and discharge is to be detected.
“Natural Resources Wales” means the Natural Resources Body for Wales established by article 3 of the Natural Resources Body for Wales (Establishment) Order 2012. The Natural Resources Body for Wales (Functions) Order 2013 transferred the relevant functions of the Countryside Council for Wales, and functions of the Environment Agency and the Forestry Commission in Wales to the Natural Resources Body for Wales.
“overflow” for the purposes of schedule 7, overflow means the weir or orifice or other control which directs excess flow away from the continuation sewer when the flow exceeds the overflow setting due to rainfall and/or snowmelt. 

“overflow event” any individual operation, of any duration, of the event recorder or any recorded discharge of sewage from the outfall.
“overflow setting” means the minimum flow passed forward to the continuation sewer when the overflow operates.
“quarter” means a calendar year quarter commencing on 1 January, 1 April, 1 July or 1 October.
“significant pollution” means a high-level impact incident as indicated by NRW incident classification system.
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]“significant spill” any spill that has not been demonstrated to have been, or measured as being, less than 50 m3 in volume.
[bookmark: _Hlk13661209]“SOAF” means Storm Overflow Assessment Framework.
“year” means calendar year ending 31 December.
“Formula A” is defined as (PG+I+E) + 1360P + 2E litres/day.  Where P = population served, G = water consumption per head per day (litres/head/day) I = infiltration (litres/day) E = trade effluent flow to sewer (litres/day)
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