Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1b
Reporting of emissions to air for the period from 01/01/19 to 30/06/19 

	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A1
	Particulates
	-
	
	
	
	
	

	A1
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	0.30 mg/m3
	BS EN 14791
	18/06/19, 11:25 – 13:25
	0.15 mg/m3

	A1
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	6.0 mg/m3
	BS EN 13526
	17/06/19, 17:00 – 21:00
	1.3 mg/m3

	A1
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.03 mg/m3
	BS ISO 15713
	17/06/19, 12:30 – 14:30
	0.02 mg/m3

	A1
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	5.21 mg/m3
	BS EN 1911
	18/06/19, 09:00 – 11:00
	0.59 mg/m3

	A1
	Dioxins
	0.1 ng/m3
	4 hour average
	0.011 ng/m3
	BS EN 1948
	17/06/19, 11:15 – 15:15
	0.009 ng/m3

	
	
	
	
	
	
	
	

	A1
	Carbon Monoxide
	100 mg/m3
	Hourly average
	87.5 mg/m3
	BS EN 15058
	17/06/19, 17:00 – 21:00
	3.5 mg/m3

	
	
	
	
	
	
	
	

	A1
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	7.0 mg/m3
	BS EN 14792
	17/06/19, 17:00 – 21:00
	2.1 mg/m3


Signed …Joel Priest ……………………………………………………….  

Date……26/07/19………

(Authorised to sign as representative of Operator)

Calibration test of particulate CEM not completed due to planned replacement of the CEM with a new system, due to be installed August 2019. New system will be calibrated as part of the installation.
Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1c
Reporting of emissions to air for the period from 01/01/19 to 30/06/19
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A12
	Particulates
	-
	
	
	
	
	

	A12
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	0.00 mg/m3
	BS EN 14791
	18/06/19, 11:10 – 13:10
	0.11 mg/m3

	A12
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	-0.63 mg/m3
	BS EN 13526
	17/06/19, 11:00 – 15:00
	1.3 mg/m3

	A12
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.02 mg/m3
	BS ISO 15713
	17/06/19, 12:10 – 14:10
	0.02 mg/m3

	A12
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.02 mg/m3
	BS EN 1911
	18/06/19, 09:00 – 11:00
	0.01 mg/m3

	A12
	Dioxins
	0.1 ng/m3
	4 hour average
	0.05 ng/m3
	BS EN 1948
	17/06/19, 11:15 – 15:16
	0.02 ng/m3

	
	
	
	
	
	
	
	

	A12
	Carbon Monoxide
	100 mg/m3
	Hourly average
	-0.5 mg/m3
	BS EN 15058
	17/06/19, 11:00 – 15:00
	9.9 mg/m3

	
	
	
	
	
	
	
	

	A12
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	10.9 mg/m3 
	BS EN 14792
	17/06/19, 11:00 – 15:00
	2.1 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……26/07/19………

(Authorised to sign as representative of Operator)

Calibration test of particulate CEM not completed due to planned replacement of the CEM with a new system, due to be installed August 2019. New system will be calibrated as part of the installation.

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1d
Reporting of emissions to air for the year ……2019……
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result 
	Test

Method 
	Sample

Date and Times 
	Uncertainty



	A13
	Particulates
	-
	4 hour average
	
	BS EN 13284-1
	
	

	A13
	Carbon monoxide
	150mg/m3
	Hourly average
	
	BS EN 15058
	
	

	
	
	
	
	
	
	
	

	A13
	Oxides of nitrogen
	60mg/m3
	Hourly average
	
	BS EN 14792
	
	


Signed …Joel Priest………………………………………………………….  

Date……26/07/19……………

(Authorised to sign as representative of Operator)
To be sampled during second annual visit due to access restrictions to sampling point at time of first visit.
