
Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V013

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	21/092019 17:10

	Reference or description of the location of the event 
	Kiln outlet and inlet seal.

	Description of where any release into the environment took place
	The seals connecting the kiln with the cooler hood and the Pre-calciner tower.

	Substances(s) potentially released
	Clinker dust

	Best estimate of the quantity or rate of  release of substances
	500kg

	Measures taken, or intended to be taken, to stop any emission
	FN04 exhaust fan rate increased and FN08 fan reintroduced when cooler bag filter temperature was below limit, both actions taken to create negative pressure in the system. Calibration of Kiln and Calciner Pfister feeders.

	Description of the failure or accident.
	Cyclone 5 temperature increased at 16:00 without additional input of fuels, in reaction the kiln burner reduced coal and SRF input to the calciner to compensate. After the system recovered the Cemfuel feed rate was lost to the main burner, this required higher rates of coal on the burner which had been reduced previously. There was a measured discrepancy between the measured and actual feed rates of coal to the kiln main burner, the resultant effect was that the heat input for the burner and calciner after reacting to high C5 temps was not enough to maintain stable conditions in the kiln. FN08 (cooler) tripped on high BF temp and at this point feed to the kiln was stopped, for 6.5 minutes there was a resultant over pressure on the system and dust release from the inlet and outlet seals primarily.  


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	


	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of Castle Cement Limited
