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1 INTRODUCTION

This Management System Plan has been prepared by AP Waters Building Contractors Ltd and is a component of a suite of documents that form the company’s Environmental Management System for managing recycling activities at the facility known as The Old Foundry Yard, Rockhill Road, Pontypool, NP4 8AN.
The Environmental Management System fulfils the requirements of the site’s Environmental Permit by “providing a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances, closure and those drawn to the attention of the operator as a result of complaints”.  It describes the processes and operations undertaken at the facility, how they are managed and controlled to meet the requirements of the site’s Environmental Permit and Waste Exemptions and any associated best practices and guidance.  In addition, it provides systems and procedures to enable the company to operate in accordance with its Environmental Policy (MPP1).

This Management System Plan is considered a ‘live’ document and as such has been presented in a way which can be easily amended by adding to or removing superseded information.  Each change to the plan will be subject to Natural Resources Wales’ approval prior to insertion in the document.  The plan presents the general engineering details of the site, along with proposed working arrangements, infrastructure, environmental controls, monitoring and site management procedures.

Reference is made throughout this document to processes and procedures within the EMS and in particular to a Corrective Action Response (CAR) which details how the company will deal with any deficiencies identified during a scheduled or unscheduled system audit/check or justified customer/resident/staff complaint.  Where critical activities have been identified, the company has reviewed the processes and procedures that are in place with a view to meeting, and preferably exceeding any statutory obligations placed on them.  Where current measures are deemed insufficient, the company will identify additional controls such as the introduction of documented procedures and work instructions, further training programmes and infrastructure improvements.

Within this EMS Plan, text highlighted in Bold Blue refers to documents that form part of the EMS.

1.1 Overview

The site has historically operated as a builder’s yard.  This EMS Plan was prepared to support the submission of an application to Natural Resources Wales for a Tier 2 standard rules environmental permit SR2008No7 to allow waste transfer, storage, and treatment activities at the site.  The site will receive, sort, and treat largely construction and demolition (C&D) wastes arising from AP Waters’ core business activity.  Inert C&D waste will be crushed to produce hardcore for use within the company’s construction projects (under a waste exemption).  Although available under the standard rues permit, the Operator currently no plans to open the site to other companies, or to expand the waste types beyond C&D wastes.
1.2 Compliance with Permit Requirements

Table 1 summarises the key requirements of the site’s Environmental Permit and the sections of this EMS Plan or associated documents and procedures that, when effectively implemented, will enable the site to comply with these requirements.
	New Format Permit Condition*
	Description
	System Reference or Evidence of Compliance

	1.1.1
	General

management
	(a) Environmental Management system

(b) EMS Plan 4.1.2/4.1.3/4.1.5 and TCM Attendance

	1.1.2
	Records demonstrating compliance
	Site Diary

Archived Forms FR1-FR11
Compliance Audits (Internal/External)

	1.1.3
	Permit copy
	Copy on Staff Notice Board and in Site Office

	1.1.4
	Competence scheme
	EMS Plan 4.1.3 and copies of TCM qualifications

	1.2.1
	Waste hierarchy
	(a) and (b) Environmental Policy and EMS Plan 4.2.1
(c) EMS Plan 4.2.1

	1.2.2
	Review
	EMS Plan1.3

	2.1.1
	Permitted activities
	EMS Plan 5.2
Compliance Audits (Internal/External)

	2.2.1
	Waste acceptance
	EMS Plan 8.3
Procedure PR9

	2.3.1
	Operating techniques
	EMS Plan section 5.2.1.1

	2.4.1
	Site Boundary
	Drawing 10999-001-A in MPP5
Daily site inspections

Compliance Audits (Internal/External)

	2.4.2
	Separation from European Site/SSSI
	Drawing 10999-001-A in MPP5
Daily site inspections

Compliance Audits (Internal/External)

	2.4.3
	Separation from well, spring or borehole.
	Drawing 10999-001-A in MPP5
Daily site inspections

Compliance Audits (Internal/External)

	2.5.1
	Technical Requirements
	EMS Plan 5.2.1.2

	3.1.1/3.1.2
	Emissions
	EMS Plan 9.1.2

	3.1.3
	Secondary Containment
	EMS Plan 7.5/9.1.2.1/9.1.2.2

	3.2.1/3.2.2
	Odour
	EMS Plan 9.1.2.5

	3.3.1/3.3.2
	Noise and Vibration
	EMS Plan 9.1.2.4

	4.1
	Record keeping
	EMS Plan 10

	4.2.1/4.2.2
	Reporting
	EMS Plan 9.3

	4.3.1/4.3.2
	Notifications
	EMS Plan 9.3.2

	4.3.3
	Monitoring or sampling
	EMS Plan 9.1.1.2

	4.3.4
	Other matters
	EMS Plan 9.3.2

	4.4
	Interpretation
	EMS Plan 9.3.3


Table 1. Requirements of Permit

1.3 EMS Review

The Environmental Management System (including this EMS Plan) shall be reviewed annually to confirm whether changes are required to system and procedures.

1.4 Regulations and Guidance

Various guidance documents and statutory instruments have been considered when preparing this plan.  These documents include:

· The Waste (England and Wales) Regulations 2011 (as amended by The Waste (England and Wales) (Amendment) Regulations 2012).

· Environmental Permitting (England and Wales) Regulations 2010

· Environmental Permitting (England and Wales) (Amendment) Regulations 2010

· Environmental Permitting (England and Wales) (Amendment) Regulations 2010 (No. 2)

· Environmental Permitting (England and Wales) (Amendment) Regulations 2011

· Environmental Permitting (England and Wales) (Amendment) (No 2) Regulations 2011

· Environmental Permitting (England and Wales) (Amendment) Regulations 2013

· Industrial Emissions (Integrated Pollution Prevention and Control) (Recast) 2010

· Environment Protection Act 1990

· Clean Neighbourhoods and Environment Act 2005

· Groundwater regulations 1998, SI 2746

· Water Resources Act 1991, as amended

· Hazardous Waste (England and Wales) Regulations 2005 as amended by Hazardous Waste (England and Wales) (Amendment) Regulations 2009)

· Environmental Permitting Guidance -Core Guidance for the Environmental Permitting (England and Wales) Regulations 2010 – March 2013
· Sector Guidance Note IPPC S5.06: Guidance for the Recovery and Disposal of Hazardous and Non-Hazardous Waste

· Horizontal Guidance Note H1 Environmental Risk Assessments for Permits - Overview Document, v2.1 December 2011 and Annexes A to K

· Horizontal Guidance Note H3 Part 2 - Noise Assessment and Control, v3 June 2004

· Horizontal Guidance Note H4 Odour Management, March 2011

· Horizontal Guidance - H6 Environmental Management Systems
· Fire prevention and mitigation plan guidance – Waste Version 2, August 2017
· Environmental Management Toolkit - General Version for Waste Handling Industry, Environment Agency

Elements of this environmental management system plan also consider guidance from the following historic documents:

· Working Plan Guidance and Specification, Volume 1, 19 February 2000
· Technical Guidance Document: ‘How to comply with your environmental permit’

2 Permit Details and Contacts
2.1 Environmental Permit Number

EPR/AB3898HB
2.2 Site Operator

AP Waters Building Contractors Ltd
2.3 Site Address
AP Waters Building Contractors Ltd
The Old Foundry Yard

Rockhill Road

Pontypool

NP4 8AN
2.4 Site Contacts

Switchboard: 01495 758454
General Email:
info@apwaters.com
Managing Director: 
Mr. Adrian Waters
Mobile:


07974 386220
Email:


Adrian@apwaters.com
Technically Competent Person: Mr. A C Lilley WAMITAB Qualified
Mobile:


07833973759
Email:


craiglilley@apwaters.com
Site Manager:

Mr. Adrian Waters

Mobile:


07974 386220

Email:


Adrian@apwaters.com
3 SITE DETAILS
3.1 Site Location
The site comprises an existing building and yard situated on the northern edge of Pontymoile, approximately 0.9km south east from the centre of Pontypool and 1.4km north of the centre of Griffithstown (OS Grid Reference SO 28926 00502).
The surrounding area is characterised by a mix of commercial and residential properties to the south and east, with the River Lwyd and woodland to the north and west.

3.2 Site Access

Access to the site is from the A472 Pyle Road via Rockhill Road.  The A48 connects to the A4042 and then to the M4 at Junction 25A (approximately 7 miles by road to the south of the site).
The Grid reference of the site entrance is SO 28982 00452.
3.3 Site Ownership
The site is owned by Velterhunter Ltd and leased to AP Waters Building Contractors Ltd.

3.4 Site Layout

The permitted area of the site is shown in Drawing 10999-001-A in MPP5.  Drawing 10999-001-B in MPP5 shows the location of the site within the context of the surrounding area.
The site occupies an area of 0.4117 hectares (~1.02 acres) and comprises:

· A car parking area located at the front of the site with space for 10 vehicles.
· A three-story office building comprising welfare and office space of c.38m2 ground floor area adjacent to the entrance of the site.

· A large yard occupying the majority of the site within which are two large workshop buildings and the waste transfer station building.
A block plan for the site is shown in Drawing 10999-001-C in MPP5.  The layout (describing the site in an approximate east to west direction) comprises the following primary areas:

· The site entrance, staff, and visitor parking area.
· A building containing the administrative offices, staff welfare facilities (including kitchen and toilet facilities).
· A Waste Transfer Station Building including waste reception, inspection, treatment and storage area to the south side and a small wood waste storage building on the northern boundary.
· An inert C&D waste storage and processing area occupies much of the north eastern corner of the yard.
· A workshop/office and store/workshop buildings define the southern boundary of the site.
3.5 Sensitive Receptors
A Receptor Plan highlighting human and ecological receptors within the vicinity of the site is presented as Drawing 10999-001-F in MPP5.
3.5.1 Human

The site is located approximately 0.4km north of Pontymoile on a small commercial estate at the edge of the settlement.
The surrounding area is characterised by a mix of commercial and residential properties to the south and east, with the River Lwyd and woodland to the north and west.  The site immediate neighbours are a petrol station, builders’ merchants, and a small number of residential properties to the south west.

The nearest residential housing is located approximately 60m to the south east of the inert C&D processing area and 90m to the west opposite the site entrance.
3.5.2 Ecological
There are no designated sites (SSSI, SAC, RAMSAR, etc.) located within 2km of the site boundary.

To the south west, Cwmynyscoy Quarry LNR is located 966m from the site boundary.
The Brecon Beacons National Park is located 637m to the north east at its closest point.
3.6 Flood Risk

According to NRW’s Flood Risk map the site lies within a flood plain.  The site occupies a significantly elevated position above the River Lwyd and the likelihood of flooding occurring, even in full spate during an extreme weather event, is negligible.
3.7 Groundwater

The site is not located in a Source Protection Zone.

The underlying bedrock and superficial layer designations are Secondary A aquifer.  This identifies the geology as permeable layers capable of supporting water supplies at a local rather than strategic scale, and in some cases forming an important source of base flow to rivers. These are generally aquifers formerly classified as minor aquifers.
4 MANAGEMENT

4.1 General Management

4.1.1 Site Operations

The site shall be operated in accordance with the EMS (of which this Environmental Management System Plan (EMSP) is part).

4.1.2 Site Personnel

Technically competent staff will supervise the site and ensure that it is operated in accordance with the Environmental Permit/Waste Exemptions, the EMS and this Environmental Management System Plan, and current legislation.

The Site Manager will ensure that sufficient competent staff are present on-site to manage and operate the sites’ activities without causing pollution.  Staff will be competent in the activities they are expected to carry out.  Staff will be expected to not only be competent in normal situations, but also be adequately trained so that they are competent in abnormal situations such as plant failures or accidents. 
Procedure PR12 details the method by which the company will record staff responsibilities.  It ensures that staff roles and responsibilities are clearly defined and recorded (Form FR9) and names placed against each role and responsibility (e.g. Technically Competent Person).  Details of who is responsible for ensuring compliance with each part of the permit and other relevant legislation and guidance are also registered.  Documents are reviewed and updated at least every 6 months, or if staff change roles or leave the organisation.
4.1.3 Technically Competent Person

The company will employ and train at least one Technically Competent Person.

The site does have a Technically Competent Manager, who holds a WAMITAB Level 4 qualification HROC6
Other Technically Competent Persons will be recruited as necessary to maintain compliance with permit attendance criteria.  The times that the Technically Competent Person spends at the facility during operating hours will be recorded in the Site Diary.

4.1.4 Access to Permit

All site staff are made aware of the Environmental Permit and EMS, and any person with duties that are controlled by the permit will have convenient access to a copy of it.  This includes not only staff but any contractors that may be working on the site as well.  Staff and contractors will be made aware of the Environmental Permit, what is contained in it, what their obligations are under it and where and how to access it during their initial site induction.

A copy of the Environmental Permit and the most up-to-date approved copy of the Environmental Management System are kept in the Site Office.  The copies may be in paper form and/or electronically available.

4.1.5 Staff Training
New employees will be given full induction training by site managerial staff or other appropriately qualified persons and records will be kept of all staff training in relation to operation of the site, site specific emergency procedures and the content and requirements of the Environmental Permit and Environmental Management System Plan.

According to their various roles and responsibilities, individuals will be instructed in the following necessary procedures regarding the environmental aspects of the site operations:

· Receiving and inspecting loaded waste vehicles.

· Duty of Care requirements and record keeping.

· Unloading and scrutinising tipped loads.

· Dealing with any unauthorised wastes.

· Waste segregation and bulking-up of the separated substances.

· Use of any mechanical plant at the site.

· Storage and inspection of wastes.

· Dispatch of recovered materials and discards.

· Hazardous waste controls.

· General housekeeping including cleanliness of the site and its environs, equipment maintenance, inspection, and maintenance of any drainage systems.

All Technically Competent Persons will undertake training as required to demonstrate Continuing Competence.

Environmental training is undertaken by in-house personnel.  Technical competence training is undertaken by WS Training.
A copy of this Management System Plan and Environmental Permit will be made available at the facility for all staff to read and, as a minimum; they will be informed of the importance of these documents and of the key areas of concern.  They will also be fully briefed on the role of Natural Resources Wales in enforcing compliance.

Competence and training of all site employees is monitored by the site’s HR Manager in accordance with Procedure PR10.  A training matrix and training records (Forms FR7 and FR8) are kept and maintained in the Site Office.

4.1.6 Site Health and Safety

The company is conscious of its obligations to their staff, contractors and visitors and the company’s Environmental Management System dovetails with the company’s in-house Health and Safety management and Quality management processes and/or systems.

The company’s Health and Safety Policy, induction pack/employee handbook and training programmes provide significant information to staff and visitors relating to on-site Health and Safety features, processes, and duties.

Signage around the site highlights important safety considerations for staff and visitors before entering site.  The full set of site rules (ROI1 Site Rules) is displayed at the site entrance for drivers and visitors entering the facility.
A copy of the site rules is also available at the main reception and a further copy affixed to the staff notice board.
4.2 Avoidance, Recovery and Disposal of Wastes Produced by the Activities

4.2.1 Waste Hierarchy

The Waste Hierarchy (as defined in Article 4 of the Waste Framework Directive) will be applied to the generation of waste by the activities and any waste generated will be treated in accordance with the Waste Hierarchy.  Where disposal is necessary, this will be undertaken in a manner that minimises any impact on the environment.  To this end, energy recovery will be used before landfill wherever possible.

4.2.2 Review

Reviews of measures taken to comply with the Waste Hierarchy will be reviewed at least every 4 years.  The Site Manager will be responsible to scheduling the review and ensuring relevant staff and advisors are in attendance.  Any further appropriate measures identified should be carried out to agreed timescales.

5 OPERATIONS
5.1 Site Usage
The site has been developed for:

· A Household, commercial and industrial waste transfer station with treatment and asbestos storage
All site operations are designed for the purposes of recycling all waste arising from household, commercial and industrial, and construction and demolition sources imported predominantly by our own vehicles and occasionally by other licensed waste carriers.
5.2 Permitted Activities
The site is only authorised to carry out the activities specified in 5.2.1.
The activities are only to be undertaken within the boundary of the site as shown in Drawing 10999-001-A in MPP5.
5.2.1 HCI WTS with Treatment and Asbestos Storage (Standard Rules Environmental Permit SR2008No7)
	Household, Commercial and Industrial Waste Transfer Station

	Description of Activities
	Limits of Activities

	D15: Storage pending any of the operations numbered D1 to D14 (excluding temporary storage, pending collection on the site where the waste is produced)
R13: Storage of waste pending any of the operations numbered R1 to R12 (excluding temporary storage, pending collection, on the site where the waste is produced)
D14: Repackaging prior to submission to any of the operations numbered D1 to D13

D9: Physico-chemical treatment not specified elsewhere in Annex IIA
 which results in final compounds or mixtures which are discarded by means of any of the operations numbered D1 to D8 and D10 to D12
R3: Recycling/reclamation of organic substances which are not used as solvents

R4: Recycling/reclamation of metals and metal compounds
R5: Recycling/reclamation of other inorganic materials

	The maximum quantity of asbestos waste received at the site shall not exceed 10 tonnes per day.

The maximum quantity of asbestos waste stored at the site shall not exceed 10 tonnes.

Treatment consisting only of manual sorting, separation, screening, baling, shredding, crushing or compaction of non-hazardous waste into different components for disposal, (no more than 50 tonnes per day) or recovery.

There shall be no treatment of asbestos waste.

No more than a total of 50 tonnes of intact and shredded waste vehicle tyres (waste codes 16 01 03 and 19 12 04) shall be stored at the site.


Table 2 Waste management operations to be undertaken

Waste shall only be accepted if:
(a) it is of a type and quantity listed in Table 3 below; and

(b) it conforms to the description in the documentation supplied by the producer and holder.

NOTE: Any waste whose six-digit code is marked with an asterisk (*) is a hazardous waste.  
	Exclusions: 

Wastes having any of the following characteristics shall not be accepted. 
· Wastes consisting solely or mainly of dusts, powders, or loose fibres. 
· Wastes that are in a form which is either sludge or liquid

	1
	WASTES RESULTING FROM EXPLORATION, MINING, QUARRYING, AND PHYSICAL AND CHEMICAL TREATMENT OF MINERALS

	01 01
	wastes from mineral excavation

	01 01 01
	wastes from mineral metalliferous excavation

	01 01 02
	wastes from mineral non-metalliferous excavation

	01 03
	wastes from physical and chemical processing of metalliferous minerals

	01 03 06
	tailings other than those mentioned in 01 03 04 and 01 03 05

	01 03 09
	red mud from alumina production other than the wastes mentioned in 01 03 07

	01 04
	wastes from physical and chemical processing of non-metalliferous minerals

	01 04 08
	waste gravel and crushed rocks other than those mentioned in 01 04 07

	01 04 09
	waste sand and clays

	01 04 11
	wastes from potash and rock salt processing other than those mentioned in 01 04 07

	01 04 12
	tailings and other wastes from washing and cleaning of minerals other than those mentioned in 01 04 07 and 01 04 11

	01 04 13
	wastes from stone cutting and sawing other than those mentioned in 01 04 07

	2
	WASTES FROM AGRICULTURE, HORTICULTURE, AQUACULTURE, FORESTRY, HUNTING AND FISHING, FOOD PREPARATION AND PROCESSING

	02 01
	wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing

	02 01 03
	plant-tissue waste

	02 01 04
	waste plastics (except packaging)

	02 01 07
	wastes from forestry

	02 01 10
	waste metal

	02 02
	wastes from the preparation and processing of meat, fish, and other foods of animal origin

	02 02 03
	materials unsuitable for consumption or processing

	02 03
	wastes from fruit, vegetables, cereals, edible oils, cocoa, coffee, tea and tobacco preparation and processing; conserve production; yeast and yeast extract production, molasses preparation and fermentation

	02 03 04
	materials unsuitable for consumption or processing

	02 04
	wastes from sugar processing

	02 04 01
	soil from cleaning and washing beet

	02 04 02
	off-specification calcium carbonate

	02 05
	wastes from the dairy products industry

	02 05 01
	materials unsuitable for consumption or processing

	02 06
	wastes from the baking and confectionery industry

	02 06 01
	materials unsuitable for consumption or processing

	02 06 02
	wastes from preserving agents

	02 07
	wastes from the production of alcoholic and non-alcoholic beverages (except coffee, tea, and cocoa)

	02 07 01
	wastes from washing, cleaning, and mechanical reduction of raw materials

	02 07 02
	wastes from spirits distillation

	02 07 04
	materials unsuitable for consumption or processing

	3
	WASTES FROM WOOD PROCESSING AND THE PRODUCTION OF PANELS AND FURNITURE, PULP, PAPER AND CARDBOARD

	03 01
	wastes from wood processing and the production of panels and furniture

	03 01 01
	waste bark and cork

	03 01 05
	sawdust, shavings, cuttings, wood, particle board and veneer other than those mentioned in 03 01 04

	03 03
	wastes from pulp, paper and cardboard production and processing

	03 03 01
	waste bark and wood

	03 03 07
	mechanically separated rejects from pulping of wastepaper and cardboard

	03 03 08
	wastes from sorting of paper and cardboard destined for recycling

	03 03 10
	Fibre rejects, fibre-, filler- and coating-sludges from mechanical separation

	4
	WASTES FROM THE LEATHER, FUR AND TEXTILE INDUSTRIES

	04 01
	Wastes from the leather and fur industry

	04 01 08
	waste tanned leather (blue sheeting’s, shavings, cuttings, buffing dust) containing chromium

	04 01 09
	wastes from dressing and finishing

	04 02
	wastes from the textile industry

	04 02 21
	wastes from unprocessed textile fibres

	04 02 22
	wastes from processed textile fibres

	6
	WASTES FROM INORGANIC CHEMICAL PROCESSES

	06 09
	wastes from the MSFU of phosphorous chemicals and phosphorous chemical processes

	06 09 02
	phosphorous slag

	06 09 04
	calcium-based reaction wastes other than those mentioned in 06 09 03

	06 11
	wastes from the manufacture of inorganic pigments and opacifies

	06 11 01
	calcium-based reaction wastes from titanium dioxide production

	7
	WASTES FROM ORGANIC CHEMICAL PROCESSES

	07 02
	wastes from the MFSU of plastics, synthetic rubber, and man-made fibres

	07 02 13
	waste plastic

	9
	WASTES FROM THE PHOTOGRAPHIC INDUSTRY

	09 01
	wastes from the photographic industry

	09 01 07
	photographic film and paper containing silver or silver compounds

	09 01 08
	photographic film and paper free of silver or silver compounds

	09 01 10
	single-use cameras without batteries

	09 01 12
	single-use cameras containing batteries other than those mentioned in 09 01 11

	10
	WASTES FROM THERMAL PROCESSES

	10 01
	wastes from power stations and other combustion plants (except 19)

	10 01 01
	bottom ash, slag, and boiler dust (excluding boiler dust mentioned in 10 01 04)

	10 01 05
	calcium-based reaction wastes from flue-gas desulphurisation in solid form

	10 01 07
	calcium-based reaction wastes from flue-gas desulphurisation in sludge form

	10 01 15
	bottom ash, slag, and boiler dust from co-incineration other than those mentioned in 10 01 14

	10 01 19
	wastes from gas cleaning other than those mentioned in 10 01 05, 10 01 07 and 10 01 18

	10 01 24
	sands from fluidised beds

	10 02
	wastes from the iron and steel industry

	10 02 01
	wastes from the processing of slag

	10 02 02
	unprocessed slag

	10 02 08
	solid wastes from gas treatment other than those mentioned in 10 02 07

	10 02 10
	mill scales

	10 02 14
	sludges and filter cakes from gas treatment other than those mentioned in 10 02 13 (consisting of filter cakes only)

	10 02 15
	other sludges and filter cakes (consisting of other filter cakes only)

	10 03
	wastes from aluminium thermal metallurgy

	10 03 02
	anode scraps

	10 03 05
	waste alumina

	10 03 16
	skimming’s other than those mentioned in 10 03 15

	10 03 18
	carbon-containing wastes from anode manufacture other than those mentioned in 10 03 17

	10 03 24
	solid wastes from gas treatment other than those mentioned in 10 03 23

	10 03 26
	sludges and filter cakes from gas treatment other than those mentioned in 10 03 25 (consisting of filter cakes only)

	10 03 28
	wastes from cooling-water treatment other than those mentioned in 10 03 27

	10 03 30
	wastes from treatment of salt slags and black drosses other than those mentioned in 10 03 29

	10 04
	wastes from lead thermal metallurgy

	10 04 10
	wastes from cooling-water treatment other than those mentioned in 10 04 09

	10 05
	wastes from zinc thermal metallurgy

	10 05 01
	slags from primary and secondary production

	10 05 09
	wastes from cooling-water treatment other than those mentioned in 10 05 08

	10 05 11
	dross and skimming’s other than those mentioned in 10 05 10

	10 06
	wastes from copper thermal metallurgy

	10 06 01
	slags from primary and secondary production

	10 06 02
	dross and skimming from primary and secondary production

	10 06 10
	wastes from cooling-water treatment other than those mentioned in 10 06 09

	10 07
	wastes from silver, gold, and platinum thermal metallurgy

	10 07 01
	slags from primary and secondary production

	10 07 02
	dross and skimming from primary and secondary production

	10 07 03
	solid wastes from gas treatment

	10 07 05
	sludges and filter cakes from gas treatment (consisting of filter cakes only)

	10 07 08
	wastes from cooling-water treatment other than those mentioned in 10 07 07

	10 08
	wastes from other non-ferrous thermal metallurgy

	10 08 09
	other slags

	10 08 11
	dross and skimming’s other than those mentioned in 10 08 10

	10 08 13
	carbon-containing wastes from anode manufacture other than those mentioned in 10 08 12

	10 08 14
	anode scrap

	10 08 18
	sludges and filter cakes from flue-gas treatment other than those mentioned in 10 08 17 (consisting of filter cakes only)

	10 08 20
	wastes from cooling-water treatment other than those mentioned in 10 08 19

	10 09
	wastes from casting of ferrous pieces

	10 09 03
	furnace slag

	10 09 06
	casting cores and moulds which have not undergone pouring other than those mentioned in 10 09 05

	10 09 08
	casting cores and moulds which have undergone pouring other than those mentioned in 10 09 07

	10 09 14
	waste binders other than those mentioned in 10 09 13

	10 09 16
	waste crack-indicating agent other than those mentioned in 10 09 15

	10 10
	wastes from casting of non-ferrous pieces

	10 10 03
	furnace slag

	10 10 06
	casting cores and moulds which have not undergone pouring, other than those mentioned in 10 10 05

	10 10 08
	casting cores and moulds which have undergone pouring, other than those mentioned in 10 10 07

	10 10 14
	waste binders other than those mentioned in 10 10 13

	10 10 16
	waste crack-indicating agent other than those mentioned in 10 10 15

	10 11
	wastes from manufacture of glass and glass products

	10 11 03
	waste glass-based fibrous materials

	10 11 10
	waste preparation mixture before thermal processing, other than those mentioned in 10 11 09

	10 11 12
	waste glass other than those mentioned in 10 11 11

	10 11 16
	solid wastes from flue-gas treatment other than those mentioned in 10 11 15

	10 11 18
	filter cakes from flue-gas treatment other than those mentioned in 10 11 17

	10 12
	wastes from manufacture of ceramic goods, bricks, tiles, and construction products

	10 12 01
	waste preparation mixture before thermal processing

	10 12 05
	sludges and filter cakes from gas treatment (consisting of filter cakes only)

	10 12 06
	discarded moulds

	10 12 08
	waste ceramics, bricks, tiles, and construction products (after thermal processing)

	10 12 10
	solid wastes from gas treatment other than those mentioned in 10.12 09

	10 12 12
	wastes from glazing other than those mentioned in 10.12.11

	10 13
	wastes from manufacture of cement, lime and plaster and articles and products made from them

	10 13 01
	waste preparation mixture before thermal processing

	10 13 04
	wastes from calcination and hydration of lime

	10 13 07
	sludges and filter cakes from gas treatment (consisting of filter cakes only)

	10 13 10
	wastes from asbestos-cement manufacture other than those mentioned in 10 13 09

	10 13 11
	wastes from cement-based composite materials other than those mentioned in 10 13 09 and 10 13 10

	10 13 13
	solid wastes from gas treatment other than those mentioned in 10 13 12

	10 13 14
	waste concrete

	11
	WASTES FROM CHEMICAL SURFACE TREATMENT AND COATING OF METALS AND OTHER MATERIALS; NON-FERROUS HYDRO METALLURGY

	11 01
	wastes from chemical surface treatment and coating of metals and other materials (for example galvanic processes, zinc coating processes, pickling processes, etching, phosphating, alkaline degreasing, anodising)

	11 01 10
	filter cakes other than those mentioned in 11 01 09

	11 01 14
	degreasing wastes other than those mentioned in 11 01 13

	11 02
	wastes from non-ferrous hydrometallurgical processes

	11 02 03
	wastes from the production of anodes for aqueous electrolytical processes

	11 02 06
	wastes from copper hydrometallurgical processes other than those mentioned in 11 02 05

	11 05
	wastes from hot galvanising processes

	11 05 01
	hard zinc

	11 05 02
	zinc ash

	12
	WASTES FROM SHAPING AND PHYSICAL AND MECHANICAL SURFACE TREATMENT OF METALS AND PLASTICS

	12 01
	wastes from shaping and physical and mechanical surface treatment of metals and plastics

	12 01 01
	ferrous metal filings and turnings

	12 01 03
	non-ferrous metal filings and turnings

	12 01 05
	plastics shavings and turnings

	12 01 13
	welding wastes

	12 01 17
	waste blasting material other than those mentioned in 12 01 16

	12 01 21
	spent grinding bodies and grinding materials other than those mentioned in 12 01 20

	15
	WASTE PACKAGING: ABSORBENTS, WIPING CLOTHS, FILTER MATERIALS AND PROTECTIVE CLOTHING NOT OTHERWISE SPECIFIED

	15 01
	packaging (including separately collected municipal packaging waste)

	15 01 01
	paper and cardboard packaging

	15 01 02
	plastic packaging

	15 01 03
	wooden packaging

	15 01 04
	metallic packaging

	15 01 05
	composite packaging

	15 01 06
	mixed packaging

	15 01 07
	glass packaging

	15 01 09
	textile packaging

	15 02
	absorbents, filter materials, wiping cloths and protective clothing

	15 02 03
	absorbents, filter materials, wiping cloths and protective clothing other than those mentioned in 15 02 02


	16
	WASTES NOT OTHERWISE SPECIFIED IN THE LIST

	16 01
	end-of-life vehicles from different means of transport [including off-road machinery] and wastes from dismantling of end-of-life vehicles and vehicle maintenance (except 13,14, 16 06 and 16 08)

	16 01 03
	end-of-life tyres

	16 02
	wastes from electrical and electronic equipment

	16 02 14
	discarded equipment other than those mentioned in 16 02 09 to 16 02 13 

	16 02 16
	components removed from discarded equipment other than those mentioned in 16 02 15

	16 03
	off-specification batches and unused products

	16 03 04
	inorganic wastes other than those mentioned in 16 03 03

	16 03 06
	organic wastes other than those mentioned in 16 03 05

	16 06
	batteries and accumulators

	16 06 04
	alkaline batteries (except 16 06 03)

	16 06 05
	other batteries and accumulators

	16 11
	waste linings and refractories

	16 11 02
	carbon-based linings and refractories from metallurgical processes others than those mentioned in 16 11 01

	16 11 04
	other linings and refractories from metallurgical processes other than those mentioned in 16 11 03

	16 11 06
	linings and refractories from non-metallurgical processes others than those mentioned in 16 11 05

	17
	CONSTRUCTION AND DEMOLITION WASTES (INCLUDING EXCAVATED SOIL FROM CONTAMINATED SITES)

	17 01
	concrete, bricks, tiles, and ceramics

	17 01 01
	Concrete

	17 01 02
	Bricks

	17 01 03
	tiles and ceramics

	17 01 07
	mixtures of concrete, bricks, tiles, and ceramics other than those mentioned in 17 01 06

	17 02
	wood, glass, and plastic

	17 02 01
	Wood

	17 02 02
	Glass

	17 02 03
	Plastic

	17 03
	bituminous mixtures, coal tar and tarred products

	17 03 02
	bituminous mixtures other than those mentioned in 17 03 01

	17 04
	metals (including their alloys)

	17 04 01
	copper, bronze, brass

	17 04 02
	Aluminium

	17 04 03
	Lead

	17 04 04
	Zinc

	17 04 05
	iron and steel

	17 04 06
	Tin

	17 04 07
	mixed metals

	17 04 11
	cables other than those mentioned in 17 04 10

	17 05
	soil (including excavated soil from contaminated sites), stones and dredging spoil

	17 05 04
	soil and stones other than those mentioned in 17 05 03

	17 05 08
	track ballast other than those mentioned in 17 05 07

	17 06
	insulation materials and asbestos-containing construction materials

	17 06 01*
	insulation materials containing asbestos

	17 06 04
	insulation materials other than those mentioned in 17 06 01 and 17 06 03

	17 06 05*
	construction materials containing asbestos

	17 08
	gypsum-based construction material

	17 08 02
	gypsum-based construction materials other than those mentioned in 17 08 01

	17 09
	other construction and demolition wastes

	17 09 04
	mixed construction and demolition waste other than those mentioned in 17 09 01, 17 09 02 and 17 09 03

	19
	WASTES FROM WASTE MANAGEMENT FACILITIES, OFF-SITE WASTEWATER TREATMENT PLANTS AND PREPARATION OF WATER INTENDED FOR HUMAN CONSUMPTION/INDUSTRIAL USE

	19 01
	wastes from incineration or pyrolysis of waste

	19 01 02
	ferrous materials removed from bottom ash

	19 01 12
	bottom ash and slag other than those mentioned in 19 01 11

	19 01 18
	pyrolysis wastes other than those mentioned in 19 01 17

	19 01 19
	sands from fluidised beds

	19 02
	wastes from physico/chemical treatments of waste (including dechromatation, decyanidation, neutralisation)

	19 02 03
	premixed wastes composed only of non-hazardous wastes

	19 02 10
	combustible wastes other than those mentioned in 19 02 08 and 19 02 09

	19 04
	vitrified waste and wastes from vitrification

	19 04 01
	vitrified waste

	19 05
	wastes from aerobic treatment of solid wastes

	19 05 01
	non-composted fraction of municipal and similar wastes

	19 05 02
	non-composted fraction of animal and vegetable waste

	19 05 03
	off-specification compost

	19 12
	wastes from the mechanical treatment of waste (for example sorting, crushing, compacting, pelletising) not otherwise specified

	19 12 01
	paper and cardboard

	19 12 02
	ferrous metal

	19 12 03
	non-ferrous metal

	19 12 04
	plastic and rubber

	19 12 05
	glass

	19 12 07
	wood other than that mentioned in 19 12 06

	19 12 08
	textiles

	19 12 09
	minerals (for example sand, stones)

	19 12 10
	combustible waste (refuse derived fuel)

	19 13
	wastes from soil and groundwater remediation

	19 13 02
	solid wastes from soil remediation other than those mentioned in 19 13 01

	20
	MUNICIPAL WASTES (HOUSEHOLD WASTE AND SIMILAR COMMERCIAL, INDUSTRIAL AND INSTITUTIONAL WASTES) INCLUDING SEPARATELY COLLECTED FRACTIONS

	20 01
	separately collected fractions (except 15 01)

	20 01 01
	paper and cardboard

	20 01 02
	glass

	20 01 08
	biodegradable kitchen and canteen waste

	20 01 10
	clothes

	20 01 11
	textiles

	20 01 34
	batteries and accumulators other than those mentioned in 20 01 33

	20 01 36
	discarded electrical and electronic equipment other than those mentioned in 20 01 21, 20 01 23 and 20 01 35

	20 01 38
	wood other than that mentioned in 20 01 37

	20 01 39
	plastics

	20 01 40
	metals

	20 01 41
	wastes from chimney sweeping

	20 02
	garden and park waste (including cemetery waste)

	20 02 01
	biodegradable waste

	20 02 02
	soil and stones

	20 03
	other municipal wastes

	20 03 01
	mixed municipal waste

	20 03 02
	waste from markets

	20 03 03
	street-cleaning residues

	20 03 07
	bulky waste


Table 3.  Permitted waste types for HCI Waste Transfer Station with Treatment
5.2.1.1 Operating techniques

The activities shall be operated in accordance with the documentation specified in Table 4 unless otherwise agreed in writing with Natural Resources Wales.

	Description
	Parts
	Document Ref.

	1. Unless stored or treated outside as specified waste
:
(a) all bulking, transfer or treatment of non-hazardous waste shall be carried out inside a building
;

(b) all non-hazardous waste shall be stored in a building or within a secure container.
(c) all non-hazardous waste shall be stored and treated on an impermeable surface
 with sealed drainage system
.

2. Specified waste shall be stored and treated on hard standing or on an impermeable surface with sealed drainage system.
3. Asbestos waste shall be double bagged and stored within clearly identified, segregated, secure, lockable containers on an impermeable surface with sealed drainage system.


Table 4  Operating techniques.
5.2.1.2 Discharges from Site

Point source emissions into surface waters or groundwater are not permitted.

Discharge(s) of site drainage are permitted in accordance with any criteria set out in Table 4.
5.2.1.3 The Site
The activities shall not extend beyond the site, being the land shown edged in green on the site plan attached to the permit.

The activities shall not be carried out within 500 metres of a European Site or SSSI.

The activities shall not be carried out within 50m of any well spring or borehole used for the supply of water for human consumption. This must include private water supplies.

No treatment of specified waste, unless undertaken in a building, shall take place within a specified AQMA.
5.2.1.4 Technical Requirements
5.2.1.4.1 Waste battery and accumulator treatment

Treatment of waste batteries and accumulators must meet the minimum requirements set out in Annex III, Part A of Directive 2006/66/EC of the European Parliament and of the Council on batteries and accumulators and waste batteries and accumulators and repealing Directive 91/157/EEC.

5.2.1.4.2 Hazardous waste storage and treatment

Hazardous waste shall not be mixed, either with a different category of hazardous waste or with other waste, substances or materials, unless it is authorised by Table 2 and appropriate measures are taken.
5.2.1.5 Site Capacity
The total quantity of waste that can be accepted at the site must be less than 75,000 tonnes per annum.

6 SITE INFRASTRUCTURE

6.1 Site Entrance
An identification sign shall be erected and maintained in a prominent position at the site entrance.  The sign shall be approximately 0.75m by 1m and display the following information.

•
Site name and address

•
Name of site operator

•
Name of EP holder

•
EP number

•
Emergency contact telephone number

•
Statement that the site is licensed by NRW

•
NRW contact details

•
Operational site hours
A copy of the site rules (ROI1 Site Rules) is also to be displayed at the site entrance for drivers and visitors entering the facility.  The sign shall be approximately 0.75m by 1m.
6.2 Site Accommodation

The site is equipped with the following facilities:

•
Site office facilities

•
Welfare/Mess facilities

The site office is positioned at the front of the main office building (adjacent to the site entrance), and will be equipped with a telephone line, suitable for emergency calls.  The office will provide suitable space to permit secure short-term record keeping.  All records specifically relating to recycling operations shall be retained on-site.  The site office will keep a copy of the Environmental Permit/Waste Exemptions and the most up-to-date approved copy of the Environmental Management System (EMS).  All site staff shall be made aware of the Environmental Permit/Waste Exemptions and EMS and will be required to be aware of the documents’ contents.

Appropriate welfare facilities will be provided at site and maintained by site staff.  Car parking will be provided for staff members and site visitors just inside the site entrance.  This area will be maintained to minimise surface water ponding and to direct surface water to the site’s drainage system.

With the exception of collection vehicles and storage containers in the yard, all site equipment and machinery will be securely stored within the transfer station building or workshop buildings.

6.3 Plant and Equipment

The following plant and equipment are located within the site:

· Mobile lifting and waste handling equipment – excavators, telehandlers, and forklift trucks, etc.
· Crushing and screening equipment (crusher bucket attachment)
· Storage areas

· Small fuel storage containers
6.4 Lighting

Security lighting and lighting to ensure H&S requirements are met in low-light conditions shall be available.

6.5 Site Security

The permitted area is within an enclosed site occupied by AP Waters Building Contractors Ltd.

Access to the site is via a pair of 2.0 m high steel palisade fence type gates.  An earth embankment/bund and 2.0m strained wire fence encloses the site boundary to the front.  
A wall ~0.4m-1.2m high surrounds the yard along the northern and western perimeters of the site, with the concrete surface graded to ensure that surface water flows away from this wall.    In addition to the wall, a 2.4m solid steel sheet fence mounted to concrete posts also surrounds the northern and western perimeters of the site.  A wall up to ~8m high surrounds the yard along its southern perimeter.
The security gates and site boundary are inspected daily as part of the site inspection schedule.  The gates are always locked when the site is unattended.

During the period which the site has been operational, the security boundary has been proven to be fit for purpose.

CCTV is used to monitor key areas for security and Health and Safety purposes.  

In the event of unauthorised intrusion, the circumstances and any subsequent action taken will be entered in the Site Diary.

6.6 Inspection and Maintenance Procedures for Site Infrastructure

The yard, building, office/welfare area, fence and entrance gates/doors are inspected twice daily, and the outcome of those inspections are recorded on the daily inspection checklist as shown in EMS Form FR1 and if necessary, as a CAR (Form FR11).  The CAR will identify the root cause of the problem and allocate a person and timeframe to ensure that the corrective action is carried out.  Any defect encountered during inspection will be repaired as soon as is reasonably practicable within the working day as a temporary measure and permanent repairs will be completed within 7 working days.

The existing concrete slab will be cleared of all wastes in a phased sequence to ensure that all areas are progressively exposed for inspection at a frequency no less than once per month.  The cleared areas will be swept clean or scraped to remove any adhering solids.  The exposed areas will then be inspected thoroughly, with impervious surfaces inspected to ensure continuing impervious integrity and all surfaces inspected for wear and tear that may impact their suitability for use.  Any defects will be repaired to a standard no less than that when new.  The dates of all such inspections, the findings and any repairs and cleaning undertaken will be entered in the Site Diary.

Maintenance procedures are detailed in Procedure PR11.  Maintenance schedules identifying items of plant and vehicles, location of maintenance instructions and responsibilities will be kept and maintained (Form FR5A and FR5B).  Maintenance records (Form FR6A and FR6B) for site infrastructure, plant and vehicles will be kept in the Site Office and maintained by the Site Manager.

6.7 Site Health and Safety

The company’s Health and Safety Policy, employee handbook and training programmes provide significant information relating to on-site Health and Safety duties.

7 SITE ENGINEERING FOR POLLUTION PREVENTION AND CONTROL
In general waste management activities at the site relate to the receipt, storage, segregation, and recovery of a wide range of construction and demolition wastes, and the storage of asbestos.
7.1 Overview of Site
The site comprises a number of buildings and a large open yard area nominally divided into areas for the different waste activities.  
Waste treatment and storage activities are undertaken on surfaces as follows:

	Description of Activities
	Surface

	HCI Waste Transfer Station
	All waste is stored and treated (sorted, bulked) in a building on impermeable surface with sealed drainage.

	Specified wastes (inert C&D wastes)
	All waste is stored and treated (crushed and screened) on impermeable surface with sealed drainage.


7.2 Yard Areas

7.2.1 Design and Construction

The front yard/car park area is surfaced in asphalt ~150mm thick laid on MOT Type 1 sub-base ~200mm thick.  

The rear yard area is surfaced in reinforced concrete >200mm thick laid on MOT Type 1 sub-base >200mm thick. 

7.2.2 Drainage Design

The surface of the main yard area is graded to channel run-off towards a central gully.  From the gully, surface water is directed to a silt trap and then to an interceptor before being piped into the combined (foul and surface water) sewer that runs under the site.  A catch pit within the wash-down area to the north of the main yard also directs water to the silt trap.

The western side of the yard is graded to channel surface water to a linear (aco) drain.  This is also connected to the silt trap/interceptor.  This area is not currently used for waste storage but may be used on a temporary basis to cope with seasonal demand.
The asphalt car park and access road at the entrance to the site are graded to channel surface run-off to a central gulley.  This is connected directly to the combined sewer.  This area is not used for waste storage or treatment.

A wall ~0.4m-1.2m high surrounds the yard along the northern and western perimeters of the site, with the concrete surface graded to ensure that surface water flows away from this wall.  Were there to be a blockage in the drainage system, no water would run directly off of the site and into the adjacent River Lwyd.
Drawing 10999 – 001 – D in MPP5. shows a drainage plan for the site.
On a monthly basis, from experience, and more often during other periods such as adverse weather conditions site operatives will inspect the storage tanks/interceptor and arrange removal of residual materials and cleaning of the traps.  This will be recorded and monitored within the site inspection and maintenance records (Forms FR1 and FR6A).

7.3 Waste Transfer Station Building and Wood Storage Building
7.3.1 Design and Construction

The Waste Transfer Station and wood storage buildings comprises a steel portal frame construction covered in trapezoidal formed steel cladding.
The existing floor comprises an impermeable reinforced concrete surface >150mm thick.

The floor will be inspected annually by a Chartered Civil Engineer who will report whether or not the impermeable surface is in a good condition and suitable for the purpose described in the Environmental Management System Plan.

7.3.2 Drainage Design

A fall towards the centre of the slab channels liquid by gravity such that it is contained and can be removed using spill kits.
Roof water from the Waste Transfer Station building is directed through gutters and downpipes from where it is channelled through underground pipes to soakaway.
7.4 Foul Drainage

Foul water from the welfare facilities passes through underground pipes to the combined sewer connection that runs under the site.
7.5 Design and Construction of Fuel and Oil Storage Tanks

The following fuel and oil storage are present on-site:

· Red diesel is stored in a locked, bunded container to the north of the yard. (1340 litres max.)

· Petrol is stored in a locked cupboard within the workshop/office building. (20 litres max.)

· Workshop oils and lubricants are stored in 5-10l containers on a storage rack and in 4 x 205l drums within the workshop/office building (20 litres max.)
· Waste workshop oils are stored in 3 no. 1000 litre metal tanks within the workshop/office building.  In the event of a failure of a tank the floor is graded to channel spills into a sealed sump (inspection pit)
8 SYSTEMS AND PROCEDURES
8.1 Operational Flowchart

Drawing 10999 – 001 - G in MPP5 provides a summary of processes and materials flows to be undertaken at the facility.

8.2 Hours of Operation

The hours of operation are:
	Monday – Friday
	Saturday
	Sunday
	Bank/Public Holidays

	09:00hrs – 17:00hrs
	Closed
	Closed
	Closed


Table 5. Hours of operation

8.3 Waste Acceptance, Control Systems and Procedures

Refer to Procedure PR9 for details of Waste Acceptance Procedure.
Procedure PR8 describes what to do in the event of suspicious items being identified (or potentially identified) within loads.
8.4 Waste Quantity Measurement System 

Waste arriving at the facility will be delivered in the Operator’s own vehicles.  These comprise a number of transits van-based tippers, a 13 T Hiab lorry, 13T hook loader and 7.5 T tippers.  The Hiab lorry and hook loader have a maximum tare weight of 13 Tonnes and as such no quantities above that enter (or leave) the site by company vehicles.
All waste arriving or leaving the facility in smaller vehicles are required to pass over the site weighbridge for the purposes of recording the consignment weight.  The weighbridge receives at least 1 annual calibration check in addition to the regular system checks as required under weights and measures legislation.  The information regarding weights passing over the weighbridge is retained at the weighbridge office for further reference.  CCTV footage is recorded at the Weighbridge.
Larger vehicles are unable to use the weighbridge.  The weight of received/dispatched waste will be assessed, by utilising the conversion factors specified by Natural resources Wales or else by measurement on an independent weighbridge. The weight of dispatched waste containers will be retrieved from the waste disposal or receiving site, historical information or assessed using conversion factors. 

All waste arriving or leaving the facility is issued a waste transfer note by either us or a third-party stating waste type and quantity.  All employees are trained in the identification of waste types and quantities and issuing of waste transfer notes.  
Larger quantities may be removed by third parties when exchanging their roll on roll off/skips/drums and these are issued a waste transfer note by the destination which states quantities and all the relevant information.  All waste transfer notes are kept on site for a minimum of 3 years
8.5 Waste Sampling and Testing

It is not normally necessary for the Permit Holder to sample and analyse waste supplies since these are limited to materials of a relatively innocuous and predictable nature.  Where there is uncertainty over the content of deliveries or any suspicion of contamination (e.g. liquid residues in drums or suspected fibrous asbestos etc.) these will be quarantined, and expert advice sought.  This, as appropriate, will include the advice of NRW.

Should a waste supply be offered for which more detailed chemical information is required, then in order to avoid any environmental risk in the handling of such waste, specialist advice and testing to ensure compliance with the site’s waste acceptance criteria (as appropriate) will be sought prior to its acceptance.

The occasions when any sampling is undertaken will be recorded in the Site Diary. Results of all such analyses will be maintained in the site office.

8.6 Waste Treatment Procedures

This document, and any other procedures contained within the EMS (and relevant H&S and Quality documents) should be followed at all times.
8.7 Burning of Wastes
Burning of any wastes, either in the open, inside buildings or in any form of incinerator is not permitted anywhere within the site.

8.8 Waste storage

8.8.1 General

Waste will be stored in designated areas of the facility.

Storage areas will include:

· The waste reception, tipping, and sorting area (in-building)
· The segregated material containers within the WTS building adjacent to the sorting area
· The external bays and containers
· The covered quarantine area

A storage plan for the facility is presented in Drawing 10999 – 001 – E in MPP5.
All waste storage will comply with prevailing guidance for Fire Prevention and Mitigation plans published by Natural Resources Wales and as detailed in the sites Fire Prevention and Mitigation Plan (MPP6).
8.8.2 Storage Durations

The facility will have the following maximum tonnages and storage times:

	Material
	Tonnes
	Storage Time

	Unsorted Mixed C&D Waste
	35
	72 hours

	Green
	5
	1 Month

	Residual
	30
	1 Month

	Paper/Card
	5
	3 Months

	Wood
	30
	3 Months

	Plastic (Film or Rigid)
	10
	3 Months

	Cables
	3
	3 Months

	Metals
	10
	3 Months

	Quarantine
	1
	3 Months

	Gypsum
	10
	6 Months

	Fibreglass/Glass
	1
	6 Months

	Asbestos
	5
	6 Months

	Inert aggregates, Soil & Stone
	1,000
	3 Years


8.9 Dispatch

Wastes leaving the site for further treatment, disposal, or recovery, will be described, quantified, and appropriately containerised in accordance with the Duty of Care.  NB: regular deliveries of waste to the same outlet may be recorded by way of the 'season ticket' provisions.  Such materials are transported by authorised waste carriers only and dispatched only to authorised outlets.
In the event of any hazardous wastes being removed from the site, these will be removed in accordance with the required consignment note procedures. 

All records of delivery and dispatch, including copies of the Duty of Care Transfer Notes and Hazardous Waste Consignment Notes will be maintained in the site office.  These are available for inspection by authorised officers of NRW at any reasonable time.  Quarterly 'waste returns' will be provided to NRW as required.

The Company's regular waste suppliers and outlet providers will be periodically visited, and their control procedures assessed to safeguard the Permit Holders' Duty of Care responsibilities.

8.10 Contingency

Acceptance of waste into the site will operate in this order:

· The site will not accept more waste than it can process effectively at any one time and not above the permitted tonnage per annum or storage capacities stated in Section 8.8.

· In the event that the site reaches its maximum capacity, the Site Manager will divert any further incoming waste from the site to neighbouring facilities that are able to process the same types of waste.  This will continue until such a time as the site can resume operations within its normal operating capacity.

· Receipt of feedstock materials shall not recommence until a full review of this Management Plan has been conducted and process controls amended as required.
8.11 Records

Records for wastes received and dispatched at the site are kept securely in the Site Office.

The company will maintain a register of waste facilities to which it dispatches wastes along with copies of their environmental permits and EWC codes permitted at the facility (MPP2 Table 3).
9 POLLUTION CONTROL, AMENITY MANAGEMENT, MONITORING AND REPORTING SYSTEMS

9.1 Pollution Control and Amenity Management

9.1.1 General

9.1.1.1 Site Inspections

The Site Manager is responsible for carrying out site inspections on a twice daily basis.  These inspections provide a mechanism to assess whether site operations are being carried out in accordance with the EMS and that environmental management and control systems are operating within expected performance limits.  A record of site inspections is made on a Site Inspections Checklist (Form FR1), along with any remedial action required.

9.1.1.2 Monitoring and Sampling

Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator will inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place.  The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.

9.1.1.3 Site Emergency Plan

The company has an Accident/Pollution Incident Management Plan which forms part of its Environmental Management System (MPP4).  This complies with Natural Resources Wales’s requirements for a Site Emergency Plan.

9.1.1.4 Accidents and Incidents

The Accident/Pollution Incident Plan (MPP4) and Accident/Pollution Incident Response Procedures (Procedures PR1 – PR8) detail the approaches that should be followed in the event of an accident or pollution incident.  Any incident should be recorded on an Environmental Accident (and Incident) Record (Form FR10) and reported in accordance with Procedure PR13.

9.1.1.5 Environmental Risk Assessment

An Environmental Risk Assessment (Risk Assessment SRA1) has been undertaken for the facility and has informed the measures implemented in the following sections.  Although no specific areas of concern have been highlighted, the following general aspects of the facility have been taken into consideration in the preparation of this EMS Plan:

· Contamination of groundwater and surface water (spillage and fire). 
· Noise and vibration; and

· Release of fugitive emissions.
Due to the scale of the facility, nature of wastes received and operations, in combination with its distance from sensitive receptors, the likelihood of impact is assessed as medium to low without mitigation.  Infrastructure and/or management controls are in place to reduce these risks to low or very low.
9.1.1.6 Environmental Impacts and Controls
A register of Environmental Impacts and Controls can be found in MPP2.

9.1.2 Management of Environmental Risks

Risks are mitigated through the use of equipment or management techniques to reduce the risk of impact to an acceptable level.  These approaches are detailed in the following sections.
If notified by Natural Resources Wales that the activities are giving rise to pollution, the Operator will submit to Natural Resources Wales for approval within the period specified, additional management plans.  These plans will be implemented from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.

9.1.2.1 Surface Water and Groundwater Pollution
All site containment and drainage systems will be inspected at least weekly, throughout the operational life of the site for cracks, defects, and cleanliness, by appropriate site staff.  The results of each site inspection shall be recorded on the daily/weekly site checklists.  All maintenance and repair works will be carried out at the earliest opportunity and with due consideration given to the nature and scale of the issue. NRW shall be informed of all remedial works.
In the event that a fuel storage container is found to be leaking, arrangements will be made to have the contents transferred to an alternative container.  Liquids in any bunded storage area (fuel/oil and any contaminated water) will be removed by an appropriately registered waste management contractor.

The outside storage area will be checked daily as part of the daily site inspection.

The following control measures will be implemented to minimise potential impacts on surface and groundwater:

· Regular maintenance of operational areas such as drainage channels will be carried out.

· Containers and bunds will be inspected and maintained.
· Written management systems in place for the identification and minimisation risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances.
The Company spillage procedure (Procedure PR3) will be followed in the event of a spill (see 9.1.2.2 for details regarding the control and monitoring of Leaks and Spills).

9.1.2.2 Leaks and Spills

Accident/Pollution Incident Response Procedure – Spillage (Procedure PR3) will be followed in the event of a spill.
The following control measures will be implemented to minimise potential impacts from Leaks and Spills:

· Spill equipment will be available and site staff are responsible for and trained in its use.

· To minimise the risk of leaks and spills, the following operational procedures shall be implemented: 

· Only small quantities of red diesel for use in plant will be stored onsite.  Red diesel is stored in a bunded tank adjacent to the wash down area.
· All hydraulic, lubricating and waste oils will be stored in a lockable container, complete with a suitable spillage containment tray, which will collect any leaks from the drums.

· All drums and similar containers stored within the facility will have their contents and capacity clearly marked.

· To prevent spillages, drum openings will be carried out on a spillage tray.

· Absorbent granules are always to be kept on site for immediate use to soak up minor spillages.

· In the event of a major spill, immediate action will be taken to contain the spillage and prevent contamination of surface water run-off.  Once contained, the spillage will be treated with absorbent and removed to a sealed container for disposal at a licensed facility.  The stock of granules shall be replenished as soon as possible.

· A supply of lime or similar material will be maintained to neutralise any spillage of battery acid.

· Records shall be recorded in the site diary and a CAR raised (Form FR11) to show how the spillage occurred (if known), what the spillage was, and the remedial actions taken.

· Operational staff will receive pollution prevention and spill response training.

· Any spillages will result in a CAR (Form FR11) being raised to establish the root cause of the problem and if deemed necessary reviewed at quarterly business management meetings or sooner if there is a significant risk to the environment or operations of the business.

9.1.2.3 Fire Prevention and Control

Accident/Pollution Incident Response Procedure – Fire (Procedure PR2) and procedures described within the Site Emergency Plan should be followed in the event of a fire.
The following control measures will be implemented to prevent and/or minimise potential impacts from Fires:
· No material of any kind shall be burned within the boundaries of the site.

· Smoking is only permitted in the designated area outside of the entrance to the facility.

· A fire watch will be carried out as part of the routine end of day inspection.

· Suitable and adequate firefighting materials and equipment will be maintained and kept at appropriate locations on the site as advised by the local fire service.

· All site staff will be trained in the use of onsite firefighting equipment and all firefighting equipment will be replaced/refilled immediately after use.  Scheduled maintenance, inspection and overhauling of all firefighting equipment will be carried out on an annual basis.
· In the event of a fire the site will be evacuated and all non-essential personnel, including all members of the general public/visitors.  The appropriate emergency services will be called to attend to, or be informed of, any outbreak of fire.  Refer to Procedure PR2 for further detail.
9.1.2.4 Noise and Vibration

Site noise is only likely to occur as a result of the movement of plant and vehicles on site or during use of recycling equipment.  The crushing bucket is likely to be have the greater magnitude source emission levels for noise.
All vehicles and plant used at the facility will be of a roadworthy type and to the Construction and Use Transport Regulations in respect of engine noise and emissions and exhaust silencers.  They will be well-maintained and serviced at regular intervals as recommended by the manufacturer.

An auditory inspection shall be carried out by the site manager at least twice per day.  Noise levels which are considered higher than usual shall be investigated and recorded in the site diary.  Activities will be reduced or stopped until operations are able to commence without elevated noise levels.

The following measures will be taken to minimise the risk of noise and vibration:

· Tipping/processing of waste will only take place during the hours shown in section 8.2;

· Trafficked surfaces will be kept in a reasonable condition such that potential noise from vehicles is minimised.
· All plant machinery will subject to regular inspection and maintenance.
· Installed noise reducing equipment (acoustic panels, silencers, etc.) shall be used and maintained.
· Equipment shall be switched off when not in use; and
· Processing operations shall be arranged in such a way as to minimise noise production as far as possible.
9.1.2.5 Odours
Accident/Pollution Incident Response Procedure – Odour (Procedure PR6) should be followed in the event of an odour release.
The majority of wastes received at site are C&D wastes and not usually associated with significant risk of odour (unless contaminated).  
The following measures will be taken to minimise the risk of impacts from odours:

· Source segregation of most wastes to allow odorous/putrescible waste to be identified and appropriately managed before being reaching site.
· The site will not accept animal by-products or food waste that could cause odour.
· Odour checks during waste acceptance and tipping.
· Storage of food waste in a sealed container within the WTS building and removal from site within 72 hours.
· Twice daily site inspections and olfactory checks.
· Waste storage and processing within a building to contain odours.
· Adequate ventilation used to disperse low-level odour.
· Staff informed of importance of maintaining cleanliness of welfare area during induction training; and
· General measures taken to reduce odour: good housekeeping, regular disposal of waste, etc.
9.1.2.6 Dusts, Fibres and Particulates
EMS Procedure PR7 details the procedure and should be followed in the event of air emissions from site.
Due to the nature of the treatment processes employed on-site there is potential for dust to be generated, albeit due to these treatment processes being undertaken in enclosures of buildings under normal operating conditions dust is unlikely to cause nuisance to nearby receptors.
Operations that may give rise to dust are:

· Waste receipt and stockpiling.
· The on-site transfer of materials between the processing and the stockpiling/storage areas.
· Processing operations such as sorting.
· The loading of processed materials onto transport vehicles.
· Where appropriate the sweeping of roads where there have been deposits observed.

The following measures will be taken to minimise the risk of dust release:

· Source segregation of most wastes to allow potentially dust-generating waste to be identified and appropriately managed before being reaching site.
· Waste shall be sheeted and secured during transport.
· Vehicle speed shall be limited; and
· Visual dust monitoring shall be undertaken at least twice per day (and records of such recorded on the site inspection form) and generally on an ongoing basis by Site Operatives during processing.
Where airborne material is observed, this will be recorded, and corrective/preventive action taken.  Action will include:

· The use of dust suppression comprising of a hose spray within the yard area. 

· Sweeping of the site to remove dust or mud; and
· Cessation of processing until the cause of excessive dust generation has been identified and addressed.
Records of such will be recorded within the site diary/inspection form and if necessary, raised as a CAR (Form FR11).
If notified by Natural Resources Wales that the activities are giving rise to nuisance dust outside the site, the Operator will submit to Natural Resources Wales for approval within the period specified, a dust management plan.  This plan will be implemented from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.

9.1.2.7 Pests

Animal by-products and food waste will not be accepted at the facility.

The permitted wastes may attract vermin and scavengers, notably to food waste within the small quantities of mixed waste received onsite or quarantined as contamination from incoming waste.  The most likely pest to be attracted by the waste are fly species, rodents, and carnivores (foxes, etc.).
The following measures will be taken to minimise the risk of pests:

· Source segregation of most wastes to allow food waste to be identified and appropriately managed before being reaching site.
· Waste inspected before tipping to identify potential contaminants.
· Quarantine non-conforming putrescible wastes in a sealed container and removal off-site within 72 hours.
· Visual monitoring for pests, vermin performed daily including inspections for evidence of droppings, damage to property/plant or ground disturbance e.g. burrow, nests, and excessive infestation present; and
· Good housekeeping and regular inspection of mess facilities.
In the event of a pest infestation being detected the following measures will be implemented:

· Suitable treatment will be implemented either by employees or by suitable contractors, this may involve the application of insecticides or growth inhibitors, the setting of traps and poisons, or other measures as appropriate.
· Any waste identified as attracting scavengers shall be isolated and removed from site.
Details of any pest control activities will be recorded during the site inspection and if necessary, raised as a CAR (Form FR11).

9.1.2.8 Litter

As the general site operations are principally contained within the waste transfer building, the potential for windblown litter from site is minimal.

A daily record of litter inspection is logged on the Site Inspection Record (Form FR1) and during the working day, site supervisors will be alerted to incidents of litter on site.

Any evidence of litter will be attended to by hand clearance.  The litter collected will be deposited in the relevant container, either for recycling or disposal.

The following measures will be taken to minimise the risk of litter:

· All wastes shall be sheeted and secured during transport.
· Light fractions to be stored correctly; and
· Site fencing to be maintained as an effective barrier to litter being blown offsite.
In the event of litter being detected during the daily inspection the following measures will be implemented:

· Any litter that is blown into adjoining parts of the site will be collected at no greater than daily intervals.
· Any litter that is blown outside of the site boundary will be collected no later than 1 hour after the end of the working day.

9.1.2.9 Mud and Debris

The site is largely laid to concrete or asphalt.  This results in limited opportunity for mud generation.  
Daily and ongoing inspections of site movements and the adjacent highway will ensure that any mud or debris caused by the site operations is cleansed manually as soon as the mud or debris is detected.

If during extensive adverse weather conditions, the surfaced areas are seen to be deteriorating in standard of cleanliness, mechanical sweeping and cleansing will be implemented.

9.1.2.10 Other Fugitive Emissions

Due to the nature of operations other fugitive emissions have been risk assessed and it determined that emissions are below threshold levels.  The contribution to local Air Quality levels via onsite exhaust emissions is negligible and insignificant compared to emissions from nearby highways.  The facility will however ensure that it is not a generator of significant additional emissions.

The following measures will be taken to control other fugitive emissions:

· All plant machinery will subject to regular inspection and maintenance.
· Good fuel tank and transfer pipework design.
· Vehicles shall be compliant with relevant exhaust emissions standards; and
· All plant machinery will subject to regular inspection and maintenance.

9.1.2.11 Utility Failure
Procedure PR5 describes what to do in the event of services (water, electricity, gas, or sewerage system) supply failure.

Steps to be taken include the manual shut down of equipment, start-up of emergency generators, use of standby materials, etc.
9.1.2.12 Flooding
EMS Procedure PR4 details the procedure and should be followed in the event of a flood.

Localised flooding of the site from rivers and coastal water is NOT an identified risk for the site.  Any flood risk results solely from surface water inundation in the event of localised flooding resulting from blockages of drains, fire water run-off, etc.

In the event of a flood the permitted waste types that may be washed off site would add to the volume of the post-flood clean-up workload, rather than the hazard.

In the event of flooding (or of the potential for flooding) of the site, the following steps would be taken (only where safe to do so):

· Wastes, liquids, and other materials with potential to be washed from the site shall be removed from site (or relocated within the site to areas less likely to be affected by floodwater).
· The boundaries of the site will be bunded/have bunding reinforced using appropriate materials in order to retain waste materials within the site and/or impede the flow of floodwater into the site; and

· Where any risk of contaminated water discharging from site as flood waters recede is identified, actions required to retain and manage flood water within the site will be identified and actioned in agreement with Natural Resources Wales and the Emergency Services.

9.2 Monitoring

No formal monitoring is required under the existing Permit conditions.
9.3 Reporting

9.3.1 Periodic Reporting of Environmental Performance

A quarterly summary will be submitted to NRW in a form to comply with requirements.

A copy of the waste classification (EWC) will be held on site for reference.

9.3.2 Notifications

The following information will be submitted to Natural Resources Wales:

1. Natural Resources Wales shall be notified without delay following the detection of:
a. any malfunction, breakdown or failure of equipment or techniques, accident or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution.
b. the breach of a limit specified in these standard rules; or
c. any significant adverse environmental effects.
2. Written confirmation of actual or potential pollution incidents and breaches of emission limits shall be submitted within 24 hours.
3. Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.

4. Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters except where such disclosure is prohibited by Stock Exchange rules:
(a) Where the operator is a registered company:

· any change in the operator's trading name, registered name, or registered office address; and

· any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement, or being wound up.

(b) Where the operator is a corporate body other than a registered company:

· any change in the operator's name or address; and

· any steps taken with a view to the dissolution of the operator.

(c) In any other case:

· the death of any of the named operators (where the operator consists of more than one named individual).
· any change in the operator’s name(s) or address(es); and

· any steps taken with a view to the operator, or any one of them, going into bankruptcy, entering into a composition or arrangement with creditors, or, in the case them being in a partnership, dissolving the partnership.

5. Other notifications (not specified in permit)

· Breach of operating procedures (within 3 days).
· A change of TCM (7 days).
· A conviction and/or an appeal (14 days).
· Financial changes affecting the site operations with regard the conditions within the permit (14 days); and

· Activity commencement and/or changes (7 days). 

9.3.3 Interpretation

As per the meanings described within the permit.

9.4 Complaints

The company’s complaints procedure (Procedure PR14) applies to all complaints, feedback and requests made by third parties regarding operational activities.

Complaints are to be investigated immediately by the Site Manager.  The nature and details of the complaint will be logged on a complaints record form (Form FR2), along with the findings of the investigations and any action required.  Odour complaints are logged on an External Odour Complaints Investigation Record (Form FR3), with an Internal Odour Investigation Record (Form FR4) being completed during investigation of the incident.
The Site Manager is responsible for determining the appropriate action to be taken and will communicate the nature of the actions to be taken and timescales to the Complainant.

All complaints from third parties including external customers, potential customers, statutory authorities, statutory consultees, members of the general public and internal clients will be forwarded to the Site Manager to action as below.

The Site Manager will ensure that:

· All complaints are logged.
· The complaint is investigated to identify the cause.  If a complaint is relayed to the company by a 3rd party (e.g. Natural Resources Wales), this may require direct communication with the complainant in order for the complaint to be effectively investigated.
· Necessary preventative action is taken to both address the cause of the complaint and that measures are implemented to prevent a reoccurrence of the same problem.  These actions must be documented, and a CAR (Form FR11) raised as required.
· The Complainant will be contacted and given information on the investigations conducted and actions taken as appropriate.
· Where a complaint or query is likely to involve a statutory authority, the emergency services, an insurance company, or the media, the Managing Director will be informed.
· Complaints linked to contracts with specific complaints procedures will be reported in line with contractual requirements and timescales.  Local procedures may need to be in place to ensure these are adhered to.
· All complaints are discussed at site meetings and reviewed at monthly management meetings; and

· If the investigation indicates that the complaint has not been justified this will be clearly recorded on the Incident Report.

In the event of a complaint being verified as resulting from the operation of the facility the Site Manager is responsible for identifying short and long-term mitigation measures to minimise the risk of future incidents.  The efficacy of any mitigation measures will be confirmed through further monitoring at the receptor (subject to the Complainant’s agreement) or at a representative position along the site boundary.

Complaints logs, in combination with meteorological data and site monitoring information will be used to assess any trends.
10 SITE RECORDS
10.1 General
All records required to be made by the environmental permit shall:

a) be legible.
b) be made as soon as reasonably practicable.
c) if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and

d) be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made, or in the case of the following records until permit surrender:

(i) off-site environmental effects; and
(ii) matters which affect the condition of the land and groundwater.
10.2 Security and Availability of Records

Most documents are securely stored electronically, with paper copies also available where required. 
Access to the statutory documents and records are made available to any authorised NRW Officer.

Details of documentation and security arrangements are considered to be confidential but can be a matter of discussion with an authorised NRW Officer.

All wastes delivered to the facility will be quantified or weighed and a ticket shall be issued to the customer (or on the rare occasion when waste is brought to site) or vehicle transporting the material, with a copy of the ticket filed at the site office.

NRW will be provided with a summary of types of quantities of wastes received at the site.  These records will be relayed to NRW in an agreed format and at an agreed frequency.  The site diary will be stored in the office which is locked outside of office hours.  The diary will be used to record site activity and any unusual events.  The diary will be made readily available for inspection by any NRW Officer at any reasonable time.  

A record of site visitors will be kept including.
· Name (including signature) and company/organisation

· Car Registration

· Person to See
· Time of arrival and departure

The time (when necessary) and the date of the following events shall also be recorded in the site diary:
· Start and finish of any construction/engineering works within the site boundary.
· Start and finish of any management processes carried out on site.
· All maintenance.
· Breakdowns.
· Emergencies and environmental incidents and remedial actions taken.
· Problems with waste received and action taken.
· Evidence of all waste entering and leaving the site; where from, date, time, quantity/weight.
· Site inspections - who carried out the site inspection, date, and time, why and the consequent actions carried out by the operator.
· Attendance of technically competent management on site and the date and time of departure of the technically competent manager.
· Despatch of records to NRW.
· Extreme weather conditions; and

· Complaints and actions taken.

DRAWINGS AND PLANS

Refer to MPP5 for current Site Drawings and Plans

DEFINITIONS
Disclaimer


Every skill and care have been taken in completing this work within the terms of the contract commissioning our services and taking into account the resources assigned to the commission in agreement with the client.  Similarly, every skill and care has been taken to ensure the accuracy of the information within this document.  No liability or responsibility of any kind to the client or 3rd parties can be accepted by Technia Environment and Planning Ltd for any matters outside of the stated scope.  The opinions and interpretations presented in this document represent our reasonable interpretation of the data made available to us.  Drawings and descriptions within this document are not intended to represent detailed design unless otherwise stated and should not be used for construction.








� “Annex II” means Annex II to Directive 2008/98/EC of the European Parliament and of the Council on waste


� “specified waste” means the following waste codes in � REF _Ref462295466 \h � \* MERGEFORMAT �Table 3�: 01 01 01, 01 01 02, 01 04 08, 01 04 09, 01 04 13, 02 04 01, 10 11 12, 10 12 08, 10 13 14, 15 01 07, 17 01 01, 17 01 02, 17 01 03, 17 01 07, 17 02 02, 17 03 02, 17 05 04, 17 05 08, 19 12 05, 19 12 09 and 20 02 02.


� “building” means a construction that has the objective of providing sheltering cover and minimising emissions of noise, particulate matter, odour and litter.


� “impermeable surface” means a surface or pavement constructed and maintained to a standard sufficient to prevent the transmission of liquids beyond the pavement surface, and should be read in conjunction with the term “sealed drainage system”


� “sealed drainage system” in relation to an impermeable surface, means a drainage system with impermeable components which does not leak and which will ensure that, (a) no liquid will run off the surface otherwise than via the system and (b) except where they may lawfully be discharged to foul sewer, all liquids entering the system are collected in a sealed sump.






