
Grays Waste Management Ltd

Site Working Plan for Site Plot 6, Ecoparc Mon,

Mona Industrial Park

 SEQ CHAPTER \h \r 1CONTENTS:





    


      Page No.
1.0
GENERAL CONSIDERATIONS
1.1
Site operator/licence holder




3


1.2
Site history and planning status



4


1.3
Licence area/waste management operations


4

1.4
Hours of operation





5


1.5
Waste types and quantities




5


1.6
Staffing and management




7


1.7
Health and safety





7


1.8
Fit and proper persons





7

2.0
SITE ENGINEERING AND INFRASTRUCTURE 

2.1
Access and parking





8

2.2
Notice board and signs




8


2.3
Site security






8


2.4
Site office 






9


2.5
Weighbridge






9

2.6
Wheel cleaning facilities




9

2.7
Fuel storage






10


2.8
Waste transfer and storage areas



10

2.9
Drainage






11


2.10
Vehicles, plant and equipment



11

3.0
SITE OPERATIONS

3.1 
Preliminary procedures




12

3.2
Checking in & inspection of loads 



13


3.3
Waste deposit, handling and storage 



14

3.4
Record keeping





15


4.0
ENVIRONMENTAL CONTROL, MONITORING AND REPORTING


4.1
Breakdowns and spillages




16


4.2
Site inspections and maintenance
 


16


4.3
Control of mud and debris




17


4.4
Control and monitoring of dust



17

4.5
Odour control






18

4.6
Litter control 






18

4.7
Control of pests, birds and other scavengers


18

4.8
Control and monitoring of noise



18

Appendices:

Appendix I - Drawings:


Drawing No. 2664/819/01
Site Location Map @ 1:25,000 scale
  


Drawing No. 2664/819/02 
Site Location Plan (application boundary)
  

Drawing No. 2664/819/03 - 
Site layout Plan



Drawing No. 2664/819/04
Construction Details (Process Building)
Appendix II - Record Keeping Forms


Waste Inputs –P&L Report: Weighbridge Transaction Audit Report (WTAR) 

Rejected Waste – P&L Report: Rejected Load/Waste Report

Waste Output Record Form – Contained within WTAR, but also covered within Excel 

Report “Tonnages Out (by year)” 
Site Inspection Form: AEMRR/RF/4

Visitors log/complaints record – Peninsula GWM Visitors Record Book
Technical competence record: GWM TCR
Appendix III - Waste types (EWC listing)
Appendix IV - Health and Safety - Conditions of site use for staff and visitors
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Appendix VI - Permissions & exemptions
Note: 
Appendices IV and VI are attached to this working plan for information only. 

All other appendices form part of this working plan and are subject to conditions in the waste management licence for the site.
1.0
GENERAL CONSIDERATIONS
1.1
Site operator/licence holder


1.1.1
Grays Waste Management Ltd will hold the waste management licence for the recycling centre.  The site will receive the majority of its waste inputs from in-house operations and a limited number of other carriers from the Anglesey and Gwynedd area.

1.1.2
Recent developments in legislation such as the annual increases of landfill tax have increased the effectiveness and scope of operations for waste transfer and recycling centres, permitting greater recovery rates for recyclable waste from households, commerce and industry. The recycling centre will allow the further sorting and storage of non-hazardous inert, metal, degradable household, degradable commercial and degradable industrial wastes to permit the recycling, recovery or re-use of waste primarily sourced from commercial and industrial premises.
1.1.3
The company is currently administered from the address below 


Grays Waste Management Ltd


Ecoparc Môn



Tel:
01407 720285


Mona Industrial Park


Fax:
01407 721976


Gwalchmai


Anglesey


LL65 4RJ

1.1.4
This working plan has been prepared to meet the requirements of Waste Management Paper No.4 - Licensing of Waste Management Facilities. The document provides information to Natural Resources Wales to enable it to set licence conditions and gives instructions to staff specifying how the site is managed.
1.2
Site history and planning status


1.2.1
The site is located on Mona Industrial Park, Mona, Anglesey [NGR. SJ.418.757].  The surrounding land uses are industrial, and land to the North and West of the site is used by the  Royal Air Force for pilot training.  

1.2.2
This site has been operating as a recycling centre since 2003, and has recently (June – Oct 2013) had buildings constructed for use as a transfer station and as a vehicle maintenance facility.  A change of use application for the operation of the site as a recycling centre and was granted by Anglesey County Council on 28/08/2002 (App. Reference No. 14C28K) and a copy of the planning consent is attached to this document as Appendix VI.

Since then, Grays Waste Management Ltd (GWM) has sort and secured planning consent to build new buildings on the site and to develop more undercover processing space (14C281/E - 12th February 2013). Subsequently, GWM sought consent to handle putrescible wastes and enlarge the process building. Consent was granted (14C28F/1 – 7th July 2013). 

1.3
Licence area/waste management operations

1.3.1 
The area which is the subject of the waste management licence is outlined in red on Drawing No. GWM/01.   All references to ‘the site’ in this working plan shall mean this area (the recycling centre) and the associated infrastructure, plant and equipment. 


This site is operated in conjunction with the License Holder’s other site, which lies on the opposite (Eastern) side of the main Industrial Park service road. This other site occupies 5 acres of what was known as Plot 8+, Mona Industrial Park and is managed by GWM under permit number EPR/DB3830AQ.  is used for the storage of materials processed on this site and for the storage of empty skips, bins, plant, machinery and vehicles. This area was enlarged in a variation determined on 28th November 2011 (Reference EPR/DB3830AQ/V002)

1.3.2
The waste management licence is required for the storage (keeping) prior to removal, and treatment (all types of handling/processing) of waste. Waste treatment processes carried out on site may include the following:


Compacting (by loading shovel/telehandler)

Sorting (with loading shovel, 3600 machine or by hand)

Screening using a vibrating screen or trommel screen

Crushing/shredding - using mobile plant (not subject to licence conditions ie: Part B authorisation).
1.3.3
Specified waste management operations include waste disposal and waste recovery operations listed in Parts II and III of Schedule 4 of the Waste Management Licensing Regulations 1994 (as amended).  They are listed in summary below:

D15:
Storage of waste pending disposal.

D9: 
Physico-chemical treatment of waste

R2:
Recycling or reclamation of organic substances

R3:
Recycling or reclamation of metals

R4:
Recycling or reclamation of other inorganic materials

R13:
Storage of waste pending recovery
1.4
Hours of operation
1.4.1
The site will be operated during the following hours for all waste operations, i.e. deposit, sorting, moving, storing and removing waste:


Monday to Friday 

0700 to 1900


Saturday


0700 to 1600

Sunday 


0700 to 1600

Bank Holidays

0700 to 1600

24 hour access is required for the haulage operation (excluding haulage of waste).
The offices will be manned and the site open to customers during the following hours:


Monday to Friday 

0800 to 1600


Saturday


Closed 
Sunday 


Closed
Bank Holidays

Closed
1.4.2
Floodlights are installed in the waste transfer building for use if necessary operations or emergency procedures are carried out after official lighting up times 
1.5
Waste types and quantities

1.5.1
The waste types accepted at the site will be non-hazardous inert, metal, degradable household, degradable commercial and degradable industrial wastes as defined in The Controlled Waste (England and Wales) Regulations 2012 and Section 75 of the Environmental Protection Act 1990 (Q WEEE REGS). 

1.5.2
A detailed breakdown of the waste types from the European Waste Catalogue is attached to this working plan as Appendix III.  The breakdown is not exhaustive and other wastes which have not been listed but which fall within the category described in 1.5.1 above will be accepted with the written agreement of Natural Resources Wales.  No clinical, special or liquid wastes will be accepted.
1.5.3
A maximum of 75 loads of waste will be deposited at the site in any full working day with restrictions of a maximum of 50 loads on a Saturday, Sunday or Bank Holiday. Such loads will be delivered to the site contained within skips, containers, fixed body vehicles, on flat bed trailers or multilift vehicles.The site is also open to licensed waste carriers for the disposal of waste and recyclables. To this end it is anticipated that the site will receive vans and trailers from local businesses seeking an outlet for their waste.  

Traffic levels arising from the site will be as follows:

i
75 incoming  loads of waste in any full working day (150 movements).

ii
15-20 outgoing HGV loads carrying recycled product/ waste to landfill (40 movements).

iii
15 HGVs engaged in the haulage operation (30 movements).

iv
The estimated peak hourly use is 20 HGV vehicles (40 movements).
1.5.4
The throughput of the site will be limited to a maximum of 500 tonnes per day and <25,000 tonnes per annum.  Notwithstanding the daily limit the following limits will apply to other waste types:

Waste type


Daily maximum input
Inert



500 tonnes


Scrap metal


50 tonnes


Special



Not accepted


Degradable household 
200 tonnes


Degradable commercial 
200 tonnes





Degradable industrial 

300 tonnes
1.5.5
The maximum amount of waste (authorised by the waste management licence) to be stored on site at any time will be 150 tonnes.    

Waste type



Max duration 


Maximum quantity 

of storage 


stored


Mixed waste (inc putrescible)

10 working days

108 tonnes

Inert waste 



31 days


100 tonnes 

Rejected waste 


48 hours


< 8 tonnes

The above storage periods will only be varied with the agreement of the Environment Agency.  The above figures exclude storage of recycled product and sorted waste to be submitted to exempt recycling operations. 

1.5.6
If more than 8 tonnes of waste is rejected it will be removed from the site immediately.  Stockpile heights will be limited to the height of the waste transfer bays.
1.5.7
If the maximum storage capacity of the site is reached then no further waste will be accepted until waste can be removed from the site and taken to a suitably licensed or exempt site.

1.5.8
Strict requirements will apply to certain types of wastes i.e.

i. 
Empty used containers which have contained chemicals or special waste must be cleaned or certified as clean before they will be accepted.  Paint tins or other containers will be accepted if they have residues in as long as those residues are solid and non-special.  Any containers found within mixed loads which do not meet the above criteria will be stored within a bund and disposed of in accordance with the relevant regulations. 
ii. 
Potentially dusty loads or loads containing powder have to be notified in advance to ensure that suitable plant and equipment is available to reduce dust emissions.  Some powdered waste will have to be bagged prior to receipt to prevent a dust problem.  No whole loads of powdered waste will be accepted. 

iii. 
Shot blasting residue will only be accepted from known sources or where the contents of the residue can easily be identified.  Residues containing tributyl tin will not be accepted. 

iv. 
Tyres will not be accepted - any discovered within mixed loads will be consigned stored for submission to a recycling operation.

1.6
Staffing and management

1.6.1
The site will open for the deposit of waste or for other essential operations during the hours listed in Section 1.4 above.  The list below details the staff structure of the site when operating at full capacity.  Positions in bold italic print below are the minimum staff requirements when the site is open for the reception of waste: 

Position



No.
Responsibilities
Site Manager



1
Overall site management


Machine/plant operator

1 (2)
Waste handling, reception and plant operation


General operatives


1 (2)
Sorting & screening waste, maintenance and tidying the site
1.7
Health and safety

1.7.1
All operations on site will be carried out in accordance with the relevant requirements of the Health and Safety at Work Act 1974.  Conditions of site use for employees, visitors and contractors are attached to this working plan as Appendix IV. These conditions will be shown to all site users and must be signed prior to using the site.  Anyone not complying with the conditions of use will be asked to leave the site.
1.8
Fit and proper persons


1.8.1
Technical competence – Trefor Jones holds the WAMITAB (Waste Management Industry Training and Advisory Board) COTC (Certificate of Technical Competence) Level TSB-4 (managing transfer operations - biodegradable waste).  He is the technically competent manager at the site. Matthew Davis and Gibb Williams are also WAMITAB holders and will assist Trefor Jones.
1.8.2
Relevant convictions - on the date of the application neither the directors nor any employees of Grays Waste Management Ltd have been convicted of a relevant offence.
2.0
SITE ENGINEERING AND INFRASTRUCTURE 
2.1
Access and parking
2.1.1
The main access route to the Mona Industrial Park is from the A5 Llangefni - Holyhead road.  The entrance to the site is situated off the industrial estate road  shown on Drawing No. 2664/819/03.  The site entrance is concreted and adjoining road is constructed from tarmacadam.

2.1.2
Parking will be available for 11 heavy goods vehicles, 3 trailers and 16 cars at the locations shown on Drawing No. 2664/819/03
2.2
Notice board and signs

2.2.1
A notice board measuring approximately 1 metre square has been erected on the fencing at the entrance to the site and will display the following information:


-
The site name and address.


- 
The name of the licence holder.


- 
The waste management licence number and accompanying statement stating that the site is licenced by Natural Resources Wales.


- 
Natural Resources Wales contact details. Emergency No. 0800 807060 and 



General enquires No. 0845 933 3111.


- 
Operators “out of hours” emergency contact details

- 
Operating hours.
2.2.2
Additional signs may be displayed around the site for operational/health and safety purposes.  All staff and visitors will be required to comply with the requirements of all signs whilst on site.
2.3
Site security


2.3.1
Gates - The main entrance gates will be located as shown on Drawing No.2664/819/03 and will be of steel frame construction, covered with steel panels and reinforced with steel cross-braces.  The gates remain padlocked when the site is unmanned. 

2.3.2
Fencing - the site will be surrounded by galvanised palisade fencing to the height of 2.4 metres.
2.4
Site office

2.4.1
The office/weighbridge buildings will be cladded and steel portal frame units, located as shown on Drawing No. 2664/819/03.  Toilets, washing and canteen facilities will be provided for site staff in the mess room area as identified.
The telephone/facsimile numbers for the recycling centre are the numbers listed in Section 1.1.3 above.

2.4.2
The table below details the relevant site documentation which is located in the 


offices on site.

	Documents to be retained in the site office

	Waste management licence (original)

	The working plan (agreed document)

	Current site diary 

(to record all inspections/visitors to the site). 

	Natural Resources Wales inspection forms

	In-house inspection sheets/recording forms

	Duty of care transfer notes (for 2 years minimum)

	Special waste consignment notes

(for rejected loads, kept for 3 years)

	Waste delivery tickets

	Weighbridge tickets

	Accident book (& 1st aid kit)


2.5
Weighbridge








2.5.1
A weighbridge is installed at the location shown on Drawing No. 2664/819/03
2.6
Wheel cleaning facilities



2.6.1
No wheel cleaning facilities are proposed at the site.   The waste types handled on site and the fact that the main vehicle running surfaces are hard surfaced reduces the likelihood of mud or debris being carried onto the industrial estate roads.  The public highway is also a considerable distance from the site.  

2.6.2
Procedures are also in place to ensure that mud and debris are not tracked onto the industrial estate road and the public highway (refer to section 4.3).
2.7
Fuel storage

2.7.1
Any fuel or oil stored on site will be surrounded by a bund which is capable of containing a minimum of 110% of the volume of fuel stored.

 2.8
Waste transfer and storage areas
2.8.1
The waste transfer area is contained within the main process building (as shown in drawing 2664/819/04.  The floor space of the process building is surfaced with reinforced concrete of sufficient strength for the tipping of loads, storage of waste and running loading plant.  The floor is laid to a fall of 1:200 (minimum) and will drain to the foul sewer via a Class II by-pass separator.  The layout of the site is shown on Drawing No. 2664/819/03.
  2.8.2
The floors of the bays are surfaced with concrete of sufficient strength for the tipping of loads, storage of waste and running of plant and machinery. The minimum specification for the concrete is shown below:


Concrete specification:
Mix: C40 (minimum 35% cement)



  Depth: 
Minimum 150 mm, fibre or mesh reinforced
2.8.3
All mixed waste loads will be deposited in the waste transfer station to permit effective sorting of waste and storage prior to the removal off site to a suitably licenced or exempt site or to other bays located on site.  The bays are constructed from concrete or railway sleepers set in vertical steel stanchions to a height of 1 - 3 metres.
2.8.4
Area for the deposit of rejected wastes - a clearly labelled enclosed skip with a capacity of between 4 and 8 cubic yards or similar will be provided for the deposit of rejected waste which cannot be removed from the site immediately. The location of this skip will be within the waste transfer station.
2.9
Drainage







2.9.1
Surface water control - all surface water from outside the transfer bays will drain to the surface water system via a Class II by-pass separator.  The layout of the site is shown on Drawing No. 2664/819/03.

Drainage falls and channels are also shown on Drawing No. 2664/819/03 

2.10
Vehicles, plant and equipment



2.10.1
Waste will be handled using the plant listed below.  Additional plant will be hired to cover any very busy periods. Only trained operators will be permitted to drive/operate the plant listed below.   Any changes to the list will be notified to Natural Resources Wales prior to implementation (minimum level of plant highlighted in italics).

Type of plant/equipment*
No.
Function

Loading shovel/JCB


1
waste loading/unloading/movement


3600 excavator – grab/bucket
1
waste loading/unloading/movement


Skid steer – bucket/grab/brush
1
waste movement/cleaning

3.0
SITE OPERATIONS
3.1 
Preliminary procedures
3.1.1
Guidance will be given by the site management (operator and licence holder) to all employees, sub-contractors, other waste carriers and customers regarding the waste types which are acceptable at the site i.e. a copy of the short waste list from Appendix III of this document.    The site will be primarily used for the receipt of waste from Grays Waste Management Ltd’s own operations.  Where waste is brought in under sub-contract or is delivered by other hauliers, then the carrier registration details will be taken for all new haulage operators bringing waste to the site and the details will be periodically checked with Natural Resources Wales to ensure that they are still registered. The procedures below are followed prior to the receipt of waste on site.

3.1.2
When a driver employed by the licence holder/operator arrives at the customers site to pick up a consignment of waste he will inspect the load for conformity with relevant regulations and safety procedures.  

i.
If the load is satisfactory the driver will sign the relevant paperwork (Duty of Care transfer note/skip ticket) and remove the load from the customer’s premises.
ii.
If the waste does not meet the description stated on the controlled waste transfer note the customer will be advised to check the note and give a more detailed description of the waste. 
iii.
If the more detailed description of the waste reveals that the waste is not permitted at the recycling centre then the customer will be advised that the waste must be taken to a suitably licenced site.
iv.
The driver may also report back to the site manager for instructions.
3.2
Checking in & inspection of loads
3.2.1 
All incoming vehicles are required to report to the weighbridge office.  The details of the load will be recorded and the duty of care note/company documentation will be further checked by the operator to ensure that the load is acceptable at the recycling centre.  Any deviation from the procedures or problems with any loads will be reported to the site manager. 
3.2.2
Once a load has been provisionally accepted the driver will be asked to un-sheet the vehicle (if it is sheeted) and a visual inspection of the contents will be carried out to ensure that the waste types comply with the waste management licence.  The nature of mixed waste makes full inspection difficult until the load is deposited.  If rejected waste is discovered before deposit the load will be rejected by the operator and returned to the producer.  In cases where the presence of unauthorised waste is likely to lead to a breach of licence conditions Natural Resources Wales will be contacted.

3.2.3
If the load is acceptable the driver will be instructed to deposit it within the designated area for storage or processing, as shown on Drawing No. 2664/819/03.  If the load is unacceptable after deposit it will be loaded back onto the delivery vehicle and returned to the producer.

3.2.4
The weight of incoming loads will be measured using the weighbridge
3.3
Waste deposit, handling and storage 
3.3.1
Once a load has been accepted by the operator the contents of the delivery vehicles will be discharged in the transfer bays, subject to the following procedures:

i. 
Wholly inert loads will be tipped in the topsoil/rubble storage areas, under the supervision of the operator. If any contamination is discovered, this will be removed immediately by the operator.
ii. 
Where the visual inspection reveals a load is not made up wholly of inert waste, these will be tipped into the bays in the transfer station for sorting prior to storage or removal off site, to a suitably licenced or exempt location.
iii. 
Loads containing mixed wastes will be deposited in the bays and will be crudely sorted using the loading shovel or skid steer. 




iv. 
Operatives will manually sort recyclable waste such as cardboard, plastics and metals for recycling.  Wood will be removed and deposited in the timber skip stored between the workshop building and the process building 
v. 
Waste which is not suitable for recycling will be stored within the transfer station prior to removal off site.
vi. 
Tyres which are found in loads will be stored in a skip prior to removal off site by a suitably licensed operator
vii. 
A maximum of 15 full sheeted skips will be stored prior to tipping.
3.3.2
Rejected wastes will be deposited in the skip provided for non conforming wastes located in the waste transfer station.  This will occur when non conforming waste is discovered after the deposit of a load and the producer of the load cannot be contacted (or identified) or where the removal off-site of the waste may cause further problems.  Natural Resources Wales will then be contacted to agree a course of action where necessary.  The contents of the skip will be recorded in the site diary and no wastes will be placed in the skip which are likely to react with other wastes.

3.3.3
The weight of loads will be calculated by the calibrated weighbridge.   The actual weight of waste deposited at the site may also be verified when loads removed from the site are weighed at the destination landfill or recycling centre. 

3.3.4
When a collection vehicle arrives at the site the driver will be instructed to report to the weighbridge office.  All relevant documentation will be completed and the vehicle will be passed to pick up the load and take it to the designated recycler/disposal site.  The product or waste will be loaded using the loading shovel or 3600 machine.

3.4
Record keeping
3.4.1
The details below will be recorded on a combination of the record keeping forms listed in Appendix II, invoices, weighbridge tickets,  the site diary and controlled waste transfer notes (where required). The records will be stored using P&L software on a server at the site (with a secondary back-up server) There will also be paper copies kept.

3.4.2
The following details will be recorded for every load deposited at the site (P&L Weighbridge Transaction Audit Report): 



(i)
The date and time of delivery.




(ii)
The name and address of the waste producer.




(iii)
The type and quantity of waste (in tonnes or cubic metres).



(iv)
The carrier's name and address

(v)
Driver’s name, signature and vehicle registration No.
(vi)
Signature or initials of person accepting/ inspecting the waste

(vii)
Additional handling details/notes made by the driver after inspection of the load

3.4.3
The following details will be recorded for all deposits of non conforming waste at the site and will be forwarded to Natural Resources Wales, where required (P&L Rejected Waste Report):


(i)
Date and time of deposit.



(ii)
A description of the waste.



(iii)
The quantity of waste (in tonnes or cubic metres).



(iv)
Name, address and telephone No. of waste producer. 



(v)
The carrier's name, registration number and vehicle registration.



(vi)
Reason for the rejection of waste and action taken.

3.4.4
The following details will be recorded for every load of waste leaving the site (P&L Weighbridge Transaction Audit Report):


(i)
The date and time of removal.



(ii)
The type and quantity of waste (in tonnes).



(iii)
The destination waste management site or exempt facility.



(iv)
The name and registration No. of the carrier or employee removing the waste (if applicable) and vehicle registration No.

3.4.5
A summary of waste types and quantities deposited at and removed from the site will be forwarded to Natural Resources Wales at intervals specified in the waste management licence for the site.  

3.4.6
The outcome of all inspections of waste types, hardstanding areas, push walls, drainage channels etc. will be recorded on site inspection form AEMRR/RF/4  and detailed comments regarding any construction, maintenance, breakdowns, emergencies and severe weather conditions will be entered into the  site diary (including action taken or proposed).

3.4.7
Visitors to the site will sign the visitor’s book upon arrival and exit stating the purpose of their visit and whom they represent.  

4.0
ENVIRONMENTAL CONTROL, MONITORING 

AND REPORTING





4.1
Breakdowns and spillages
4.1.1
In the event of a breakdown of the loading plant an alternative loading shovel/ 3600 machine will be used on site until it is repaired.  If an alternative machine cannot be used then waste will be securely stored until the plant is repaired.   The repair will be carried out at the most convenient location with absorbents used to clear oil or fuel spillages.  For major repairs the vehicle will be moved to a workshop until the repair is affected. 

4.1.2
All internal and external site surfaces will be inspected daily when the site is in operation.  Debris will be swept as required and placed in a skip for disposal.   

4.1.3.
Any spillages of fuel will be cleared immediately by depositing sand or absorbents on the affected area.  The sand or absorbents/spill kits will be placed in a skip to be taken to a suitably licensed site for disposal. All spillages of waste and windblown litter will be cleared by the end of the working day in which they occur.  Spillage clearance procedures are detailed in Appendix V below - Emergency procedures.  Sand and absorbents/spill kit are stored in the vehicle workshop.

4.1.4
All wastes liable to give rise to contamination will be removed from the site if the site is not secure or if operations cease or are temporarily suspended.
4.2
Site inspections and maintenance

4.2.1
The inspection frequencies for maintenance/housekeeping are listed on record form AEMRR/RF/4.  The inspection form will be completed by a person who is familiar with the requirements of the working plan and licence for the site.  All details of defects, problems and repairs carried out will be recorded on the form on the day that each event occurs. Detailed comments may also be recorded in the site diary.  All repairs will be carried out within 5 working days unless agreed otherwise with Natural Resources Wales.

4.2.2
All repairs to site security fencing will be made within 5 working days of the discovery of the damage and the site will be made secure until the repair has been affected.

4.2.3
Any major defects found during the daily site inspection which are likely to lead to a breach of licence conditions will be repaired by the end of the working day in which they are found where possible.  If a repair is not possible by the end of the working day Natural Resources Wales will be contacted to agree a suitable timescale for repair.

4.2.4
All defects and problems likely to give rise to pollution will be recorded on the form AEMRR/RF/4 and the site diary, with repairs/solutions being carried out immediately.

4.2.5
All drainage gullies and silt traps will be inspected at weekly intervals to ensure that they are functioning effectively.  Silt traps will be inspected every 2 weeks and emptied when necessary.  The interceptor will be inspected weekly and oil will be removed by a vacuum tanker when required and in accordance with the manufacturer’s recommendations.  The date and time of emptying will be recorded in the site diary.
4.3
Control of mud and debris 

4.3.1
Vehicles will be visually inspected before exit to check that loads are safe and that no mud is carried out on the wheels or body of the vehicle. Visual inspections of the site roads are carried out daily and recorded on form AEMRR/RF/4.  Staff will report any problems with mud or debris on the site roads immediately to the site manager.

4.3.2
The deposit of material on the industrial estate roads or the public highway will be treated as an emergency and will be cleared immediately by the operator using a hand brush or a brush towed by a vehicle or loading plant.  Silt will not be washed into roadside drains or gullies.  In addition a road sweeper will be hired in as necessary to ensure that hard surfaced areas of the site are free from mud and debris and to sweep the highway if required.
4.3.3
A water hose will be provided to permit the effective spraying of the whole site surface.

4.3.4
All loads of waste will be sheeted or sprayed with water prior to leaving the site to ensure that they comply with the requirements of the Duty of Care.

4.4
Control and monitoring of dust 
4.4.1
Water Supply - A constant supply of mains water will be available for dust suppression in all climatic conditions.  All external water pipes will be lagged to prevent frost damage during Winter months.

4.4.2
All site operations will be carried out to minimise the creation of dust.  The hose will be used to spray the concreted areas on site, any dusty surfaces and inert waste to prevent the formation of excessive dust.   During dry conditions or when dealing with particularly dry wastes a bowser or vacuum tanker will be also used to spray the site surfaces to prevent the formation of excessive dust.

4.5
Odour control 
4.5.1
The containment of waste within the transfer station present a low risk of odour nuisance.   If malodorous waste is deposited on site it will be consigned to the skip for rejected waste or removed from the site immediately.

4.6
Litter control 
4.6.1
The containment of waste within the transfer station presents a low risk of litter on site. Inspections will be carried out for the presence of windblown litter daily and operatives will be instructed to collect the litter and place it in a skip for disposal/recovery before the end of the working day.   In any event all light waste will be contained in the transfer station or placed in skips before the end of the working day.

4.7
Control of pests, birds and other scavengers
4.7.1
It is unlikely that vermin will present a problem as an ongoing pest control contract is in place. The presence of local birds of prey means it is unlikely there will be any nuisance from other birds (such as seagulls). A bird deterrent is stored on site for use if such a problem becomes apparent. The site will be inspected daily for the presence of vermin or nuisance birds and the results of the inspection noted in the site diary or site inspection form. 

4.8
Control and monitoring of noise
4.8.1
It is not anticipated that site operations will be cause a noise nuisance because of the scale and location of the operation.  The Best Practicable Means will be employed on site at all times to ensure that all plant and equipment does not produce excessive noise beyond the site boundary and complies with planning conditions.  
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