Permit Number: 	EPR/XP3830UR			Operator: 		The First Milk Cheese Company Limited

Facility:		Haverfordwest Creamery	                      Form Number: 	Water1 / 04/12/2023
Reporting of emissions to water (other than to sewer) and land for the period from XX/XX/XXXX to XX/XX/XXXX
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value [5]
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W2
	Maximum daily discharge volume
	2500 m3/day (total daily volume)
	Total daily volume
	
	Flow meter
	
	

	
	Maximum rate of discharge
	120 m3/hr
	Instantaneous (continuous)
	
	Flow meter
	
	

	
	Temperature
	35 ºC (absolute maximum)
	Instantaneous (continuous)
	
	Standard thermocouple
	
	

	
	Biochemical oxygen demand
	40 mg/L (absolute maximum)
	Instantaneous (spot sample)
	
	BS EN 1899-1
	
	

	
	
	20 mg/L (95th percentile)
	Instantaneous (spot sample)
	
	
	
	

	
	Chemical oxygen demand (COD)
	125 mg/L (daily average)
	24 hour flow proportional composite
	
	BS 6068-2.34
	
	

	
	Total suspended solids
	50 mg/L (daily average)
	24 hour flow proportional composite
	
	BS EN 872
	
	

	
	Ammonia
	10 mg/L (absolute maximum)
	Instantaneous (spot sample)
	
	BS EN ISO 11732
	
	

	
	
	3.5 mg/L (95th %ile)
	Instantaneous (spot sample)
	
	
	
	

	
	Total nitrogen
	20 mg/L (daily average)
	24 hour flow proportional composite
	
	BS EN 12260 or BS EN ISO 11905-1
	
	

	
	Total phosphorus
	4 mg/L (daily average)
	24 hour flow proportional composite
	
	BS EN ISO 11732
	
	

	
	Iron
	10 mg/L (absolute maximum)
	Instantaneous (spot sample)
	
	BS EN ISO 11885
	
	

	
	
	5 mg/L (95th %ile)
	Instantaneous (spot sample)
	
	
	
	

	
	Aluminium
	2 mg/L (absolute maximum)
	Instantaneous (spot sample)
	
	BS EN ISO 11885
	
	

	
	
	1 mg/L (95th %ile)
	Instantaneous (spot sample)
	
	
	
	

	
	pH
	 6 – 9 (minimum, maximum)
	Instantaneous (continuous)
	
	BS ISO 10523
	
	

	
	Chloride (Cl-)
	No limit set
	24 hour flow proportional composite
	
	Various EN standards available including EN ISO 10304-1 and EN ISO 15682
	
	

	
	Mercury and its compounds [6]
	228 g [6]
	-
	
	Compliance based in mass calculation
	
	

	
	Cadmium and its compounds [6]
	96 g [6]
	-
	
	Compliance based on mass calculation
	
	



Notes:
[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] For 95%ile of all measured values according to look up table
[6] This is an annual limit and only requires to be reported annually.

Signed ………………………………………………		Date………………………..

(Authorised to sign as representative of Operator)







