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Introduction

This note does not form part of the authorisation.

This licence is granted under Section 35 of the Environmental Protection Act 1990. It consists of the authorisation certificate, the site plan and subsequent conditions. 

The licence is written to prevent the authorised activities causing pollution of the environment or harm to human health.

You are reminded that it is an offence under Section 33 of the Environmental Protection Act 1990 not to comply with the terms of this licence.

This licence does not free you from the need to comply with any other regulatory regimes controlled by other bodies (such as planning or environmental health etc).

The Agency is required to maintain an up to date copy of this licence on the public register which is freely available to anyone wishing to view it.

If you wish to transfer or surrender the licence, or modify any of its conditions, you cannot do so without the consent of the Agency. Further advice can be obtained on these issues or any other aspect of the licence from your local Environment Agency office.

Status Log

	Detail
	Date
	Comment

	Application Received
	30/03/2006
	

	Application Duly Made
	30/03/2006
	

	Licence drafted for consultation
	05/09/2006
	Consulted with HSE and Ceredigion County Council

	Relevant Convictions assessed and approved
	10/04/2006
	

	Financial Provision Approved
	20/12/2006
	

	Technical Competence Approved
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	WAMITAB Certificate: Managing Transfer Hazardous Waste (4TSH).
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	Licence


Environmental Protection Act 1990

Waste Management Licensing

Regulations 1994

Waste Management Licence Number EAWML34292
Facility Type: Household, Commercial and Industrial Waste Transfer Station with Treatment & Asbestos and Clinical Waste Storage

The Environment Agency (“the Agency”) in exercise of its powers under section 36 of the Environmental Protection Act 1990, hereby authorises:

Ceredigion County Council ("the licence holder"),

whose registered office (or principal place of business) is
Department of Highways, Property and Works

Glanyrafon Office

Glanyrafon Industrial Estate

Aberystwyth

Ceredigion

SY23 3JQ

to carry out the keeping and treating of waste at  

Penrhos Depot

Croeslan

Nr. Llandysul

Ceredigion

SA44 4SX

the boundary of which is shown on the site plan at schedule 1 to this licence

to the extent authorised by and subject to the conditions of this licence.

	Signed
	Date

	
	


Audrey Evans

Authorised to sign on behalf of the Agency

1 General Considerations

1.1 Specified waste management operations

1.1.1 No waste management operations shall be authorised by this licence unless:

a specified in and undertaken in accordance with the limitations in table 1.1 and tables 4.3.1 and 4.3.2 or 

b otherwise required by the conditions of this licence as being an integral part of those operations:

	Table 1.1: Licensed activities
	

	Description of Activites
	Limits of Activities

	D15: Storage of waste pending any of the operations listed in paragraphs 1 to 14 of Part III of Schedule 4 of the 1994 Regulations, but excluding temporary storage, pending collection, on the site where it is produced.

R13: Storage of waste pending any of the operations listed in paragraphs 1 to 12 of Part IV of Schedule 4 of the 1994 Regulations, but excluding temporary storage, pending collection, on the site where it is produced.
	The maximum quantity of hazardous waste received at the site shall not exceed 10 tonnes per day.

The maximum quantity of hazardous waste stored at the site shall not exceed 10 tonnes.

All waste must be stored in the area outlined in pink on drawing no. ED1679/01 of the working plan.

Maximum storage time for biodegradable and clinical wastes shall be 72 hours.

	D14: Repackaging of waste prior to waste being submitted to any of the operations listed in paragraphs 1 to 13 of Part III of Schedule 4 of the 1994 Regulations.
	Compaction and Baling only
Only on an impermeable pavement in the area outlined in pink on drawing no. ED1679/01 of the working plan.

	D9: Physico-chemical treatment of waste not listed elsewhere in this table which results in final compounds or mixtures which are discarded by means of any of the operations listed in paragraphs 1 to 12 of Part III of Schedule 4 of the 1994 Regulations.
R3: Recycling or reclamation of organic substances that are not used as solvents, including composting and other biological transformation processes 

R4: Recycling or reclamation of metals and metal compounds

R5: Recycling or reclamation of other inorganic materials
	Treatment consisting of sorting; separation; screening; crushing or compaction of waste into different components for disposal and recovery.

Treatment of non-hazardous and inert waste for disposal shall not exceed 50 tonnes per day.
There must not be any treatment of asbestos or waste electrical and electronic equipment(WEEE).

Waste refrigeration equipment shall only be subjected to treatment in accordance with the limitiations in table 4.3.2 

There must not be any compaction of clinical waste

Treatment of waste must be carried out in the area outlined in pink on drawing no. ED1679/01 of the working plan.




1.2 Permitted wastes
1.2.1 No wastes other than those listed in Section WP/1.2 of the Working Plan shall be accepted at the site.

1.2.2 The maximum quantity of waste accepted at the site shall be less than 5,000 tonnes a year.

1.2.3 Notwithstanding the specification of permitted waste types under conditions 1.2.1 above, wastes shall not be accepted at the site which have any of the following characteristics:

a Sludges

b Consisting solely or mainly of dusts, powders or loose fibres
1.3 Staffing and understanding of requirements of licence conditions and working plan

1.3.1 Whenever the site is open to receive or despatch waste, or is carrying out any of the specified waste management treatment or disposal operations, it shall be supervised [Note on this insert:  only use where information on management structure and staffing is given in working plan, but this is an optional section and so should only require prior notification of amendments, not Agency consent]by at least one member of staff who is suitably trained and fully conversant with the requirements of the licence and the working plan regarding:

a waste acceptance and control procedures;

b operational controls and environmental monitoring;

c maintenance;

d record-keeping;

e emergency action plans;

f notifications to the Agency.

1.3.2 A copy of this licence and the working plan shall be kept available on site for reference when required by all site staff carrying out work under the requirements of the licence.

1.3.3 All site staff shall be, or shall work under the direct supervision of a member of staff who is, fully conversant with those aspects of the licence conditions and working plan which are relevant to their specific duties.

1.3.4 Attendance of the technically competent person(s)at the site shall be recorded on arrival and departure and the information shall be kept on site.

1.4 Amendments to working plan and supporting information

1.4.1 The Licence Holder shall give the Agency prior notice in writing of any proposed change to those sections of the working plan which are specified in Table 1.4 below, and to any appendices, drawings and figures which are referenced in those sections.

	Table 1.4  Sections of the working plan requiring prior consent for amendments

	Number and Heading of Working Plan Sections

And Appendices
	Sections, Subsections and Appendices requiring Prior consent for Amendments

	Section WP/1.2: Permitted Wastes
	WP/1.2

	Drawing No. ED1679/01: Proposed Waste Transfer Station Penrhos Depot, Llandysul
	Drawing No. ED1679/01


1.4.2 The notice shall be accompanied by a copy of the proposed changes, and by a written assessment of the effect that implementing the proposed change to the working plan would have on the risk posed by the site to human health and the environment.

1.4.3 The Licence Holder shall provide up to 6 additional copies of the proposed change and supporting risk assessment to the Agency, when required by the Agency in writing.

1.4.4 The proposed change to the working plan shall not be implemented unless the Agency has given its written consent to it. Following consent, the Licence Holder shall give the Agency prior written notification of the implementation date of the change, and from that date the changed section shall be deemed to be incorporated in the working plan in replacement of the previous version of that section.

1.5 Notifications

1.5.1 The Agency shall be notified without delay following the detection of:

a any malfunction, breakdown or failure of equipment or techniques, accident or fugitive emission which has caused, is causing or may cause significant pollution;

b the breach of a limit specified in this licence; and

c any significant adverse environmental and health effects.

1.5.2 Written confirmation of actual or potential pollution incidents and breaches of emission limits shall be submitted within 24 hours.

1.5.3 Prior written notification shall be given to the Agency of the following events and in the specified timescales:

a as soon as practicable prior to the permanent cessation of any of the activities;

b cessation of operation of all or part of the activities for a period likely to exceed 3 months;

c resumption of the operation of all or part of the activities after a cessation notified under (b) above

1.5.4 Where the Agency has requested in writing that it shall be notified when the licence holder is to undertake monitoring and/or spot sampling, the licence holder shall inform the Agency when the relevant monitoring is to take place. The licence holder shall provide this information to the Agency at least 14 days before the date the monitoring is to be undertaken.

1.5.5 The Agency shall be notified within 7 days of any changes in technically competent management and the name of any incoming person together with evidence that such person has the required technical competence.

1.5.6 The Agency shall be notified within 14 days of the licence holder and/or any relevant person being convicted of a relevant offence, (unless such information has already been notified to the Agency), with details of the nature of the offence, the place and date of conviction, and the sentence imposed.

1.5.7 The Agency shall be notified within 14 days of the licence holder and/or any relevant person lodging an appeal against a conviction for any relevant offence and of the outcome when the appeal is decided.

1.5.8 The Agency shall be notified within 14 days of the occurrence of the following matters except where such disclosure is prohibited by Stock Exchange rules:

a Where the licence holder is a registered company:

i any change in the licence holder's trading name, registered name or registered office address;

ii any change to particulars of the licence holder's ultimate holding company (including details of an ultimate holding company where a licence holder has become a subsidiary);

iii any steps taken with a view to the licence holder going into administration, entering into a company voluntary arrangement or being wound up; and

iv if the licence holder is not the operator: any change in the operators trading name; address; registered name or registered office address.

b Where the licence holder is a corporate body other than a registered company:

i any change in the licence holder's name or address;

ii any steps taken with a view to the dissolution of the licence holder; and

iii if the licence holder is not the operator: any change in the operators trading name; address; registered name or registered office address.

c In any other case:

i the death of any of the named licence holders (where the licence holder consists of more than one named individual); 

ii any steps taken with a view to the licence holder, or any one of them, going into bankruptcy, entering into a composition or arrangement with creditors, or, in the case of them being in a partnership, dissolving the partnership; and

iii if the licence holder is not the operator: any change in the operators trading name; address; registered name or registered office address.

1.5.9 The Agency shall be notified at least 7 days in advance of the commencement of any of the activities.

2 Site Engineering

2.1 Engineered site containment and drainage systems

2.1.1 The engineered site containment and drainage systems shall be designed, constructed, inspected, validated and maintained, and shall be fully documented and recorded, to be fit for purpose and to meet the specifications in Table 2.1 below:

[Use table to specify necessary and enforceable standards, where these are relevant to the specified waste management operations and not adequately specified in the working plan; taking into account the groundwater risk assessment accepted by the Agency.  Delete unnecessary rows.]

	Table 2.1  Site containment and drainage standards

	Type of Site Containment and Drainage
	Minimum Specified Standards of Design, Construction and Maintenance

	Hardstanding
	Areas of hardstanding shall be constructed of granular material (e.g. crushed stone, aggregate, road planings or other similar material) and maintained such that the working surface shall:

a) remain even

b) not be subject to settlement or differential settlement

c) not be subject to rutting by vehicles even when wet

d) have sufficient durability to allow cleaning for example by scraping
e) remain free of standing water.

	Impermeable pavement, bunding and sills
	Areas of impermeable pavement, bunding and sills shall be constructed and maintained to prevent:

a) fluids running off the pavement other than via the drainage system

b) the transmission of fluids through the pavement or joints.

c) ponding.

	Sealed Drainage systems
	Drainage to areas of impermeable pavement will be provided by a sealed drainage system, constructed and maintained to ensure that:
a) no liquid will run off the pavement other than via the system
b) except where they may be lawfully discharged, all liquids entering the system are collected in a sealed sump or lagoon.
c) Uncontaminated drainage from clean yard areas shall be kept separate and discharged to either surface water or sewer or watercourse or soakaway.

d) Drain/manhole covers will be colour coded on site; blue for surface water and red for foul drainage.

	Covered buildings or roofed areas
	Where wastes are stored in a building:

a) the building shall be designed, constructed and maintained to prevent ingress of rain and surface water.

b) roof water shall be kept separate from contaminated water and other liquids and shall be discharged to either surface water or a sewer or a water course or a soakaway.

	Fixed bays and other waste storage containers
	a) All fixed bays and containers used for the storage of waste must be constructed and maintained so that no waste stored within them can escape. 

b) In the event of damage or deterioration being detected to any container that is causing, or is likely to cause, a leak, that container shall be repaired or replaced immediately.

	Inspection and maintenance of engineered containment
	All areas of impermeable pavement, sealed drainage systems, covered buildings, roofed areas, fixed bays and other waste storage containers shall be inspected and maintained in accordance with the following: 

a) Inspected daily to ensure their continued integrity and that their construction remains fit for purpose. 

b) In the event of any damage occurring that breaches the integrity of the engineered containment so that it no longer meets the specified standards, the Operator shall cease importing waste into the site and shall notify the Agency immediately. The operator shall not recommence importing waste into the site until the engineered containment has been repaired to meet the required standards

c) All inspections and any necessary maintenance shall be recorded and the information kept on site


2.1.2 No wastes shall be deposited, stored, treated or otherwise handled in any area for which an engineered site containment and drainage system has been newly constructed to meet the requirements of  this condition until:

a details of the identities, relevant experience and relevant qualifications of the personnel who will be providing Quality Assurance of the engineered site containment and drainage systems have been submitted in writing to the Agency and acknowledged in writing by the Agency;

b the Validation Report on the construction of the engineered site containment and drainage system has been submitted in writing to the Agency and has been acknowledged in writing by the Agency.

2.1.3 No wastes shall be deposited, stored, treated or otherwise handled in any area for which a previously constructed and existing engineered site containment and drainage system is being used to meet the requirements of this condition unless:

a details of the identities, relevant experience and relevant qualifications of the suitably qualified Engineer who will be providing inspection and validation of the existing engineered site containment and drainage systems have been submitted in writing to the Agency and acknowledged in writing by the Agency;
b the engineered site containment and drainage system for that area has been inspected by the designated Engineer and has been maintained or improved, in accordance with their recorded advice, to be fit for purpose in that :
i areas of impermeable pavement are laid to take weight of relevant vehicles, plant and equipment without cracking or breaking; and

ii areas of impermeable pavement are free from cracks which could increase permeability; and

iii areas of impermeable pavement are resistant to mechanical, physical and chemical stresses to which they may be subjected; and

iv areas of impermeable pavement fall towards the drainage system to prevent ponding; and

v no liquid will run off areas of impermeable pavement other than via the drainage system; and

vi the drainage system is sealed so that it does not leak and is capable of collecting and containing liquids draining from the impermeable pavement ; and

vii liquid from the drainage system is disposed of to an approved discharge.

c the Validation Report on the construction of the engineered site containment and drainage system has been submitted in writing to the Agency and has been acknowledged in writing by the Agency.

3 Site infrastructure

3.1 Provision of site identification board
3.1.1 No wastes shall be received at the site until an identification board has been provided at or near the site entrance.

3.1.2 In the event of damage or defect, the board shall be repaired or replaced as soon as practicable.

3.1.3 The board shall be easily readable from outside the site entrance and shall display the following information:[Specify necessary information on the basis of the following list
a Site name and address;

b Licence Holder name (company name, not individual name unless justified as necessary);

c Operator  name (company name, not individual name unless justified as necessary);

d Emergency contact name and telephone number of the permit holder and /or operator (for security reasons, personal names and home phone numbers should not be used except where no alternative is practicable);

e Statement that the site is licensed by the Environment Agency;

f Licence number;

g Agency national numbers: 08708 506506 and 0800 807060 (or any number subsequently notified in writing by the Agency);

h Days and hours site is open to receive waste and when that waste can be treated and handled.

3.2 Site security

3.2.1 Site security measures shall be provided that prevent unauthorised access to the site, as far as practicable, and shall include the following:

a Gates that are closed and locked outside normal operating hours that prevent people entering or driving on the site.

b Prevent access by humans and livestock which is not authorised either by the Licence Holder or under legal powers of entry.

4 Site operations

[specify necessary and enforceable remedial measures; e.g. periodic road cleaning, frequency dependent upon site characteristics.]

4.1 Potentially polluting leaks and spillages of waste

4.1.1 All vehicles used on the site by the operator, and all plant and all equipment used on the site in connection with specified waste management operations, shall be operated and maintained with the objective of preventing potentially polluting leaks and spillages of wastes. 

4.1.2 In the event of any potentially polluting leak or spillage occurring on site, documented control and remediation procedures shall be implemented immediately and recorded, in accordance with table 4.1 below.

[Use table to specify necessary and enforceable standards where these are relevant to the site and not adequately specified in the working plan.  Delete unnecessary rows.]

	Table 4.1  Standards for prevention and control of leaks and spillages

	Action
	Specified standards

	Loading and unloading of waste
	a) Loading and unloading of containers shall be supervised at all times by a member of staff.

b) Lids/ caps/ bungs or other closures shall be in place during loading/ unloading.

c) Loading/ unloading shall be carried out in an area provided with engineered containment of the type required for that waste under condition 4.3, and of the standard of containment specified under condition 2.1 of this waste management licence.

d) Loading and unloading of waste refrigeration equipment shall be undertaken in a manner to prevent damage.

	Filling and emptying drums and other mobile containers


	Filling and emptying of containers shall be:

a) Carried out in a bunded area maintained in accordance with condition 2.1.2 of this waste management licence

b) supervised at all times by a member of staff.

c) Lids/ caps/ bungs or other closures shall be in place at the end of filling

d) Containers shall not be filled beyond their operational capacity.

e) Measurement of level/ void space shall be by physical dipping prior to loading.

	Inspection, maintenance and repair of mobile containers 
	a) Containers shall be inspected daily for leaks

	Control and remediation of leaks and spillages
	a) All spillages at the site shall be cleared up immediately and the residues placed in alternative containers, using appropriate equipment and proprietary absorbent to clean up liquids.

b) Upon a spill occurring, the cut-off valve in the sedimentation tank will be activated.

c) For any spillage of  clinical waste, the area of spillage shall be immediately disinfected with disinfectant that is adequate in strength and volume for the spillage

d) Spillage and materials used to clear the spill that have been, or are likely to have been contaminated, by asbestos shall be double bagged and placed in the asbestos storage skip.

e) Spillage and materials used to clear the spill that have been, or are likely to have been contaminated, by clinical waste shall be placed in the clinical waste storage area.

f) All other spill material shall be packaged in an appropriate leak-proof container and either stored in the appropriate area, or removed to a suitably licenced facility as soon as practicable.

g) The Agency shall be informed immediately of any spillages which are causing, or are likely to cause, polluting emissions to the environment.

h) Records shall be maintained of all spills and their remediation.


4.2 Fires on the site 

4.2.1 No wastes shall be burned on the site

4.2.2 In the event of a fire on the site, notwithstanding the implementation of actions to suppress and extinguish the fire, the following actions shall be implemented immediately:

a the Agency shall be informed immediately of the fire

b so far as practicable, contaminated site drainage shall be prevented from entering any surface water drain or water course or unsurfaced ground.

4.2.3 Records shall be maintained of all fires on the site and what action was taken.

4.3 Waste acceptance and control procedures

4.3.1 Wastes shall only be accepted if:

a it is of a type listed in condition 1.2.1 of this licence and does not exceed the quantities specified in table 1.1 and condition 1.2.2 of this licence; and

b it conforms to the description in the documentation supplied by the producer and holder.

4.3.2 All wastes accepted at the site shall be handled, kept and recorded in accordance with the standards specified in Tables 4.3.1 and 4.3.2  below
4.3.3 Records shall be maintained of all waste accepted onto the site.

	Table 4.3.1 Standards for waste acceptance and control procedures

	Stage of Waste Handling
	Specified standards

	a) Waste inspection
	All wastes received at the site:

i) Shall be inspected on receipt to confirm their description and composition against the relevant waste transfer note and other accompanying documentation.

ii) Shall be kept separate from and shall not be mixed with other wastes until they have been confirmed and recorded for acceptance at the site.

	b) Identification of wastes
	a) Bays and containers shall be clearly defined and labelled to identify the wastes stored within them

b) Clinical waste containers must be adequately and securely labelled at all times such that the producer and source of the wastes can be identified.

	c) Incompatible wastes
	Incompatible wastes that are likely, in combination with each other or with other material at the facility, to give rise to pollution of the environment or harm to human health outside the site, shall be clearly identified and kept physically separate in designated areas.

	d) Non-permitted wastes
	i) In the quarantine area, wastes shall be kept segregated from other wastes which are or are likely to be incompatible;

ii) The maximum quantity of wastes kept in the quarantine storage area shall be 4.6m3 at any one time.

iii) Quarantined wastes shall be removed from site within 48 hours.

	e) Waste despatch procedure


	All wastes despatched from the site shall be fully documented prior to despatch to confirm their description and composition. 


	Table 4.3.2 Standards for the handling and storage of wastes with specified characteristics

	Storage requirement
	Specified standards

	a) Asbestos Waste
	a) Kept separate from other wastes.
b) double-bagged and kept within clearly identified, secure lockable containers which shall be kept closed and locked at all times when unattended.
c) Sheet asbestos shall not be intentionally broken up or damaged at the site prior to being placed in the waste storage container.

	b) Clinical and Healthcare Wastes
	a) Shall be clearly identified and stored in a well-ventilated area separate from all other wastes.

b) Stored in secure lockable containers which shall be kept closed and locked at all times when unattended

c) Wastes that arrive in bags or other non-rigid containers shall be transferred into rigid containers immediately
d) Containers for the storage of clinical wastes found to be leaking shall be either:

i) Immediately transferred to a larger over-container

ii) Have their contents immediately transferred to an alternative suitable container

e) The integrity of containers shall be protected at all times and wastes shall not be allowed to escape the containers

f) Before any container used for the storage of clinical wastes is removed from the site it shall be washed down and disinfected, unless that container is being used for the onward transfer of clinical waste to another facility. 
g) The wash waters must be contained on an impermeable surface and prevented from entering the interceptor to prevent the flow of run-off to outside the site. The wash water shall be disposed of appropriately. 
h) Static containers and surfaces shall be routinely disinfected with a disinfectant that shall contain at least 1% free chlorine.
i) Records shall be maintained of the wash down and disinfection of any container or surface used for the storage of clinical waste.

	c) Waste Refrigeration equipment
	a) stored and handled in a such manner that will prevent damage that may lead to the release of ozone depleting substances and / or oils.

b) Free storage shall not exceed a maximum storage height of 3.5metres or 2 refrigeration units high

c) Storage on pallets or racks shall not exceed a maximum storage height of 3.5metres or 2 refrigeration units high per pallet or shelf.

d) The door seal and latch shall be removed or rendered inoperative and the door adequately secured to prevent unauthorised opening.

	d) Tyres
	a) Stored on an impermeable pavement and sealed drainage system that is resistant to fire.

b) No more than 3metres high

c) At least 15metres from the site boundary and from any building.

d) Located so as to allow the Fire Service easy access to the stockpile.


4.4 Removal of residual wastes from site
4.4.1 In the event that the specified waste management operations on the site cease and the Agency has reasonable grounds to believe that they will not be resumed within 2 months, then, notwithstanding the operational limits on storage times of wastes specified in the other conditions of this licence, the licence holder shall ensure that all wastes remaining on the site shall be removed by the date specified by the Agency in writing.

4.5 Transfers off-site

4.5.1 Records of all the wastes sent off site from the activities, for either disposal or recovery shall be maintained.

5 Pollution control, monitoring and reporting

5.1 Surface water quality monitoring and reporting systems
5.1.1 Monitoring of surface water quality shall take place at the manhole after the interceptor identified as M/H No 1 on Drawing No. ED1679/01/Rev A, or at any location subsequently agreed in writing by the Agency, to ensure that periodic measurements of quality are taken at the same position.
5.1.2 Monitoring and sampling of surface water shall be carried out and recorded in accordance with the standards specified in Table 5.1A below. 

	Table 5.1A Standards for surface water monitoring and sampling programme

	Determinands


	Monitoring frequencies
	Units and accuracies
	Trigger levels

	pH
	Quarterly unless otherwise agreed in writing with the Agency.
	( 0.1
	<6 or >9

	Electrical Conductivity @ 20(C
	
	( 10 (S/cm
	1000 (S/cm

	Mineral oils
	
	None
	Visible oil and grease

	Chlorine
	
	None
	No trace of Chlorine permitted

	Total organic carbon
	
	( 0.1 mg/l
	10 mg/l

	Total Suspended Solids
	
	( 1 mg/l
	50 mg/l


5.1.3 A record of the surface water monitoring and sampling results shall be made and submitted to the Agency in accordance with the standards specified in Table 5.1B.

	Table 5.1B   Standards for surface water monitoring and sampling records

	Surface water monitoring and Sampling Records
	Specified standards

	a) Quality assurance of monitoring and sampling
	a) The records shall be quality assured in accordance with MCERTS, or a revised Quality Assurance system agreed in writing with the Agency.

	b) Making and submission of records


	a) A record of all sampling and monitoring shall be supplied to the Agency within 1 month of its being carried out and shall include the following:

i) Determinands monitored/sampled;

ii) Specified details of measurements/samples to support analytical and QA requirements; e.g. dates, times, locations, other relevant parameters;

iii) Results of measurements/sample analyses, with error limits;

b) The records shall be submitted in a format agreed in writing with the Agency.


5.1.4 In the event that any results exceed the trigger level specified in Table 5.1A above:

a  the results shall be notified to the Agency immediately and confirmed in writing.

b the following action plan shall be implemented:

i The source of contamination that led to the exceedance of the trigger level is to be identified;

ii The Agency is to be informed in writing of the identified source and the method and timescale of remediation.

6 Amenity management

6.1 Fugitive emissions of substances

6.1.1 Fugitive emissions of substances (excluding odour and noise) shall not cause pollution.  The licence holder shall not be taken to have breached this condition if appropriate measures have been taken to prevent or where that is not practicable, to minimise, those emissions.
6.1.2 Litter or mud arising from the activities shall not cause pollution. The licence holder shall not be taken to have breached this condition if appropriate measures have been taken to prevent or where that is not practicable, to minimise, the litter and mud.
6.1.3 Litter and mud arising from the activities shall be cleared from affected areas outside the site as soon as practicable. 

6.1.4 All liquid wastes, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the licence holder has used other appropriate measures to prevent, or where that is not practicable, to minimise leakage and spillage from the primary container. 

6.2 Control of odours

6.2.1 Emissions from the activities shall be free from odour at levels likely to cause annoyance outside the site, as perceived by an authorised officer of the Agency, unless the licence holder has used appropriate measures to prevent, or where that is not practicable, to minimise the odour.
[Alternative sub-condition 6.[020].1 for use where working plan is inadequate – see guidance notes.]

6.3 Control of noise

 [This condition in particular should only be used when justified by a site-specific Agency risk assessment and in accordance with LCGN 6.[030] guidance notes.]

6.3.1 Emissions from the activities shall be free from noise at levels likely to cause annoyance outside the site, as perceived by an authorised officer of the Agency, unless the licence holder has used appropriate measures to prevent, or where that is not practicable, to minimise the noise.
6.4 Control of pests

6.4.1 Scavenging animals, scavenging birds and other pests shall not cause pollution, unless the licence holder has used appropriate measures to prevent, or where that is not practicable, to minimise such pollution.
[Alternative sub-condition 6.[040].1 for use where working plan is inadequate – see guidance notes.]

7 Records and Reporting

7.1 Records 

7.1.1 All records required to be made by this licence shall:

a be legible;

b be made as soon as reasonably practicable;

c if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and

d be retained, unless otherwise agreed by the Agency, for at least 6 years from the date when the records were made, or in the case of the following records until licence surrender:

a) off-site environmental and health effects; and

b) the condition of land and groundwater 

7.1.2 Any records required to be made by this licence shall be supplied to the Agency within 14 days, where the records have been requested in writing by the Agency.

7.2 Reporting

7.2.1 All reports and notifications required by the licence shall be sent to the Agency using the contact details supplied in writing by the Agency.

7.2.2 A summary report of the waste types and quantities accepted and removed from the site shall be made for each quarter.  It shall be submitted to the Agency within one month of the end of the quarter, and shall be in the format required by the Agency.

8 Interpretation

In these conditions and their interpretation, unless the context otherwise requires, the following terms have the specified meanings:

“accepted”

for waste being delivered to the site, shall mean accepted as waste input to the site for storage and/or processing and/or disposal under the specified waste management operations;

“authorised officer of the Agency”

means any person(s) authorised in writing by the Agency pursuant to section 108(1) of the 1995 Act to exercise any of the powers specified in subsection (4) of that section;

“clinical waste”

has the meaning as defined in regulation 1(2) of the Controlled Waste Regulations 1992 or any statutory provisions amending or replacing them;

“consequences”

for risk assessments carried out within these conditions, means the adverse effects of harm as a result of realising a hazard which cause the quality of human health (other than health and safety of site staff or visitors to the site covered under the Health and Safety at Work Act 1974) or the environment to be impaired in the short or longer term;

“engineer”

for engineering works specified in these conditions, means a person who works in the relevant branch of engineering, as a qualified professional;

“engineered”

for works specified in these conditions, means carried out and completed using the relevant engineering process specified in these conditions;

“engineered site containment and drainage system”

means all elements relating to engineered containment of activities on the site, other than final disposal to land, and incorporating site surfacing, bunding and drainage systems, buildings and fixed tanks;

“engineering”

for engineering works specified in these conditions, means the relevant process of design, construction or installation, quality assurance or validation or commissioning specified in these conditions;

“engineering survey”

means a survey carried out in accordance with recognised or approved standards by a suitably qualified competent person;

“environmental targets or receptors”

for risk assessments carried out within these conditions, shall mean identified human and environmental populations or components, as specified in these conditions or otherwise agreed by the Agency within these conditions;

“groundwater”

means any water contained in underground strata;

“hazard”

means a property or situation that in particular circumstances could lead to harm;

“immediately”

for carrying out of actions under the conditions, shall mean without delay and within a reasonable time, taking into account any more immediate direct action necessary to prevent or minimise risk to human health and the environment.  For carrying out notifications to the Agency, shall also mean by the fastest effective means available (for example, telephone) and confirmed in writing within 1 working day (or such other time as may be agreed by the Agency within the conditions);

“inert waste “

means  waste which when disposed of in or on land does not undergo any significant physical, chemical or biological transformation;

“maintenance”

for engineering maintenance specified in  these conditions, means the process of inspection, testing, repair of the relevant engineering works specified in these conditions;

“livestock”

livestock includes: cattle, horses, goats, sheep and pigs; but does not include domestic pets, such as dogs and cats, or any wild animals;
“preparatory works”

means engineering works required prior to the carrying out of the activities authorised by this licence;

“probability”

means the quantified expression of chance, denoted either as:

· the ratio or percentage of the occurrence of a  particular event as one among a number of possible events; 

· or as the frequency of occurrence of a particular event in a given period of time;

“received”

for waste being delivered to the site, shall mean delivered to the site and undergoing the waste acceptance procedures specified in the working plan, including storage of those wastes during those procedures prior to acceptance of the waste;

“release pathways”

for risk assessments carried out within these conditions, shall mean the routes by which defined hazards may potentially realise their consequences, defined in terms of releases or emissions from the site that go beyond the site containment or boundary via one or more of the following routes, either directly or indirectly: Land; Groundwater; Surface water; Atmosphere;

“relevant offences”

are offences within the meaning of regulation 3 of the Waste Management Licensing Regulations 1994 or any statutory provisions or regulations amending or replacing them;

“risk”

means a combination of the probability and consequences of occurrence of a defined hazard;

“risk assessment”

means the systematic identification, analysis, estimation and evaluation within a defined scope of the defined risks of a particular activity, operation, process or design, carried out and reported by suitably qualified or competent persons, using recognised quantified or semi-quantified methods and techniques.

Unless otherwise agreed by the Agency within these conditions, a risk assessment shall include and record the following:

· definition of  the hazards associated with an activity, operation, process or design;

· assessment of the probability of those hazards occurring;

· determination of the potential consequences of those hazards for defined environmental targets or receptors, taking into account defined release pathways and defined protective measures;
· evaluation of the potential magnitude of those consequences and the probability of their occurrence;

“scope of risk assessment”

means the boundaries of the risk assessment and the risks to be assessed within those boundaries, as defined in the conditions or otherwise agreed by the Agency within the conditions;

“specified waste management operations”

means the waste management operations authorised by condition 1.1 of this licence;
“surface water management system”

means all elements relating to collection of rain water or surface water from individual landfill phases and the landfill site as a whole, and incorporating methods of water collection, containment and the subsequent treatment and/or disposal system, either on or off the site;

“surface water”

means any lake, pond, river or watercourse whether natural or artificial;

“the 1994 Regulations”

 means the Waste Management Licensing Regulations 1994 and any statutory provisions or regulations amending or replacing them.

“the Agency”

means the Environment Agency;

“the Licence Holder”

means the Licence Holder specified in this licence or other person to whom the licence has been transferred in accordance with section 40 of the Environmental Protection Act 1990;

“the operator”

means a person who is in occupation of the site and has responsibility for carrying out day to day activities at the site;

“the site”

means the land, structures, plant and equipment to which this licence relates;
“time periods, e.g. annually, quarterly, monthly, per year, etc. “

Where periods are referred to in conditions, they shall be calculated in the following way:

· annually or per year: 1 April to 31 March;

· quarterly: 1 April to 30 June, 1 July to 30 September, 1 October to 31 December, 1 January to 31 March;

· monthly: calendar month;

· weekly:  Monday to Sunday.

Where the issue of the licence does not coincide with the start of any of these periods, then any relevant limits for the first period shall apply pro rata;

“waste”

means controlled waste as defined in section 75(4) of the 1990 Act and the Controlled Waste Regulations 1992 or any statutory provisions or regulations amending or replacing them;

“working plan”

means the working plan identified in writing by the Agency at the time of issue of this licence and any subsequent amendments to it made in accordance with the conditions of this licence.

Schedule 1- Site plan
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Asiantaeth yr Amgylchedd Cymru

Maes Newydd, Llandarsi, Nedd Port Talbot, SA10 6JQ

Ffon 08708 506 506

Environment Agency Wales

Maes Newydd, Llandarcy, Neath Port Talbot, SA10 6JQ

Tel 08708 506 506
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