Permit Number: 	EPR/EP3738NG					Operator: WEPA UK Ltd

Facility:		Bridgend Papermill					Form Number: 	Performance 1 31/03/2016

Reporting of other performance indicators for the period DD/MM/2016 to DD/MM/2017

	Parameter
	
	Units 
	

	
	
	
	

	Oxides of Nitrogen
	Tonnes/T
	

	Carbon Dioxide 
	Tonnes/T
	

	Biological Oxygen Demand
	kg/T
	

	Suspended Solids 
	kg/T
	

	Nitrogen and phosphorus
	kg/T
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)




Permit Number: 	EPR/EP3738NG			Operator: 	WEPA UK Ltd

Facility:		Bridgend Papermill			Form Number: 	Resource efficiency 1 31/03/2016

Reporting of Resource efficiency performance metrics for the period DD/MM/2016 to DD/MM/2017

	Parameter

Water
	Units                                                                        Methodology

Total m3/p.a                                     m3/t           Measured or Calculated 

	
	

	Water Inputs to the Mill
	
	
	

	Surface water (actual not licensed) eg: river water
	
	
	

	Groundwater (actual not licensed) eg: borehole water
	
	
	

	Mains water (only report if used in the paper or pulp manufacturing process)
	
	
	

	Other water (eg; if rainwater harvesting is practised)
	
	
	

	Water used in manufacturing
	
	
	

	Cooling water (once through or hybrid systems)
	
	
	

	Process water
	
	
	

	Other water used in manufacturing
	
	
	

	Other inputs of water/moisture
	
	
	

	Pulp or other fibre or wood at X% moisture content2 
	
	
	

	Waste paper for recycling at X% moisture content2
	
	
	

	Water outputs
	
	
	

	Waste Water discharged to surface waters 
NB; this figure should be the one used to report water usage per tonne as per BREF benchmarks under BATC No.5 and should exclude site drainage and cooling water
	
	
	

	Waste water discharged to sewer
	
	
	

	Losses to evaporation
	
	
	

	Losses in final product at Y% moisture content2
	
	
	

	Losses in major waste stream outputs at Y% moisture content such as sludge2
	
	
	

	Losses in major waste stream outputs at X% moisture content such as rejects (EWC 03 03 07)2
	
	








	Parameter

Waste 
	Units

 Total tonnes/p.a                            Measured or Calculated                         

	
	

	Waste/raw material Inputs (other than those reported via quarterly waste returns)
	
	

	Pulp 
	
	

	Starch & main fillers
	
	

	Other significant raw material inputs if >1000 tonnes
	
	

	
	
	

	Waste/raw material outputs (other than those reported via quarterly waste returns)
	
	

	
	
	

	
	
	

	Production (Net annual production reported as total as defined in the BREF BATCs1)
	
	

	
	
	

	
	
	



Notes: 
1. (i) For paper mills: the unpacked, saleable production after the last slitter winder, i.e. before converting. (ii) For off-line coaters: production after coating. (iii)  For tissue mills: saleable production after the tissue machine before any rewinding processes and excluding any core.  (iv) For market pulp mills: production after packing (ADt). (v) For integrated mills: Net pulp, production refers to the production after packing (ADt) plus the pulp transferred to the paper mill (pulp calculated at 90 % dryness, i.e. air dry). Net paper production: same as (i)
2. X% & Y% moisture content. Is defined as the average moisture content over the 12 month period. Monitoring frequency determined by each mill but to be noted on the return for each input/output.


	Operator’s comments:






Signed …………………………………………………………….		Date………………………..
	(Authorised to sign as representative of Operator)









Permit Number: 	EPR/EP3738NG			Operator: WEPA UK Ltd

Facility:		Bridgend Papermill			Form Number: 	 Water 1 31/03/2016
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/2016 to DD/MM/2017
	Emission
Point
	Substance /
Parameter
	Emission/
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4] [5]]

	
	
	
	
	
	
	
	

	W1
	Flow rate
	No limit set
	Instantaneous
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Maximum Daily Flow [6]
	17,500m3/day
	24 hours
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Mean Daily Flow
	No limit set
	24 hours
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	pH
	6.5 (min) 8.5 (max)
	Daily average
	
	MCERTS approved instrumentation or equivalent
	
	

	W1
	Temperature
	25oC
	Daily average
	
	Standard Temperature Sensor
	
	

	W1
	Chemical Oxygen Demand (COD) [7]
	No limit set
	24-hour flow proportional sample
	
	COD: BS ISO 15705

TOC: BS EN 1484
	
	

	W1
	Biological Oxygen Demand (BOD)
	10 mg/l
	24-hour flow proportional sample
	
	BS EN 1899-1
	
	

	W1
	Total Suspended Solids
	25 mg/l
	Daily
	
	BS EN 872
	
	

	W1
	Ammonia as N
	1 mg/l
	Daily
	
	BS EN ISO 11732 or ISBN 0117516139
	
	

	W1
	Total Nitrogen
	No limit set
	24-hour flow proportional sample
	
	BS EN 12260
	
	

	W1
	Total Phosphorus
	No limit set
	24-hour flow proportional sample
	
	BS EN ISO 6878 followed by BS EN ISO 15681-1
	
	

	W1
	Mercury and its compounds, expressed as mercury (Total Hg)
	0.1 µg/l
	24-hour flow proportional composite sample
	
	BS EN ISO 17852
	
	

	W1
	Cadmium and its compounds, expressed as cadmium (Total Cd)
	0.6 µg/l
	24-hour flow proportional composite sample
	
	BS EN ISO 17294
BS EN ISO 5961
BS EN ISO 1185
	
	

	W1
	Other compounds: AOX
	
	24-hour flow proportional sample
	
	AOX: BS EN ISO 9562 or other method as agreed in writing with Natural Resources Wales
	
	

	W1
	Priority Hazardous Substances Screen [8]
	--
	24-hour flow proportional composite sample
	
	GCMS analysis at UKAS accredited laboratory
	
	

	W1
	Zn (total and dissolved) and its compounds
	--
	24-hour flow proportional sample
	
	BS EN ISO 15586:2003
	
	

	W1
	Cu (total and dissolved) and its compounds
	--
	24-hour flow proportional sample
	
	BS EN ISO 15586:2003
	
	

	W1
	Cd (total and dissolved) and its compounds
	--
	24-hour flow proportional sample
	
	BS EN ISO 15586:2003
	
	

	W1
	Pb (total and dissolved) and its compounds
	--
	24-hour flow proportional sample
	
	BS EN ISO 15586:2003
	
	

	W1
	Hg (total and dissolved) and its compounds
	--
	24-hour flow proportional sample
	
	BS EN ISO 15586:2003
	
	

	W1
	Ni (total and dissolved) and its compounds
	--
	24-hour flow proportional sample
	
	BS EN ISO 15586:2003
	
	

	W1
	Pentachlorophenol
	1.0 µg/l
	24-hour flow proportional sample
	
	As agreed with Natural Resources Wales
	
	

	W1
	Tributylin
	0.01µg/l
	24-hour flow proportional sample
	
	As agreed with Natural Resources Wales
	
	




[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] In the case of results for the Hazardous pollutants screen supply the quoted Limit of Detection (LOD) with the result.
[6] In the case of daily flow supply the maximum and mean figure for each month within the 6 month reporting window.
[7] If TOC is already monitored as a key process parameter, there is no need to measure COD, however the correlation between the two parameters must established and checked regularly.
[8] Hazardous pollutants screen substances are: Chlorpyriphos, Cypermethrin, Endosulphan (A & B), 4- nonylphenols & Nonylphenol ethoxylates, PCP, TBT
[9] For integrated or multi product mills where the BAT AEL range has been calculated according to a mixing rule based on their share of the discharge, based on information supplied by the Operator, the Operator must notify Natural Resources Wales if the product/ raw material mix changes by more than 10% in any direction.


Signed …………………………………………………………….  		Date………………………..




Permit Number: 	EPR/EP3738NG		Operator: WEPA UK Ltd

Facility:		Bridgend Papermill		Form Number: 	 Air 1 31/03/2016
Reporting of emissions to air for the period from DD/MM/2016 to DD/MM/2017
	Emission
Point
	Substance /
Parameter
	Emission/
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	250 mg/m3
	Hourly average
	
	BS EN 14792
	
	

	A1
	Sulphur dioxide
	50 mg/m3
	Hourly average
	
	BS EN 14791 / TGN M21
	
	

	A1
	Particulates
	10 mg/m3
	Hourly average
	
	BS EN 13284-1
	
	

	A1
	Carbon monoxide
	150 mg/m3
	Hourly average
	
	BS EN 15058
	
	

	A2
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	250 mg/m3
	Hourly average
	
	BS EN 14792
	
	

	A2
	Sulphur dioxide
	50 mg/m3
	Hourly average
	
	BS EN 14791 / TGN M21
	
	

	A2
	Particulates
	10 mg/m3
	Hourly average
	
	BS EN 13284-1
	
	

	A2
	Carbon monoxide
	150 mg/m3
	Hourly average
	
	BS EN 15058
	
	

	A4
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	40 mg/m3 (natural gas) 100 mg/m3 (gas oil)
	Hourly average
	
	BS EN 14792
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)



Permit Number: 	EP3738NG			Operator:  WEPA UK Ltd

Facility:		Bridgend Papermill		Form Number: 	WaterUsage1 31/03/2016

Reporting of Water Usage for the year DD/MM/2016 to DD/MM/2017

	Water Source
	Usage
(m3/year
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	Site borehole
	
	
	

	River abstraction
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)


[bookmark: _GoBack]Permit Number: 	EP3738NG			Operator:  WEPA UK Ltd

Facility:		Bridgend Papermill		Form Number: 	Energy1 31/03/2016

Reporting of Energy Usage for the year DD/MM/2016 to DD/MM/2017

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


