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                       The working plan
1 The premises as a whole are approximately 80 metres long and 25 metres at it’s widest point, and incorporates a steel framed and clad building with a square footage of around 150 metres.
2 Complete motor vehicles as well as damaged vehicles are collected from outside sources by our own transport. complete vehicles are also purchases from the public on site and the v5 documentation processed through the dvla website online. Unusable residue from these vehicles is disposed of as follows.
3 Car bodies, engines etc are sold for defragmenting to a large registered scrap metal dealer 

4 Tyres are disposed of to registered rubber disposal agents for recycling in the equestrian arena

5 Fluids are as above 
6 Non-ferrous metals are our main line of business and these are stored and processed in our secure workshop.
7 Elv’s are de-polluted on a specially made stand which is next to the bunded area for the waste oils and spent fluids.the area is covered over and locked when the site is not in use.although the area is bunded, the cover ensures weather resistance at all times.
8 A site diary is available at all times, documenting any issues and the appropriate telephone numbers to the emergency services and the environment agency is duly noted.

9 The secure office is located near the entrance and all relevant paperwork is located here.

10  We do not produce mud or any other wastes.

                                        Site works

1 the main workshop is approximately 150 metres squared and contains the following,non-ferrous metal shears,non-ferrous metal bailer, toilet and hot water facilities and a compressor. the building is also fully concreted inside and has been fully clad in sheet steel.
The building also has a 5 foot concrete wall around it. There are various steel framed bins for storage of non-ferrous metals such as brass,copper and lead. The building has excellent lighting, ensuring safety and visibility at all times. There is also a small kithen area where coffee making facilities are kept along with a microwave oven and small fridge. 
2 the highway to the premises is via a council adopted public road and the entrance itself is directly off the road itself.

The whole of the yard is fully concreted and there is an appropriate interceptor tank situated under the ground. The site is fully kerbed and any rainwater etc flows through the interceptor tank. The whole site is concreted with a slight fall in it for this to be achieved. The whole perimeter is kerbed with concrete block kerb ensuring total containment in an unforeseen event.
3 the existing fence is constructed of steel palisade fencing, with a concrete plinth of around 12 inches at the base. The main entrance gates are again constructed of steel and are securely locked after working hours. The site is totally secure at all times and 24hr security cameras(4) are recording constantly.
4 Unauthorised entries are prevented by the presence of staff either working just inside the gateway or in the office which is located just inside the gate and is clearly signposted.

5 An approximate maximum of 30 vehicles are stored on the site while awaiting de-pollution. car batteries are stored in purpose built plastic containers covered with water-proof lids. Waste oil,brake fluid,spent coolant and screen wash are all stored in appropriate, clearly marked containers in an enclosed wall bunded area. This area is off-limits to the public, and is clearly signposted. All fluids are then stored in the bunded area which is covered from the elements and locked when not in use. When collection of said fluids are conducted, access is easily obtained and coned off while this work is carried out. Paperwork including hazardous waste records are carried out at the nearby office.     
                                       Use of plant and equipment
1 the company uses the following plant on site

   Diesel powered fork-lift truck

   Two flat bed trucks both with cranes (mx53dld and s314cae)
   Oxy-propane cutting equipment

  Two 360 tracked machines (for loading/unloading vehicles) one of these has a rotating grab attachment and the other electro-magnetic equipment to enable ferrous metal loading.
2 On-site handling is by the machines above and carried out by competent and fully qualified members of staff.   

3 All equipment on site is maintained by company staff however are serviced periodically by qualified mechanics.

4All items of plant are stored at the premises

5 The site office is of steel construction with plywood lining. The office has a computer and a quad designed cctv system with 24 hour hard disc recording. All paperwork is located here for easy access
6 All staff are fully licensed and are regularly assessed independently to ensure we are up to date in our industry.

7 The site is floodlit at night providing support for the cctv cameras, which record 24hrs a day ensuring total security for the site at all times.
                         Management of facility
1 The land line phone is manned at all times via the site office or via a dect digital extention.the office fax and e-mail facility can also be accessed from here. A responsible member of staff is always present on site.

2 There are toilet and hot and cold washing facilities in the main workshop which are marked staff only.
3 All employees are fully conversant in the basic handling of all the machines and the fire extinguishers. All staff is aware of basic fire drill practises and drills are carried out quarterly.
4 All electrical appliances are regularly checked by a competent electrician and fire extinguishers are maintained by a local contractor.
5 Details of all vehicles de-polluted and disposed of  are recorded in the office, both via the pc and manually in the company’s records
   Also any sales of goods are also fully recorded in order to assist waste management site returns. Everything is recorded ensuring ease of access for all forms and records. Customers of elv’s are requested to wait in the office while the certificate of destruction notice is issued or sent electronically via e-mail. 

                               Environmental controls 
1 The highway to the site is an adopted road and has a council storm water drain immediately at the foot of the site gates catching all the storm water from the highway. The access is excellent and we have never encountered any traffic problems since we began trading.
2 Our premises adjoin the road seamlessly and are 100% concreted, we do not produce mud or any other wastes.

3 No noise or vibration is produced from the premises other than noise produced is from our vehicles which have the normal silencing equipment which is maintained to restrict noise to the original manufacturer’s specification.

4 No odours of any kind are produced by operations at the premises

5 Because of the substantial fencing to the site no litter can be transferred outside by weather factors, however any debris is cleared away when the site inspection is carried out each morning.
6 The outer boundary of the site has been fully landscaped with a variety of different trees and shrubs, providing the site with foliage all year round. A landscape gardener is contracted to maintain this.

7 There are currently no issues with pest control at the site and if a problem should arise it would be dealt with by Blaenau Gwent county council.

8 Hazardous scrap metal is not processed at the site, however if anyone needs a key holder at the premises, a member of staff is always available via cell phone on 0771 55 937 55. The police and Blaenau Gwent council are also aware of this number in an emergency. This number is also listed on the site id board on the entrance to the site.
9 General rubbish is removed periodically and taken to silent valley amenities site via the council. This is done mainly for rubbish collected from the council contract for the collection of abandoned vehicles which we hold.    

 Up to date site plan
1 poly plastic sealed battery storage

2 site office

3 workshops
4 storage skip for pc cable

5 storage skip for stainless steel

6 storage skip for rolled aluminium

7 storage skip for cast aluminium

8container unit for spare parts

9former concrete building (no longer in use)

7 Storage skips (empty)

8 Ferrous metals bin

9 De-pollution station

10 Bunded area for fluids

11 Cars awaiting de-pollution area

12 Re-useable tyre storage

13  De-polluted engine bin(sealed)   
