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Permit with introductory note
The Environmental Permitting (England & Wales) Regulations 2010

Green Waste Company (Abergavenny) Limited

Maindiff Court Farm 
Llantilio Pertholey
Abergavenny
NP7 8AY




Permit number
EPR/HB3597TC

Maindiff Court Farm
Permit number EPR/HB3597TC
Introductory note
This introductory note does not form a part of the permit
The main features of the permit are as follows.

This Tier 3 Bespoke permit allows the operator to carry out a composting activity involving the storage, physical treatment and composting of specified green, biodegradable wastes only, in an open composting system. Composting can only be carried out under aerobic conditions and no hazardous wastes are allowed. 

This permit allows more than 500 tonnes to be composted at one time. The total quantity of waste accepted at the site shall not exceed 13,163 tonnes a year.
This permit does not allow the burning of any wastes, either in the open, inside buildings or in any form of incinerator.

Biological treatment of waste is a newly prescribed activity under the Industrial Emissions Directive.  This activity is subject to Section 5.4 A (1)(b)(i) of the Environmental Permitting Regulations – biological treatment of non-hazardous waste for recovery (with a capacity exceeding 75 tonnes per day).  Therefore, treatment limits have been included in Table S1.1 of this permit to reflect that the permit has been assessed on the basis that it is a waste facility, and to therefore prevent the site from operating over this threshold, and becoming an installation. 

This permit does not allow any point source emission into surface waters or groundwater. However, under the emissions of substances not controlled by emission limit rule, clean surface water from roofs, or from areas of the site that are not being used in connection with storing or treating waste, may be discharged directly to surface waters, or to groundwater by seepage through the soil via a soakaway. Liquid waste from permitted activities is directed by engineered drainage channels to a sealed tank. Leachate is then recirculated to the windrows to maintain the correct moisture balance.

Bioaerosol monitoring frequency given in Table S3.3 may be reduced to twice a year after the first year of operation if agreed in writing by Natural Resources Wales.

Liquids from the open windrow process drain to a leachate storage tank and the leachate is spread to land in accordance with a suitable environmental permit, subsequent approved deployments and in accordance with the Department for Environment, Food and Rural Affairs (DEFRA) Code of Good Agricultural Practice.

Clean surface water from roofs, or from areas of the site that are not being used in connection with storing and treating waste, may be discharged directly to surface waters, or to groundwater by seepage through the soil via a soakaway. 

The status log of the permit sets out the permitting history, including any changes to the permit reference number.

	Status log of the permit

	Description
	Date
	Comments

	Application EPR/BP3392LC/A001
	Duly made 08/07/08
	Application for composting facility.

	Permit determined
EPR/BP3392CL
	09/06/09
	Original permit issued to William Lewis and Andrew Lewis.

	Application EPR/HB3597TC/T001
(full transfer of permit EPR/BP3392LC)
	Duly made 04/07/13
	Application to transfer permit in full to Green Waste Company (Abergavenny) Limited.

	Transfer determined
EPR/HB3597TC
	04/10/13
	Full transfer of permit to Green Waste Company (Abergavenny) Limited complete.

	Variation application EPR/HB3597TC/V002
(variation and consolidation)
	Duly made
20/08/14
	Variation application to increase permitted area, include additional waste codes and increase annual throughput.

	Additional information received in response to a Schedule 5 notice sent on 11/11/14
	10/12/14

	Site treatment capacity information and bioaerosol monitoring report (dated September 2014).

	
	05/01/15
	Bioaerosol monitoring report (dated December 2014).

	Additional information received in response to an informal request for information sent on 05/02/15
	10/03/15
	Bioaerosol monitoring report (dated February 2015).

	
	
	Supplementary bioaerosol monitoring report (dated February 2015).

	
	
	Supplementary bioaerosol data (dated March 2015).

	Additional information received in response to an informal request for information sent on 01/04/15
	07/04/15
	Confirmation that activities that agitate waste will not be carried out when the wind blows in an Easterly direction and will be avoided (where possible) when the wind blows in a Southerly direction.

	Additional information received in response to an informal request for information sent on 09/04/15
	13/04/15
	Confirmation of scale of site plan (reference 'Envi~MF~002 Revision 1').

	Variation determined
EPR/HB3597TC
	15/04/15
	Varied and consolidated permit to increase permitted area, include additional waste codes and increase annual throughput, issued to Green Waste Company (Abergavenny) Limited.



End of introductory note
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Permit


The Environmental Permitting (England and Wales) Regulations 2010

Permit number 
EPR/HB3597TC
This is the consolidated permit referred to in the variation and consolidation notice for application EPR/HB3597TC/V002 authorising, 

The Natural Resources Body for Wales (“Natural Resources Wales”) authorises, under regulation 13 of the Environmental Permitting (England and Wales) Regulations 2010 
[bookmark: OperatorName2]
Green Waste Company (Abergavenny) Limited (“the operator”),

[bookmark: InstallationAddress21]whose registered office is 

Rose Cottage
Maindiff Court Farm
Abergavenny
Monmouthshire
Wales
NP7 8AJ

company registration number 08232217 

to operate waste operations at

Maindiff Court Farm 
Llantilio Pertholey
Abergavenny
NP7 8AY

to the extent authorised by and subject to the conditions of this permit.

	Name
	Date

	Holly Noble
	15/04/2015


Authorised on behalf of Natural Resources Wales



Conditions 
Management
1.1 General management
1.1.1 The operator shall manage and operate the activities:
(a) in accordance with a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances, closure and those drawn to the attention of the operator as a result of complaints; and
(b) using sufficient competent persons and resources.
1.1.2 Records demonstrating compliance with condition 1.1.1 shall be maintained. 
1.1.3 Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of it kept at or near the place where those duties are carried out.
1.1.4 The operator shall comply with the requirements of an approved competence scheme.
Avoidance, recovery and disposal of wastes produced by the activities
1.2.1 The operator shall take appropriate measures to ensure that:
(a) the waste hierarchy referred to in Article 4 of the Waste Framework Directive is applied to the generation of waste by the activities; and
(b) any waste generated by the activities is treated in accordance with the waste hierarchy referred to in Article 4 of the Waste Framework Directive; and
(c) where disposal is necessary, this is undertaken in a manner which minimises its impact on the environment.
1.2.2 The operator shall review and record at least every four years whether changes to those measures should be made and take any further appropriate measures identified by a review.
2	Operations
2.1	Permitted activities
2.1.1	The operator is only authorised to carry out the activities specified in schedule 1 table S1.1 (the “activities”). 
2.2	The site 
2.2.1	The activities shall not extend beyond the site, being the land shown edged in green on the site plan at schedule 7 to this permit.
2.3	Operating techniques
2.3.1	(a) 	The activities shall, subject to the conditions of this permit, be operated using the 
		techniques and in the manner described in the documentation specified in 	schedule 1, table S1.2, unless otherwise agreed in writing by Natural Resources Wales.		
(b)	If notified by Natural Resources Wales that the activities are giving rise to pollution, the operator shall submit to Natural Resources Wales for approval within the period specified, a revision of any plan or other documentation (“plan”) specified in schedule 1, table S1.2 or otherwise required under this permit which identifies and minimises the risks of pollution relevant to that plan , and shall implement the approved revised plan in place of the original from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
2.3.2	Waste shall only be accepted if:
(a)	it is of a type and quantity listed in schedule 2 table(s) S2.1 [, S2.2 etc]; and 
(b)	it conforms to the description in the documentation supplied by the producer and holder.
3	Emissions and monitoring
3.1	Emissions to water, air or land
3.1.1	There shall be no point source emissions to water, air or land except from the sources and emission points listed in schedule 3 tables S3.1, S3.2 and S3.3.
3.1.2	The limits given in schedule 3 shall not be exceeded.
3.2 Emissions of substances not controlled by emission limits
3.2.1 Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.
3.2.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution, submit to Natural Resources Wales for approval within the period specified, an emissions management plan which identifies and minimises the risks of pollution from emissions of substances not controlled by emission limits;
(b)	implement the approved emissions management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.2.3	All liquids in containers, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the operator has used other appropriate measures to prevent or where that is not practicable, to minimise, leakage and spillage from the primary container.
3.3	Odour
3.3.1	Emissions from the activities shall be free from odour at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved odour management plan, to prevent or where that is not practicable to minimise the odour. 
3.4	Noise and vibration
3.4.1	Emissions from the activities shall be free from noise and vibration at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved noise and vibration management plan to prevent or where that is not practicable to minimise the noise and vibration.
3.4.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to noise and vibration, submit to Natural Resources Wales for approval within the period specified, a noise and vibration management plan which identifies and minimises the risks of pollution from noise and vibration;
(b)	implement the approved noise and vibration management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.5	Pests
3.5.1 	The activities shall not give rise to the presence of pests which are likely to cause pollution, hazard or annoyance outside the boundary of the site. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved pests management plan, have been taken to prevent or where that is not practicable, to minimise the presence of pests on the site.  
3.5.2 	The operator shall:             
(a)           if notified by Natural Resources Wales, submit to Natural Resources Wales for approval within the period specified, a pests management plan which identifies and minimises risks of pollution, hazard or annoyance  from pests;
(b)           implement the pests management plan, from the date of approval, unless otherwise agreed in writing by Natural resources Wales.
3.6	Monitoring
3.6.1	The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring specified in the following tables in schedule 3 to this permit:
		(a)	process monitoring specified in table S3.1;
		(b)	bioaerosol monitoring specified in table S3.2.
[bookmark: _Toc449070323]3.6.2	The operator shall maintain records of all monitoring required by this permit including records of the taking and analysis of samples, instrument measurements (periodic and continual), calibrations, examinations, tests and surveys and any assessment or evaluation made on the basis of such data.
3.6.3	Monitoring equipment, techniques, personnel and organisations employed for the emissions monitoring programme and the environmental or other monitoring specified in condition 3.3.1 shall have either MCERTS certification or MCERTS accreditation (as appropriate), where available, unless otherwise agreed in writing by Natural Resources Wales.
3.6.4	Permanent means of access shall be provided to enable sampling/monitoring to be carried out in relation to the emission points specified in schedule 3 tables S3.1, S3.2 [,S3.3 etc] unless otherwise agreed in writing by Natural Resources Wales.
[bookmark: _Toc77056949][bookmark: _Toc457192259]4	Information
4.1	Records
4.1.1 All records required to be made by this permit shall:
(a) be legible;
(b) be made as soon as reasonably practicable;
(c) if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
(d) be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made, or in the case of the following records until permit surrender:
(i) off-site environmental effects; and
(ii) matters which affect the condition of the land and groundwater.
4.1.2	The operator shall keep on site all records, plans and the management system required to be maintained by this permit, unless otherwise agreed in writing by Natural Resources Wales. 
4.2	Reporting
4.2.1	The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
4.2.2	Within one month of the end of each quarter, the operator shall submit to Natural Resources Wales using the form made available for the purpose, the information specified on the form relating to the site and the waste accepted and removed from it during the previous quarter.
4.2.3	Within 28 days of the end of the reporting period the operator shall, unless otherwise agreed in writing by Natural Resources Wales, submit reports of the monitoring and assessment carried out in accordance with the conditions of this permit, as follows:
(a) in respect of the parameters and emission points specified in schedule 4 table S4.1;
(b) for the reporting periods specified in schedule 4 table S4.1 and using the forms specified in schedule 4 table S4.4 ; and
(c) giving the information from such results and assessments as may be required by the forms specified in those tables.
4.3	Notifications
4.3.1	Natural Resources Wales shall be notified without delay following the detection of:
(a) any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution;
(b) the breach of a limit specified in the permit; or 
(c) any significant adverse environmental effects.  
4.3.2	Any information provided under condition 4.3.1 shall be confirmed by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
4.3.3	Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.
4.3.4	Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules: 
Where the operator is a registered company:
(a) any change in the operator’s trading name, registered name or registered office address; and
(b)	any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and
(b) any steps taken with a view to the dissolution of the operator.
		In any other case: 
(a) the death of any of the named operators (where the operator consists of more than one named individual);
(b) any change in the operator’s name(s) or address(es); and
(c) any steps taken with a view to the operator, or any one of them, going into bankruptcy, entering into a composition or arrangement with creditors, or, in the case of them being in a partnership, dissolving the partnership.
4.3.5	Where the operator proposes to make a change in the nature or functioning, or an extension of the activities, which may have consequences for the environment and the change is not otherwise the subject of an application for approval under the Regulations or this permit:
(a) Natural Resources Wales shall be notified at least 14 days before making the change; and
(b)        the notification shall contain a description of the proposed change in operation.
 4.4	Interpretation
4.4.1	In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
4.4.2	In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “without delay”, in which case it may be provided by telephone. 
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	Table S1.1 activities

	
	Description of activities for waste operations 
	Limits of activities 

	Open windrow composting
	R13: Storage of wastes pending any of the operations  numbered R1 to R12 (excluding temporary storage, pending collection, on the site where it is produced)
 
R3: Recycling/reclamation of organic substances which are not used as solvents
	The storage and physical treatment of wastes shall take place on an impermeable surface with a sealed drainage system.

Physical treatment consisting only of: 
- composting 
- maturation 
- manual separation
- sorting
- shredding
- screening
- bagging 
of permitted waste for the purpose of recovery only.

The total quantities of wastes undergoing biological treatment at the whole site shall not exceed 75 tonnes per day.

The storage, physical treatment and composting of wastes under anaerobic conditions shall be prevented. 

Each composting batch shall undergo an identifiable sanitisation and stabilisation stage.

Waste types as specified in Table S2.1.




	Table S1.2 Operating techniques

	Description
	Parts
	Date Received

	Technical Guidance Note: How to comply with your Environmental Permit
	All
	N/A

	Guidance on the evaluation of bioaerosol risk assessment s for composting facilities (Environment Agency)
	All
	N/A

	The Composting Industry Code of Practice (Association for Organics Recycling) 2005
	All
	N/A

	Industry guide for prevention and control of odours at biowaste processing facilities (Association for Organics Recycling) 2007
	All
	N/A

	Quality Protocol for Compost (Waste and Resources Action Program/Environment Agency)
	All
	N/A

	Standardised protocol for the monitoring of bioaerosols at open composting facilities (Association for Organics Recycling) 2009
	All
	N/A

	Application
	Odour management plan dated April 2014 (document reference MF/OMP/002 ) – All 
	22/05/14


	
	[bookmark: _GoBack]Site specific bioaerosol risk assessment dated May 2014 – listed sections only: 

3.1 Site Description
	

	
	3.2 Site Layout (including Proposed Operation)
	

	
	3.3 Process Stages
	

	
	6.0 Conclusions
	

	
	7.0 Recommendations
	

	
	Site Environmental Management System (EMS) – listed sections only:

2.6 Waste acceptance procedure
	

	
	3.2 Engineered site containment and drainage
	

	
	3.3 Surface water management
	

	Additional information received in response to an informal request sent on 13 August 2014.
	Site biological treatment capacity calculations including minimum composting time (84 days).
	19/08/14

	Additional information received in response to Schedule 5 notice sent 11 November 2014.
	Email confirmation that:
· 12 windrows will be present on new composting pad
· 3 windrows will be present on existing composting pad 
	10/12/14

	Additional information received in response to an informal request sent on 01 April 2015.
	Email confirmation that:
· Activities that agitate waste, i.e. shredding, turning and screening, should not be carried out when the wind blows in an Easterly direction. 
· Activities that agitate waste, i.e. shredding, turning and screening, will be avoided (where possible) when the wind blows in a Southerly direction. 
	07/04/15
















Schedule 2 - Waste types, raw materials and fuels
	Table S2.1 Waste types and quantities for open windrow composting

	Maximum Quantities
The total quantity of waste accepted at the site shall not exceed 13,163 tonnes a year.

	Exclusions
	Wastes which have any of the following characteristics shall not be accepted;
1. Catering waste and other wastes containing animal by products covered by the Animal By-Products Regulations2 (except waste code 02 01 06);
1. Wastes consisting solely or mainly of dusts (except sawdust), powders or loose fibres
1. Hazardous wastes
1. Wastes containing treated wood
1. Wastes containing wood-preserving agents or other biocides
1. Wastes containing persistent organic pollutants
1. Wastes containing or contaminated with Japanese Knotweed
1. Wastes that are in a form of liquid.

	Waste Code
	Description

	[bookmark: _Toc531667060]02
	[bookmark: _Toc531667061]WASTES FROM AGRICULTURE, HORTICULTURE, AQUACULTURE, FORESTRY, HUNTING AND FISHING, FOOD PREPARATION AND PROCESSING

	02 01
	wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing

	02 01 03
	plant-tissue waste

	02 01 06
	animal faeces, urine and manure (including spoiled straw), effluent, collected separately and treated off-site

	02 01 07
	wastes from forestry (consisting of biodegradable only)

	02 01 99 
	wastes not otherwise specified (consisting of either spent mushroom compost only)

	02 03
	wastes from fruit, vegetables, cereals, edible oils, cocoa, coffee, tea and tobacco preparation and processing; conserve production; yeast and yeast extract production, molasses preparation and fermentation

	02 03 04
	materials unsuitable for consumption or processing (consisting of biodegradable only and other than those containing dangerous substances)

	02 07
	wastes from the production of alcoholic and non-alcoholic beverages (except coffee, tea and cocoa)

	02 07 01
	wastes from washing, cleaning and mechanical reduction of raw materials (consisting of spent grains or hops only)

	02 07 02
	wastes from spirits distillation (consisting of whisky filter sheets or cloths only)

	02 07 04
	material unsuitable for consumption or processing (consisting of biodegradable waste only)

	02 07 99
	wastes not otherwise specified (consisting of malt husks, malt sprouts, yeast and yeast-like residues only)

	03
	WASTES FROM WOOD PROCESSING AND THE PRODUCTION OF PANELS AND FURNITURE, PULP, PAPER AND CARDBOARD

	03 01
	wastes from wood processing and the production of panels and furniture

	03 01 01
	waste bark and cork

	03 01 05
	sawdust, shavings, wood, particle board and veneer other than those containing dangerous substances other than 03 01 04 (excluding waste containing veneers or preservatives)

	03 03
	wastes from pulp, paper and cardboard production and processing

	03 03 01
	waste bark and wood

	03 03 10
	fibre rejects, fibre-, filler- and coating-sludges from mechanical separation (consisting of fibre rejects only)

	04
	WASTES FROM THE LEATHER FUR AND TEXTILE INDUSTRIES

	04 02
	waste from the textile industry

	04 02 10
	organic matter from natural products (consisting of un-dyed and untreated only)

	15
	WASTE PACKAGING; ABSORBENTS, WIPING CLOTHS, FILTER MATERIALS AND PROTECTIVE CLOTHING NOT OTHERWISE SPECIFIED

	15 01
	packaging (including separately collected municipal packaging waste) (not containing non-biodegradable veneers or plastics)

	15 01 01
	paper and cardboard packaging (excluding waste containing non-biodegradable veneers or plastics)

	15 01 03
	wooden packaging (consisting of untreated wooden packaging only)

	15 01 05
	composite packaging (consisting of biodegradable organic packaging only)

	15 01 09
	textile packaging (consisting of biodegradable fibres only)

	17
	CONSTRUCTION AND DEMOLITION WASTES (INCLUDING EXCAVATED SOIL FROM CONTAMINATED SITES)

	17 02
	wood, glass and plastic

	17 02 01
	wood (consisting of untreated wood only)

	17 05
	soils (excluding excavated soils from contaminated sites), stones and dredging spoil

	17 05 06
	dredging spoil other than those mentioned in 17 05 05 (consisting of dewatered dredging spoil from inland waters only) 

	19
	WASTES FROM WASTE MANAGEMENT FACILITIES, OFF-SITE WASTE WATER TREATMENT PLANTS AND PREPARATION OF WATER INTENDED FOR HUMAN CONSUMPTION/INDUSTRIAL USE

	19 05
	wastes from the aerobic treatment of solid wastes

	19 05 03
	off-specification compost (consisting only from a process operated according to PAS 100 and QP requirements or another approved standard)

	19 08
	waste from waste water treatment plants

	19 08 05
	sludges from treatment of urban waste water

	19 12
	wastes from the mechanical treatment of waste (for example sorting, crushing, compacting, pelletising) not otherwise specified

	19 12 01
	paper and cardboard (excluding waste containing non-biodegradable veneers or plastics)

	19 12 07
	wood other than that mentioned in 19 12 06 

	20
	MUNICIPAL WASTES (HOUSEHOLD WASTE AND SIMILAR COMMERCIAL, INDUSTRIAL AND INSTITUTIONAL WASTES) INCLUDING SEPARATELY COLLECTED FRACTIONS

	20 01
	separately collected fractions (except 15 01)

	20 01 01 
	paper and cardboard (excluding wastes containing veneers, plastic coatings or laminates) 

	20 02
	garden and park wastes (including cemetery waste)

	20 02 01
	biodegradable waste (consisting of wood and plant tissue only)

	20 03
	other municipal wastes

	20 03 02
	waste from markets (consisting of biodegradable wastes only)




Schedule 3 – Emissions and monitoring
	Table S3.1  Process monitoring requirements 

	Monitoring point 
	Substance or parameter
	Monitoring frequency
	Monitoring method
	Other specifications

	Internal for each windrow and for any sample of waste or compost
	Temperature
	None specified
	Thermocouple probe
	Monitoring equipment shall be available on-site and used as required to ensure compliance with this permit. Equipment shall be calibrated on a 4 monthly basis or as agreed in writing by Natural Resources Wales.

	
	Moisture
	None specified
	Moisture meter or moisture touch test
	



	Table S3.2  Bioaerosol monitoring requirements

	Location or description of point of measurement
	Parameter 
	Bioaerosol threshold limits CFU m-3
	Monitoring frequency 
	Monitoring standard or method 
	Other specifications

	Bioaerosols shall be monitored at:
- nearest sensitive receptor (as highlighted in Schedule 7 – site plan).
- upwind of the site and
- downwind of the site;
in accordance with the Industry Standard Protocol.
	Gram-negative bacteria
	300
	Quarterly
	In accordance with the Industry Standard Protocol, and for gram-negative bacteria, together with the Environment Agency’s “Guidance on the evaluation of bioaerosol risk assessments for composting facilities”. 
	As described in the Industry Standard Protocol, including all the additional data requirements specified therein.

	
	Total bacteria 
	1000 
	
	
	

	
	Aspergillus Fumigatus
	500
	
	
	






Schedule 4 - Reporting
Parameters, for which reports shall be made, in accordance with conditions of this permit, are listed below. 

	Table S4.1 Reporting of monitoring data

	Parameter
	Reporting period
	Period begins

	Bioaerosol monitoring as required by condition 3.5.1(b)
	Every 4 months or as agreed in writing by Natural Resources Wales
	1 January, 
1 May, 
1 September



	Table S4.2 Reporting forms

	Media/parameter
	Reporting format

	Bioaerosol monitoring
	As specified in the Industry Standard Protocol or other form as agreed in writing by Natural Resources Wales 











































Schedule 5 - Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A 
	Permit Number
	

	Name of operator
	

	Location of Facility
	

	Time and date of the detection 
	



	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	



	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	



	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	



Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator




















Schedule 6 - Interpretation 
“accident” means an accident that may result in pollution.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“authorised officer” means any person authorised by Natural Resources Wales under section 108(1) of The Environment Act 1995 to exercise, in accordance with the terms of any such authorisation, any power specified in section 108(4) of that Act.
“bioaerosol threshold limits” means the maximum acceptable bioaerosol concentrations at the nearest sensitive receptor, or at an equivalent distance downwind of the composting operations, which are attributable to the composting operations.  The maximum acceptable concentrations are respectively 300, 1000 and 500 CFU m-3 for gram-negative bacteria, total bacteria and Aspergillus fumigatus. 
“compost” means solid particulate material that is the result of composting, which has been sanitised and stabilised, and which confers beneficial effects when added to soil, used as a component of growing media or used in another way in conjunction with plants.
“composting” means the biological decomposition of organic materials, under conditions that are predominantly aerobic and that allow the development of thermophilic temperatures as a result of biologically produced heat. 
“emissions to land” includes emissions to groundwater.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2010 No.675 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the activities, either from the emission points specified in schedule 3 or from other localised or diffuse sources, which are not controlled by an emission or background concentration limit..
“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.
“groundwater protection zones 1 and 2” have the meaning given in the document titled "Groundwater Protection: Policy and Practice" published by the Environment Agency in 2006.
“hazardous waste” has the meaning given in the Hazardous Waste (England and Wales) Regulations 2005 No.894, the Hazardous Waste (Wales) Regulations 2005 No. 1806 (W.138), the List of Wastes (England) Regulations 2005 No.895 and the List of Wastes (Wales) Regulations 2005 No. 1820 (W.148).
“Industry Standard Protocol” means “A standardised protocol for the monitoring of bioaerosols at open composting facilities” published by the Association for Organics Recycling and developed in conjunction with the Environment Agency
“maturation” means a stage when by  agitating and turning the compost it no longer results in reheating and the monitored temperature falls to ambient without the compost being too dry or anaerobic. Phytotoxins that are formed during the 'active' composting phase are metabolised by micro-organisms, which will result in the final material not being harmful to plants. This usually coincides with drop in pH toward neutral, and the conversion of ammonia into nitrates and recolonisation of beneficial micro-organisms. The maturation phase may need active management by turning to prevent the material becoming anaerobic.
“MCERTS” means the Environment Agency’s Monitoring Certification Scheme.
“nearest sensitive receptor” means the nearest place to the permitted activities where people are likely to be for prolonged periods. This term would therefore apply to dwellings (including any associated gardens) and to many types of workplace. We would not normally regard a place where people are likely to be present for less than 6 hours at one time as being a sensitive receptor. The term does not apply to those controlling the permitted facility, their staff when they are at work or to visitors to the facility as their health is covered by Health and Safety at Work legislation. NB The term would apply to dwellings occupied by the family of those controlling the permitted facility.
“Pests” means Birds, Vermin and Insects.
“quarter” means a calendar year quarter commencing on 1 January, 1 April, 1 July or 1 October.
“R” means a recovery operation provided for in Annex II to Directive 2008/98/EC of the European Parliament and of the Council on waste. 
“Waste code” means the six digit code referable to a type of waste in accordance with the List of Wastes (England)Regulations 2005, or List of Wastes (Wales) Regulations 2005, as appropriate, and in relation to hazardous waste, includes the asterisk. 
“Waste Framework Directive” or “WFD” means Waste Framework Directive 2008/98/EC of the European Parliament and of the Council on waste.
“year” means calendar year ending 31 December.
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