ENVIRONMENTAL RISK ASSESSMENT –SOUTH WALES WOOD RECYCLING LIMITED
ACTIVITY:            Waste Operation: Treatment and Export Waste Wood



KEY ELEMENT:    General site operations



ENVIRONMENTAL PERMIT:  EPR/PB3333DH 


	DATA AND INFORMATION
	JUDGEMENT
	ACTION

	Receptor
	Source
	Harm
	Pathway
	Possibility of Exposure
	Consequence
	Magnitude
	Justification of magnitude
	Risk management
	Residual Risk

	Local human population & local environment 
	Particulate matter (dusts)  release
	Harm to health – respiratory. Irritation and illness
	Air transport then inhalation.

	Low
	Low
	Low
	Permitted wastes do not include dusts, powders or loose fibres
	Referral to EMS. Control via suppression, plant techniques (slow speed shredding), wind direction, weather conditions, waste types
	Low

	Local human population & local environment
	Noise & vibration
	Nuisance, loss of amenity
	Air transmission & vibration through ground
	Low
	Low
	Low
	Sensitivity to excess noise  & vibration
	Referral to EMS. Control via suppression, plant maintenance, regulated operating hours
	Low

	Local human population & local environment 

	Litter
	Nuisance, loss of amenity – harm to animals and polluted environment
	Air transport and then deposition
	Medium
	Medium
	Medium
	Sensitive to litter
	Referral to EMS. 
Limited waste types accepted.
Control via wind direction & weather conditions, waste types
Good housekeeping 
	Low

	Local human population & local environment 
	Dust,

Fugitive emissions
	Nuisance
	Air transport then
deposition
	Medium
	Low
	Low
	Sensitive to dust
	Referral to EMS. Control via suppression, plant techniques (slow speed shredding) wind direction, weather conditions, waste types
	Low


	DATA AND INFORMATION
	JUDGEMENT
	ACTION

	Receptor
	Source
	Harm
	Pathway
	Possibility of Exposure
	Consequence
	Magnitude
	Justification of magnitude
	Risk management
	Residual Risk

	Local human population
	Wastes on local roads
	Nuisance, loss of amenity, road traffic accidents
	Vehicles using site
	Low
	Low
	Low
	Sensitivity to excess mud / wood chip on road, road safety 
	Referral to EMS. Control via waste discharge from source site, clearing up 
	Low

	Local human population 


	Odour
	Nuisance, loss of amenity
	Air transport then

inhalation
	Low
	Low
	Low
	Sensitivity to odour, smells
	Referral to EMS. Control via suppression, wind direction, weather conditions, waste types
	Low

	Local human population 


	Scavengers (animals,    birds) & pests (flies)
	Harm to human health, Nuisance, loss of amenity


	Air transport then

Over land
	Low
	Low
	Low
	Permitted wastes not known to attract scavengers etc
	Referral to EMS. Control  via waste types, access to waste restricted, limited storage periods

	Low


	DATA AND INFORMATION
	JUDGEMENT
	ACTION

	Receptor
	Source
	Harm
	Pathway
	Possibility of Exposure
	Consequence
	Magnitude
	Justification of magnitude
	Risk management
	Residual Risk

	Local human population & local environment
	Accidental fire
	Nuisance, loss of amenity, road traffic accidents
	Vehicles using site
	Medium
	High
	Medium
	Sensitivity to excess mud on road, road safety 
	Referral to EMS. Control via waste discharge, plant maintenance, clearing up, fire prevention system installed on machines, staff training, stock rotation 
	Low

	Surface waters and downstream of site

	Spillage
	Contaminant/pollutant
	Groundwater
	Low
	Low
	Low
	All surface water from stockpile or operational area contained in a sealed sump and either recycled or tanked off site.
	Clean infiltration only to soak away drainage. Potentially contaminated surface water collected in sealed sump prior to recycling  and/or off site disposal, Spillage control procedures. Plant maintenance.
	Low

	Ground - water

	Spillage
	Nuisance, loss of amenity
	Air transport then

Inhalation

	Medium
	Medium
	Medium
	Sensitivity to odour, smells
	Referral to EMS. Control via suppression, wind direction, weather conditions, waste types

	Low

	NOISE and VIBRATION MANAGEMENT PLAN
TROMMEL/SCREENING, CHIPPING & SITE ACTIVITIES

	Hazard
	Receptor
	Pathway
	Probability of Exposure
	Consequence
	Overall risk
	Risk management
	Residual Risk

	Warning noise from reversing bleepers -  H&S requirement
	Local human population
	Air transmission
	Daily 
	Intermittent  disturbance –

Low 
	Insignificant on correct management -  

Low
	Only used during regulated site operations,  vehicles maintained as supplier instructions
	Low

	Engine noise and vibration from site plant
	Local human population
	Air transmission & vibration through ground
	Daily
	Intermittent  disturbance –

Low 
	Insignificant on correct management -  
Low
	Only used during regulated site operations, vehicles maintained as supplier instructions,

Rubber wheeled plant and thus no track noise
	Low

	Noise and vibration from site screening & chipping activities 
	Local human population
	Air transmission
	Monthly
	Intermittent  disturbance –
Medium
	Insignificant on correct management -  
Low
	Only used during regulated site operations, maintained as supplier instructions,

Records taken and  any adverse events notified
Partly enclosed process, care on loading hopper assembly.


	Low
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Action: 1. Nominated personnel:








2. Target date:




