RISK ASSESSMENT – SWWR
ACTIVITY:          Workplace (Health, Safety & Welfare)
PERFORMED:  
JANUARY 2011
KEY ELEMENT: Movement of vehicles, Alexandra Docks
ASSESSOR: 
P. Rees

REVIEW DATE:  1/12, 10/12, 11/13, 11/14

	
	CATEGORY OR TASK
	WHO AT RISK
	HAZARD IDENTIFICATION
	HAZARD RATING (HR)
	CURRENT RISK CONTROL MEASURES
	FURTHER ACTION TO CONTROL RISK
	NEW (HR)

	A
	Use of vehicles and site plant
	Drivers

Operatives

Pedestrians

Site users 
	Damage

Contact

Injury

Fatality 
	H


	Ensure vehicle is fit for purpose and can access discharge area safely.

Ensure vehicle is in good condition and that reversing aids are operational.

Drivers to be competent to perform tasks.

Display site rules/signage and inform site users
	Maintain good visibility e.g. mirrors/CCTV/bleepers etc.

Regular vehicle inspection and examination.

Obtain copy of driver training records.


	L


	B
	Reversing


	Drivers

Operatives

Pedestrians

Site users
	Damage

Contact

Injury

Fatality
	H
	Ensure reversing aids are in use.

Maintain a safe operating distance between plant/personnel.

Use of PPE & HV

Restrict number of vehicles in discharge area.

Use trained reversing assistant/banksman

Signals displayed and drivers awareness
	Inspection/defect form used to record.

Monitor the number of vehicles at the discharge point/area.

Management to monitor
	M


	C
	Site conditions & Site use

	Drivers

Operatives

Pedestrians

Site users
	Damage

Contact

Injury

Fatality
	H


	Dedicated Pedestrian  routes & signage

Adequate turning area for vehicles
Site surface to be suitable for vehicle access and movement, and level as appropriate.

Use of PPE & HV
	Management to monitor.

Regular site inspection and maintenance of roadways to ensure good traction. 

Maintain site signage & monitor use
	M

	D
	Unsheeting


	Drivers

Operatives

Site users
	Injury

Fall from height
	H
	Unsheet in safe area by authorised method,     use auto-sheeting if   available.

 Use gantry if available.

Maintain auto-sheet mechanism
	Management to monitor
Use safety harness if required and attach to secure point.
	L
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Action: 1. Nominated personnel:








2. Target date:




