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1. Weather data
1.1 Site Op Data (using Kestrel 5500)
	Location (see plan for locations)
	Weather conditions
	Time
	Wind direction
	Wind speed (MPH)
	Temperature (˚C)

	SP1–Downwind IVC
	Sunny/Hot
	11:02
	E
	1.7
	26

	SP2- Upwind IVC
	Sunny/Hot
	11:18
	SSW
	1.2
	23

	SP3-Downwind MBT
	Sunny/Hot
	11:55
	SSW
	1.1
	27.9

	SP4-Upwind MBT
	Sunny/Hot
	12:02
	SSW
	0.7
	30.1
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1.2 Weather station data
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2. Site activities

	Site 
(IVC/TS/MRF/MBT)
	Activity
	Waste stream
	Tonnages

	MBT
	Pre-treatment shredding
	MSW
	173.12

	MBT
	Bio-drying Tunnel 1 – phase 8
	RDF
	404.19

	MBT
	Bio-drying Tunnel 2 – phase 8
	RDF
	401.1

	MBT
	Bio-drying Tunnel 3 – phase 8
	RDF
	371.5

	MBT
	Bio-drying Tunnel 4 – Empting
	RDF
	402.94

	MBT
	Bio-drying Tunnel 5 – phase 8
	RDF
	410.71

	MBT
	RDF dispatch
	RDF
	171

	MRF
	Baling
	Ali Cans
	1

	MRF
	Baling
	Steel cans
	2

	MRF
	Baling
	Plastics/Card
	No baling 

	IVC
	Tunnel’s 1,2,3,4,6 Hygenise
	Green 
	1000

	IVC 
	Mulch dispatch
	Mulch
	100













3. Bio filter data

3.1.  Phase 1 








[image: ]































3.2.  Phase 2 
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3.3.  Moisture data

Phase1
Filter 1 = 66%
Filter 2 = 62%
Phase 2
Filter 1 = 58%
Filter 2 = 68%
4. Site Observations
Phase1
No Shredding due to mechanical issues or screening in dispatch during the monitoring. 
Phase 2
Emptying of Tunnel 4 during the monitoring and shredding in pre-treatment. During monitoring at SP3 2 vehicles drove past delivering waste to site. At 12:16 reception door openend for vehicle tipping
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