Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	BOD is tested off site by an external laboratory.
Due to incubation times the results are always a week behind, and gives us little chance to correct any issues.

27.07.15

BOD -  53mg/l (limit 50mg/l)

03.08.15

BOD -  69mg/l (limit 50mg/l)



	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	ETP parameters checked and monitored

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	We will investigate carrying out more in depth testing on site in 2016, and will still employ the external laboratory so that we can compare results.



	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	10.02.14, 07.04.14, 02.02.2015, 27.02.2015, 28.05.2015, 01.06.2015, 27.07.15, 03.08.15


	Name*
	Mike King

	Post
	Safety Specialist / Environmental Leader

	Signature
	

	Date
	30th December 2015


* authorised to sign on behalf of the operator

