Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	BV3715IL

	Name of operator
	SCA Hygiene UK Ltd

	Location of Facility
	Chester Road, Oakenholt, Flintshire, CH6 5PU

	Time and date of the detection 
	Result from 01 June 2015


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	01 June 2015

	Reference or description of the location of the event 
	BOD W1 emission point

	Description of where any release into the environment took place
	W1 emission point

	Substances(s) potentially released
	Final effluent with an elevated BOD of 80mg/l (over 50mg/l permit limit)

	Best estimate of the quantity or rate of  release of substances
	Continuous flow to estuary (approx. 1700m3 a day)

	Measures taken, or intended to be taken, to stop any emission
	None taken – results received from external laboratory 11.06.2015

	Description of the failure or accident.
	Elevated BOD


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	W1 

	Parameter(s)
	BOD

	Limit
	<50mg/l

	Measured value and uncertainty
	80mh/l

	Date and time of monitoring
	01 June 2015

	Measures taken, or intended to be taken, to stop the emission
	None taken – results received from external laboratory 11.06.2015


	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	None anticipated.  Overspill from the reservoir.  Final effluent is being blended with the overspill.

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


