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Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY
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	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
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Permit Number: 	BP3635MR				Operator: 		Harsco Metals Limited

Facility:		Port Talbot Steelworks		Form Number: 	Performance1 / 01/10/17

Reporting of particulates for the period from DD/MM/YYYY to DD/MM/YYYY 

	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	AS3
	Particulate Matter
	20 mg/m3
	Spot Sample
	
	BS EN 13284-1
	
	




[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

