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Permit with introductory note
The Environmental Permitting (England & Wales) Regulations 2016


Maelor Foods Limited

Maelor Poultry Processing Plant
Pickhill Lane
Cross Lanes
Wrexham
LL13 0UE



Permit number
EPR/AB3591ZQ

Maelor Poultry Processing Plant
Permit number EPR/AB3591ZQ
Introductory note
This introductory note does not form a part of the permit
The main features of the permit are as follows.  
This installation is located approximately 4km south east from Wrexham and is permitted for the slaughtering of poultry and meat preparation as well as associated waste effluent treatment. The permitted throughput being 1 million birds per week.
Live birds are delivered to the site in “modules” on HGV lorry trailers. They are unloaded, remaining in the modules into the lairage area.  They are then passed into the gas stunning area and are killed, bled, scalded, de-feathered, eviscerated and chilled.
Some birds are packaged for despatch to retail at this stage while the remaining birds pass to the meat processing part of the installation where the products are packaged for dispatch. In the meat processing part of the plant, whole birds will be cut into various portions on automated and manual processing lines, and packaged for dispatch.
The blood tank is emptied and cleaned daily to reduce odour generation. Animal by-products and feathers are stored in trailers within an enclosed building and removed daily. The air from this storage area, the blood tank and de-feathering process is passed through a scrubber to reduce odours before being released from the elevated stack.
Modules and vehicles are washed before leaving the site.
Wash down waters and process effluents flow to the on site effluent treatment plant before being treated and discharged to the River Dee (Approximately half of the treated water is returned to the installation for vehicle and module washing).
Hot water for the process is provided by small scale on site boilers.

The status log of the permit sets out the permitting history, including any changes to the permit reference number.

	Status log of the permit

	Description
	Date
	Comments

	Application PAN-001271

	Duly made 07/02/17
	Application for poultry slaughterhouse, meat processing and effluent treatment

	Additional information requested
	20/03/17
	

	Additional information requested
	07/04/17
	

	Additional information received
	19/04/17
	Further data on odour modelling figures used, odour controls and procedures

	Additional information received
	26/04/17
	Updated Installation plan and further applicable information

	Additional information received
	05/06/17
	Additional information relating to containment, odour control and monitoring at the effluent treatment plant

	Additional information received
	14/07/17
	Layout plan, details of new boilers, H1 assessment

	Permit determined
	29/08/17
	Permit issued to Maelor Food Limited




End of introductory note
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Permit


The Environmental Permitting (England and Wales) Regulations 2016

Permit number 
EPR/AB3591ZQ
The Natural Resources Body for Wales (“Natural Resources Wales”)  authorises, under regulation 13 of the Environmental Permitting (England and Wales) Regulations 2016 
[bookmark: OperatorName2]
Maelor Foods Limited (“the operator”),
whose registered office is
[bookmark: InstallationAddress21]
Salisbury House
Vulcan Road
Bilston
West Midlands
WV14 7HT

company registration number 09156025 
to operate an installation at
 
Maelor Poultry Processing Plant
Pickhill Lane
Cross Lanes
Wrexham
LL13 0UE

to the extent authorised by and subject to the conditions of this permit.

	Signed
	Date

	

	29/08/2017


Iwan Hughes
Technical Specialist, Permitting Service (Regulated Industry)
Authorised on behalf of Natural Resources Wales


Conditions 
1 Management
1.1 General management
1.1.1 The operator shall manage and operate the activities:
(a) in accordance with a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances, closure and those drawn to the attention of the operator as a result of complaints; and
(b) using sufficient competent persons and resources.
1.1.2 Records demonstrating compliance with condition 1.1.1 shall be maintained. 
1.1.3 Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of it kept at or near the place where those duties are carried out.

1.2	Energy efficiency
1.2.1	The operator shall:
(a)	take appropriate measures to ensure that energy is used efficiently in the activities;
 (b)	review and record at least every four years whether there are suitable opportunities to improve the energy efficiency of the activities; and  
(c)	take any further appropriate measures identified by a review. 
1.3	Efficient use of raw materials
1.3.1	The operator shall:
(a)	take appropriate measures to ensure that raw materials and water are used efficiently in the activities; 
(b)	maintain records of raw materials and water used in the activities;
(c)	review and record at least every four years whether there are suitable alternative materials that could reduce environmental impact or opportunities to improve the efficiency of raw material and water use; and
(d)	take any further appropriate measures identified by a review.
1.4	Avoidance, recovery and disposal of wastes produced by the activities
1.4.1 The operator shall take appropriate measures to ensure that:
(a)	the waste hierarchy referred to in Article 4 of the Waste Framework Directive is applied  to the generation of  waste by the activities; and
(b)	any waste generated by the activities is treated in accordance with the waste hierarchy referred to in Article 4 of the Waste Framework Directive; and
(c)	where disposal is necessary, this is undertaken in a manner which minimises its impact on the environment.
1.4.2 The operator shall review and record at least every four years whether changes to those measures should be made and take any further appropriate measures identified by a review.


2	Operations
2.1	Permitted activities
2.1.1	The operator is only authorised to carry out the activities specified in schedule 1 table S1.1 (the “activities”). 
2.2	The site 
2.2.1	The activities shall not extend beyond the site, being the land shown edged in green on the site plan at schedule 7 to this permit.
2.3	Operating techniques
2.3.1	(a) 	The activities shall, subject to the conditions of this permit, be operated using the 
		techniques and in the manner described in the documentation specified in 	schedule 1, table S1.2, unless otherwise agreed in writing by Natural Resources Wales.		
(b)	If notified by Natural Resources Wales that the activities are giving rise to pollution, the operator shall submit to Natural Resources Wales for approval within the period specified, a revision of any plan or other documentation (“plan”) specified in schedule 1, table S1.2 or otherwise required under this permit which identifies and minimises the risks of pollution relevant to that plan , and shall implement the approved revised plan in place of the original from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
2.3.2	Any raw materials or fuels listed in schedule 2 table S2.1 shall conform to the specifications set out in that table.
2.3.4	The operator shall ensure that where waste produced by the activities is sent to a relevant waste operation, that operation is provided with the following information, prior to the receipt of the waste:
	(a)	the nature of the process producing the waste;
	(b)	the composition of the waste;
	(c)	the handling requirements of the waste;
	(d)	the hazardous property associated with the waste, if applicable; and
	(e)	the waste code of the waste.
2.3.5	The operator shall ensure that where waste produced by the activities is sent to a landfill site, it meets the waste acceptance criteria for that landfill.

2.4	Improvement programme
2.4.1 	The operator shall complete the improvements specified in schedule 1 table S1.3 by the date specified in that table unless otherwise agreed in writing by Natural Resources Wales.
2.4.2	Except in the case of an improvement which consists only of a submission to Natural Resources Wales, the operator shall notify Natural Resources Wales within 14 days of completion of each improvement.

2.5	Pre-operational conditions
2.5.1	The activities shall not be brought into operation until the measures specified in schedule 1 table S1.4A have been completed.

3	Emissions and monitoring
3.1	Emissions to water, air or land
3.1.1	There shall be no point source emissions to water, air or land except from the sources and emission points listed in schedule 3 tables S3.1 and S3.2.
3.1.2	The limits given in schedule 3 shall not be exceeded.
3.1.3 Periodic monitoring shall be carried out at least once every 5 years for groundwater and 10 years for soil, unless such monitoring is based on a systematic appraisal of the risk of contamination.

3.2 Emissions of substances not controlled by emission limits
3.2.1 Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.
3.2.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution, submit to Natural Resources Wales for approval within the period specified, an emissions management plan which identifies and minimises the risks of pollution from emissions of substances not controlled by emission limits;
(b)	implement the approved emissions management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.2.3	All liquids in containers, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the operator has used other appropriate measures to prevent or where that is not practicable, to minimise, leakage and spillage from the primary container.
3.3	Odour
3.3.1	Emissions from the activities shall be free from odour at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved odour management plan, to prevent or where that is not practicable to minimise the odour. 
3.3.3	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to odour, submit to Natural Resources Wales for approval within the period specified, an odour management plan which identifies and minimises the  risks of pollution from odour;
(b)	implement the approved odour management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.

3.4	Noise and vibration
3.4.1	Emissions from the activities shall be free from noise and vibration at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved noise and vibration management plan to prevent or where that is not practicable to minimise the noise and vibration.
3.4.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to noise and vibration, submit to Natural Resources Wales for approval within the period specified, a noise and vibration management plan which identifies and minimises the risks of pollution from noise and vibration;
(b)	implement the approved noise and vibration management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
.
3.5	Pests
3.5.1 	The activities shall not give rise to the presence of pests which are likely to cause pollution, hazard or annoyance outside the boundary of the site. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved pests management plan, have been taken to prevent or where that is not practicable, to minimise the presence of pests on the site.  

3.5.2 	The operator shall:             
(a)           if notified by Natural Resources Wales, submit to Natural Resources Wales for approval within the period specified, a pests management plan which identifies and minimises risks of pollution, hazard or annoyance from pests;
(b)          implement the pests management plan, from the date of approval, unless    otherwise agreed in writing by Natural resources Wales.


[bookmark: _Toc449070323]3.6	Monitoring 
3.6.1	The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring specified in the following tables in schedule 3 to this permit:
(a) point source emissions specified in tables S3.1 and S3.2;
3.6.2	The operator shall maintain records of all monitoring required by this permit including records of the taking and analysis of samples, instrument measurements (periodic and continual), calibrations, examinations, tests and surveys and any assessment or evaluation made on the basis of such data.
3.6.3	Monitoring equipment, techniques, personnel and organisations employed for the emissions monitoring programme and the environmental or other monitoring specified in condition 3.3.1 shall have either MCERTS certification or MCERTS accreditation (as appropriate), where available, unless otherwise agreed in writing by Natural Resources Wales. 
3.6.4	Permanent means of access shall be provided to enable sampling/monitoring to be carried out in relation to the emission points specified in schedule 3 tables S3.1 and S3.2 unless otherwise agreed in writing by Natural Resources Wales.
[bookmark: _Toc77056949][bookmark: _Toc457192259]4	Information
4.1	Records
4.1.1 All records required to be made by this permit shall:
(a) be legible;
(b) be made as soon as reasonably practicable;
(c) if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
(d) be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made, or in the case of the following records until permit surrender:
(i) off-site environmental effects; and
(ii) matters which affect the condition of the land and groundwater.
4.1.2	The operator shall keep on site all records, plans and the management system required to be maintained by this permit, unless otherwise agreed in writing by Natural Resources Wales. 
4.2	Reporting
4.2.1	The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
4.2.2	A report or reports on the performance of the activities over the previous year shall be submitted to Natural Resources Wales by 31 January (or other date agreed in writing by Natural Resources Wales) each year.  The report(s) shall include as a minimum:
(a)	a review of the results of the monitoring and assessment carried out in accordance with the permit including an interpretive review of that data; 
(b)	the annual production/treatment data set out in schedule 4 table S4.2; and
(c)	the performance parameters set out in schedule 4 table S4.3 using the forms specified in table S4.4 of that schedule.
4.2.3	Within 28 days of the end of the reporting period the operator shall, unless otherwise agreed in writing by Natural Resources Wales, submit reports of the monitoring and assessment carried out in accordance with the conditions of this permit, as follows:
(a)	in respect of the parameters and emission points specified in schedule 4 table S4.1;
(b)	for the reporting periods specified in schedule 4 table S4.1 and using the forms specified in schedule 4 table S4.4 ; and
(c)	giving the information from such results and assessments as may be required by the forms specified in those tables.
4.2.4	The operator shall, unless notice under this condition has been served within the preceding four years, submit to Natural Resources Wales, within six months of receipt of a written notice, a report assessing whether there are other appropriate measures that could be taken to prevent, or where that is not practicable, to minimise pollution.

4.3	Notifications
4.3.1	(a)	In the event that the operation of the activities gives rise to an incident or accident which significantly affects or may significantly affect the environment, the operator must immediately
(i)	inform Natural Resources Wales, 
(ii)	take the measures necessary to limit the environmental consequences of such an incident or accident, and
(iii)	take the measures necessary to prevent further possible incidents or accidents;
(b)	in the event of a breach of any permit condition the operator must immediately
(i)	inform Natural Resources Wales, and
(ii)	take the measures necessary to ensure that compliance is restored within the shortest possible time;
(c)	in the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment, the operator must immediately suspend the operation of the activities or the relevant part of it until compliance with the permit conditions has been restored.
4.3.2	Any information provided under condition 4.3. shall be confirmed by sending the information listed in schedule 5 to this permit within the time period specified in that  schedule.
4.3.3	Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.
4.3.4	Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules: 
Where the operator is a registered company:
(a) any change in the operator’s trading name, registered name or registered office address; and
(b)	any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and
(b) any steps taken with a view to the dissolution of the operator.
		In any other case: 
(a) the death of any of the named operators (where the operator consists of more than one named individual);
(b)         any change in the operator’s name(s) or address(es); and
(c) any steps taken with a view to the operator, or any one of them, going into bankruptcy, entering into a composition or arrangement with creditors, or, in the case of them being in a partnership, dissolving the partnership.
4.3.5	Where the operator proposes to make a change in the nature or functioning, or an extension of the activities, which may have consequences for the environment and the change is not otherwise the subject of an application for approval under the Regulations or this permit:
(a) Natural Resources Wales shall be notified at least 14 days before making the change; and
(b) the notification shall contain a description of the proposed change in operation.
4.3.6	Natural Resources Wales shall be given at least 14 days notice before implementation of any part of the site closure plan.
4.3.7	Where the operator has entered into a climate change agreement with the Government, Natural Resources Wales shall be notified within one month of:
(a)	a decision by the Secretary of State not to re-certify the agreement;
(b)	a decision by either the operator or the Secretary of State to terminate the agreement; and
(c)	any subsequent decision by the Secretary of State to re-certify such an agreement.


 4.4	Interpretation
4.4.1	In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
4.4.2	In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “without delay”, in which case it may be provided by telephone. 
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	Table S1.1 activities

	Activity listed in Schedule 1 of the EP Regulations 
	Description of specified activity 
	Limits of specified activity 

	S6.8 A1 (b)
	Slaughtering of animals at a plant with a carcass production capacity of more than 50 tonnes per day
	From receipt of live chickens to delivery of carcasses for meat processing. Limited to 1 million birds per week.

	S6.8 A1 (d)(i)
	Treating and processing of animal raw materials intended for the production of food with a finished product production capacity of more than 75 tonnes per day.
	From receipt of carcasses to dispatch of final products. Limited to 158 Tonnes per day.

	S5.4 A1 (a)(i)
	Disposal of non hazardous waste in a facility with a capacity of more than 50 tonnes per day by biological treatment.
	Biological treatment of effluent produced within the site through to discharge of treated effluent to the River Dee. Limited to 1,500m3 per day.

	Directly Associated Activities

	Odour abatement plant
	Chemical scrubber treating air extracted from odorous parts of the S6.8 A1 (b) process.
	From extraction of air to release of air to atmosphere via exhaust stack.

	Chemical storage
	Storage of chemicals for use on site
	Temporary storage of chemicals necessary for operation of the installation.

	Refrigeration plants
	Chilling of carcasses and processed meats
	From receipt of slaughtered birds to despatch of final products

	Water heating
	Burning fuel in a combustion plant to heat water.
	Heating of water in four gas  fired boilers, three with capacities of 1.1MW and one with a capacity of 0.38MW

	Waste arisings handling and storage
	Temporary storage of wastes on site prior to removal.
	From production of waste to removal from site.









	Table S1.2 Operating techniques

	Description
	Parts
	Date Received

	Application 
PAN-001271
	Part B2 and B3 of the application and all referenced supporting documents.


	07/02/17

	Application 
PAN-001271
	Pre-Operational Odour management Plan
	07/02/17

	Additional information 
	Section 2 Installation Plan
	26/04/17

	Response to Schedule 5 Notice dated 20/03/17
	Responses to schedule 5 Notice questions
	19/04/17

	Response to Schedule 5 Notice dated 07/04/17
	Responses to schedule 5 Notice questions
	19/04/17

	Additional information
	Additional information relating to containment, odour control and monitoring at the effluent treatment plant 
	05/06/17

	Additional Information
	Additional information relating to gas fired boilers to be installed on site
	14/07/17




	Table S1.3 Improvement programme requirements

	Reference
	Requirement
	Date

	IC1
	The operator shall inform Natural Resources Wales of the date of commencement of activity type S6.8 A1 (b)
	Within 7 days of commencement of activity S6.8 A1 (b)

	IC2
	The Operator shall undertake an operational olfactometry survey of all potentially odorous release points from the installation. The survey should quantify the odour emissions and their offensiveness once the site is fully operational and odours have become established. The survey shall include an assessment of the efficiency of the odour abatement plant.

The results of the survey shall be used to review the odour impact assessment for the installation.

A report on the olfactometry survey and odour impact assessment shall be sent to NRW for approval and shall include proposals, with timescales, for further improvements to reduce odours if the assessment identifies potentially significant offsite odour concentrations at sensitive receptors.
	Within six months from the commencement of activity type S6.8 A1 (b)

	IC3
	Upon completion of IC2 the Operator shall review the odour management plan and submit to NRW
	Within three months from the completion of IC2 above







	Table S1.4A   Pre-operational measures

	Reference
	Pre-operational measures

	PO1
	The Operator shall submit a written report to Natural Resources Wales on the implementation of its Environmental Management System prior to commencement of activity type S6.8 A1 (b)

	PO2
	The operator shall submit to Natural Resources Wales an updated site drainage plan, showing the as built site drainage and containment for all surface water and effluent drainage prior to commencement of activity type S6.8 A1 (b)







Schedule 2 - Waste types, raw materials and fuels

	Table S2.1 Raw materials and fuels
	

	Raw materials and fuel description 
	Specification

	None set
	None Set










Permit Number   EPR/AB3591ZQ  Page 1	
Schedule 3 – Emissions and monitoring.

	
	Table S3.1  Point source emissions to air – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter
	Limit (including unit) 
	Reference period
	Monitoring frequency
	Monitoring standard or method

	A1 to A4 as shown on site plan in Schedule 7
	Boiler Plant, Rehema P200 series boiler exhausts (556Kw combined thermal input)
	No parameter set
	No limit set
	N/A
	N/A
	N/A

	A5 as shown on site plan in Schedule 7
	Chemical scrubber
	No parameter set
	No limit set
	N/A
	N/A
	N/A

	High velocity roof fans outlets located on the lairage room roof
	High velocity roof fans
	No parameters set
	No limit set
	N/A
	N/A
	N/A

	Air outlet from the DAF plant emission vent 
	DAF clarifier emission vent (after passing through activated carbon filter)
	No parameters set
	No limit set
	N/A
	N/A
	N/A

	Air outlet from sludge tank
	Sludge tank emission vent (after passing through activated carbon filter)
	No parameters set
	No limit set
	N/A
	N/A
	N/A



	
	Table S3.2 Point Source emissions to water (other than sewer) and land – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter  
	Limit (incl. unit)
	Reference Period
	Monitoring frequency
	Monitoring standard or method

	W1 on site plan in schedule 7 emission to River Dee
	Effluent Treatment Plant, treated effluent
	Maximum daily volume
	1,500 m3 per day
	Daily
	Continuous flow monitoring
	MCERTS

	
	
	Mean daily volume
	1,200 m3 per day
	Per annum
	Continuous flow monitoring
	MCERTS

	
	
	Biological Oxygen Demand
	20 mg/l
	Flow proportional daily composite
	Weekly (unless otherwise agreed in writing with NRW)
	BS EN 1899-1

	
	
	Total suspended solids
	30 mg/l
	
	
	BS EN 872:2005

	
	
	Ammonia as N
	5 mg/l
	
	
	BS EN 11732:2005

	
	
	Phosphate as P
	2.5 mg/l
	
	
	BS EN ISO 15681-1:2004

	
	
	pH range minimum to maximum
	6 to 9
	Continuous
	Continuous
	MCERTS

	
	
	Temperature
	30OC
	Continuous
	Continuous
	Standard Temperature sensor

	
	
	Visible oil and grease
	None visible
	Instantaneous
	Weekly
	Visual

	W2 on site plan in schedule 7 emission to drainage ditch, leading to River Dee

	Uncontaminated surface water run off from clean yards and roofes
	Visible oil and grease
	
	None visible
	Instantaneous
	Weekly
	Visual

	W3 on site plan in schedule 7 emission to Drainage ditch, leading to River Dee

	Uncontaminated surface water run off from clean yards and roofes
	Visible oil and grease
	None visible
	Instantaneous
	Weekly
	Visual






Schedule 4 - Reporting
Parameters, for which reports shall be made, in accordance with conditions of this permit, are listed below.

	Table S4.1 Reporting of monitoring data

	Parameter
	Emission or monitoring point/reference
	Reporting period
	Period begins

	Emissions to air
Parameters as required by condition 3.6.1
	None
	None
	N/A

	Emissions to water 
Parameters as required by condition 3.6.1
	W1

	Every 3 months

	1 January



	Table S4.2: Annual production/treatment
	

	Parameter 
	Units 

	Number of chickens slaughtered per week
	Number (maximum week in reporting year)

	Chicken Products produced per week
	Tonnes (maximum week in reporting year)



	Table S4.3 Performance parameters

	Parameter
	Frequency of assessment
	Units

	Water usage per bird
	Annually
	Litres/bird

	Energy usage per bird
	Annually
	KWh/Bird



	Table S4.4 Reporting forms

	Media/parameter
	Reporting format
	Date of form

	Water 
	Form water 1 or other form as agreed in writing by Natural Resources Wales
	29/08/17

	Water usage
	Form water usage 1 or other form as agreed in writing by Natural Resources Wales
	29/08/17

	Energy usage
	Form energy 1 or other form as agreed in writing by Natural Resources Wales
	29/08/17

	Other performance indicators
	Form performance 1 or other form as agreed in writing by Natural Resources Wales
	29/08/17


Schedule 5 - Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A 
	Permit Number
	

	Name of operator
	

	Location of Facility
	

	Time and date of the detection 
	



	(a) Notification requirements for any activity that gives rise to an incident or accident which significantly affects or may significantly affect the environment

	To be notified Immediately

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



	(b) Notification requirements for the breach of a permit condition

	To be notified immediately

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	



	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	



	(c) In the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment:

	To be notified immediately

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator



Schedule 6 - Interpretation 
“accident” means an accident that may result in pollution.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“authorised officer” means any person authorised by Natural Resources Wales under section 108(1) of The Environment Act 1995 to exercise, in accordance with the terms of any such authorisation, any power specified in section 108(4) of that Act.
“disposal” means any of the operations provided for in Annex IIA to Directive 2006/12/EC of the European Parliament and of the Council of 5 April 2006 on Waste.
“emissions to land” includes emissions to groundwater.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.1154 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the activities, either from the emission points specified in schedule 3 or from other localised or diffuse sources, which are not controlled by an emission or background concentration limit..
“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.
“Industrial Emissions Directive” means DIRECTIVE 2010/75/EU OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 24 November 2010 on industrial emissions
“MCERTS” means the Environment Agency’s Monitoring Certification Scheme.
“pests” means Birds, Vermin and Insects.
“quarter” means a calendar year quarter commencing on 1 January, 1 April, 1 July or 1 October.
“quarterly” for reporting/sampling means after/during each 3 month period, January to March; April to June; July to September and October to December and, when sampling, with at least 2 months between each sampling date.
“recovery” means any of the operations provided for in Annex II to Directive 2008/98/EC of the European Parliament and of the Council on waste. 
Where a minimum limit is set for any emission parameter, for example pH, reference to exceeding the limit shall mean that the parameter shall not be less than that limit.
Unless otherwise stated, any references in this permit to concentrations of substances in emissions into air means:
in relation to emissions from combustion processes, the concentration in dry air at a temperature of 273K, at a pressure of 101.3 kPa and with an oxygen content of 3% dry for liquid and gaseous fuels, 6% dry for solid fuels; and/or
in relation to emissions from non-combustion sources, the concentration at a temperature of 273K and at a pressure of 101.3 kPa, with no correction for water vapour content
“year” means calendar year ending 31 December.
Schedule 7 - Site plan
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END OF PERMIT
Permit Number: 	AB3591ZQ						Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant			Form Number: 	Water1 / 29/08/17
Reporting of emissions to water (other than to sewer) for the period from                         to      
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1
	Flow/volume
	1,500 m3 per day
	Daily
	
	MCERTS
	
	

	W1
	Flow/volume
	1,200 m3 per day
	Per annum (mean daily volume)
	
	MCERTS
	
	

	W1
	Temperature
	30OC
	Continuous
	
	Standard Temperature sensor
	
	

	W1
	Total suspended solids
	30 mg/l
	24-hour flow proportional sample
	
	BS EN 872
	
	

	W1
	Ammonia 
	5 mg/l
	24-hour flow proportional sample
	
	BS EN 11732:2005
	
	

	W1
	Phosphate
	2.5 mg/l
	24-hour flow proportional sample
	
	BS EN ISO 15681-1:2004
	
	

	W1
	pH
	6-9
	Continuous
	
	MCERTS
	
	

	W1
	BOD
	20 mg/l
	24-hour flow proportional sample
	
	BS EN 1899-1 (1998)
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)

 
Permit Number: 	AB3591ZQ					Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant		Form Number: 	WaterUsage1 / 29/08/17

Reporting of Water Usage for the year:

	Water Source
	Specific Usage 
(litres/bird)
	

	
	
	

	
	
	

	Mains water
	
	

	Site borehole
	
	

	Other
	
	

	
	
	

	
	
	

	TOTAL WATER USAGE
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)

Permit Number: 	AB3591ZQ					Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant		Form Number: 	Energy1 / 29/08/17

Reporting of Energy Usage for the year:

	
Energy Source
	Energy Usage	
	

	
	
Quantity
	Specific Usage
(KWh/bird)
	

	
	
	
	

	
	
	
	

	
	
	
	

	Electricity *
	
	
	

	Natural Gas
	
	
	

	Gas Oil
	
	
	

	Recovered Fuel Oil
	
	
	

	
	
	
	

	TOTAL
	
	
	

	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	AB3591ZQ					Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant		Form Number: 	Performance1 / 29/08/17

Reporting of other performance indicators for the period                                      to 

	Parameter
	
	Units 
	Result
	

	
	
	
	
	

	Number of chickens slaughtered per week
	Number per week (maximum week in reporting year)
	
	

	Chicken Products produced per week
	Tonnes per week (maximum week in reporting year)
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
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