Schedule 5 – Notification

This page outlines the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.
Part A 

	Permit Number
	EPR/AP3739KS

	Name of Operator
	Flintshire County Council Waste Management Service.

	Location of Installation
	Brookhill Landfill Site, Pinfold Way, Buckley. CH7 3PL.

	
	

	Time and date of the detection
	14:00 hrs 31st October 2016


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, fugitive emission which has caused, is causing or may cause significant pollution.


	To be notified within 24 hours of detection

	Date and Time of the event
	14:00 hrs 31st October 2016

	Reference or description of the location of the event
	Remote Leachate Monitoring Points – Liquid levels Brookhill Landfill Site. 

	Description of where any release into the environment took place 
	No leachate release was detected but observed static liquid levels are above trigger values. 

	Substances(s) potentially 
released 
	Leachate 

	Best estimate of the quantity or rate of release of substances
	No release – Engineered Containment Cell Construction.

	Measures taken, or intended to be taken, to stop any emission 
	Extra pumps or more efficient pump will be installed if possible

	Description of failure or 

accident

	R1 breach of 2m trigger limit. R5 breach of 3m trigger limit 


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	R1 & R5 remote wells 

	Parameter(s) 
	Basal Leachate head

	Limit
	As per Permit

	Measured value and uncertainty 
	Varies  2m to 4m  

	Date and time of monitoring 
	 14:00 hrs 31st October 2016

	Measures taken, or intended to be taken, to stop the emission  
	Pumps to be removed from R1 & R5  wells; will be probed using drain rods to confirm base levels and silt build up


	Time periods for notification following detection of a breach of a limit 

	Parameter 
	Notification period

	Trigger level   (Apparent breach) but doubt about reliability of data.  [Perched liquid trapped over silt]. 
	24hrs.

	
	

	
	


	( c )  Notification requirements for the detection of any significant adverse environmental effect 

	To be notified within 24 hours of detection

	Description of where the effect on
the environment was detected
	             N/A

	Substances(s) detected 
	             N/A

	Concentrations of the substances

detected  
	             N/A


	Date of monitoring / sampling
	            14:00 hrs 31st October 2016


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	 Periodic de-silting of monitoring wells.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment or harm which has been or may be caused by the emission
	 No further measures necessary

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	Long standing and known problem declared to                     th   NRW Agency.

	
	


	Name*
	P Murphy

	Post
	Landfill Manager

	Signature
	Paul Murphy


	Date
	 


* Authorised to sign on behalf of Flintshire County Council - Waste Management Service 
