Permit Number: 
EA/EPR/BK3638IF/V002

Operator: 
Hydro Aluminium Limited

Facility:
Wrexham Aluminium Works
Form Number: 
Water1
Reporting of emissions to water (other than to sewer) and land for the period from 01/07/2015 to 30/09/2015
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	W1
	BOD
	10 mg/l
	Single sample
	<1
	TM045: MEWAM BOD5 2nd Ed, HMSO 1988 / Method 5210B, AWWA/APHA, 20th ed, 1999; SCA Blue Book 130
	11:30, 12/08/15
	±6.9%

	W1
	Suspended Solids
	35 mg/l
	Single sample
	19.4
	TM022: Method 2540D, AWWA/APHA, 20th ed, 1999 / BS2690 Part 120 1981; BS EN 872
	11:30, 12/08/15
	±3%

	W1
	pH
	6 – 9
	Single sample
	7.79
	TM256:determination of pH in water using the GLpH Meter
	11:30, 12/08/15
	±0.02%

	W1
	COD
	125 mg/l
	Single sample
	18.48
	TM107: ISO6060:1989
	11:30, 12/08/15
	±1.2%

	W1
	Ammoniacal Nitrogen
	5 mg /l
	Single sample
	2.32
	TM099: BS2690 Part 7, 1968 / BS6068 Part 2.11, 1984
	11:30, 12/08/15
	±3.8%

	W1
	Aluminium
	0.5 mg/l
	Single sample
	0.08
	TM152: Method 3125B, AWWA/APHA, 20th ed, 1999
	11:30, 12/08/15
	±3.8%

	W1
	Total Hydrocarbon Oil
	2 mg/l
	Single sample
	0.33
	TM172: Analysis of petroleum hydrocarbons in environmental media
	11:30, 12/08/15
	±10.5%

	W1
	Temperature
	25 oC
	Single sample
	18 oC
	Mercury thermometer
	11:30, 12/08/15
	Not known

	W1
	Flow
	N/A
	-
	-
	-
	-
	-


Signed ……Joel Priest……………………………………………………….  

Date ……………08/10/2015………..

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4.
