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Notice of variation with introductory note
Environmental Permitting (England & Wales) Regulations 2010


Hydro Aluminium Deeside Ltd

Wrexham Aluminium Works 
Bridge Road
Wrexham Industrial Estate
Wrexham
LL13 9PS


Variation application number
EPR/BK3638IF/V004
Permit number
EPR/BK3638IF






Wrexham Aluminium Works
Permit number EPR/BK3638IF
Introductory note
This introductory note does not form a part of the notice

The following notice gives notice of the variation of an environmental permit.

This variation corrects an error in table S4.1 in schedule 4 of the permit.

The schedules of this notice specify the changes made to the original permit.

The status log of a permit sets out the permitting history, including any changes to the permit reference number.  


	Status log of the permit

	Description
	Date
	Comments

	Application BK3638
	Received 7/09/01
	

	Response to Schedule 4 Part1 Notice 11 /12/01
	Received 14/01 /02
	

	Supplementary Information
	Received 30/01/02
	Map and slight amendment to waste storage information

	Supplementary Information
	Received 25/02/02
	Further slight amendment to waste storage

	Supplementary Information
	Received 08/03/02
	Clarification regarding monitoring details

	Variation Notice EA/EPR/BK36381F/V002
	Issued 14/07/09
	Agency initiated Permit review

	Variation Application
	Received 
19/03/14
	

	Variation Notice EPR/BK3638/IF/V003
	Issued 20/06/14
	

	Variation Notice
EPR/BK3638/IF/V004
	Issued 29/04/15
	NRW initiated variation to correct table S4.1



End of introductory note
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Notice of variation 


Environmental Permitting (England and Wales) Regulations 2010
[bookmark: _Hlt13295849][bookmark: OperatorName2]
The Natural Resources Body for Wales (“Natural Resources Wales”) in exercise of its powers under regulation 20 of the Environmental Permitting (England and Wales) Regulations 2010 varies 

Permit number
EPR/BK3638IF

issued to
Hydro Aluminium Deeside Ltd (“the operator”)

whose registered office is

Bridge Road
Wrexham Industrial Estate
Wrexham
LL13 9PS

company registration number 1786117

to operate a regulated facility at

Bridge Road
Wrexham Industrial Estate
Wrexham
LL13 9PS

to the extent set out in the schedules.

The notice shall take effect from 29 April 2015

	Name
	Date

	[image: ]

	29 April 2015



Eirian Macdonald
Authorised on behalf of Natural Resources Wales

Schedule 1 – conditions to be deleted
None  

Schedule 2 – conditions to be amended 
The following conditions are amended as a result of an administrative variation initiated by Natural Resources Wales

Table S4.1 shall be amended to:


	Table S4.1  Point source emissions to air – emission limits and monitoring requirements

	Emission point ref. & location
	Parameter
	Source
	Limit (including unit) 
	Reference period
	Monitoring frequency
	Monitoring standard or method

	A1
As shown on drawing number CL(50)01/B Ref 5
	Sulphur dioxide
	Vent from bag filter plants 1 and 2
	25 mg/m3
	2 hour average
	Six monthly
	BS EN 14791

	
	Volatile Organic
Carbons (as Carbon)
	Vent from bag filter plants 1 and 2
	20 mg/m3
	4 hour 
	Six monthly
	BS EN 12619:1999

	
	Gaseous fluorides (as
HF)
	Vent from bag filter plants 1 and 2
	1 mg/m3
	-
	Six monthly
	BS ISO 15713

	
	Hydrogen chloride
	Vent from bag filter plants 1 and 2
	10 mg/m3
	-
	Six monthly
	BS EN 1911

	
	Dioxins
	Vent from bag filter plants 1 and 2
	0.1 ng/m3
	Minimum 4 hour
	Six monthly
	BS EN 1948

	
	Carbon Monoxide
	Vent from bag filter plants 1 and 2
	100 mg/m3
	-
	Six monthly
	BS EN 15058

	
	Oxides of nitrogen (as
N02)
	Vent from bag filter plants 1 and 2
	60 mg/m3
	4 hour
	Six monthly
	BS EN 14792

	
	Particulate
	Vent from bag filter plants 1 and 2
	For calibration purposes – no limit
	4 hour
	Annual
	BS EN 13284-1

	
	Particulate
	Vent from bag filter plants 1 and 2
	5 mg/m3
	Monthly average
	Continuous
	BS EN 15267-3(1)

	
	Particulate
	Vent from bag filter plants 1 and 2
	10 mg/m3
	Daily average
	Continuous
	BS EN 15267-3(1)

	A12
As shown on drawing number
CL(50)01/B Ref 6
	Sulphur dioxide
	Vent from bag filter plant 3
	25 mg/m3
	2 hour average
	Six monthly
	BS EN 14791

	
	Volatile Organic Carbons (as Carbon)
	Vent from bag filter plant 3
	20 mg/m3
	4 hour average
	Six monthly
	BS EN 12619:1999

	
	Gaseous fluorides
(as HF)
	Vent from bag filter plant 3
	1 mg/m3
	-
	Six monthly
	BS ISO 15713

	
	Hydrogen chloride
	Vent from bag filter plant 3
	10 mg/m3
	-
	Six monthly
	BS EN 1911

	
	Dioxins
	Vent from bag filter plant 3
	0.1 ng/m3
	Minimum 4 hour
	Six monthly
	BS EN 1948

	
	Carbon Monoxide
	Vent from bag filter plant 3
	100 mg/m3
	-
	Six monthly
	BS EN 15058

	
	Oxides of nitrogen
(as NO2)
	Vent from bag filter plant 3
	60 mg/m3
	4 hours
	Six monthly
	BS EN 14792

	
	Particulate
	Vent from bag filter plant 3
	For calibration purposes – no limit
	4 hours
	Annual
	BS EN 13284-1

	
	Particulate
	Vent from bag filter plant 3
	5 mg/m3
	Monthly average
	continuous
	BS EN 15267-3(1)

	
	Particulate
	Vent from bag filter plant 3
	10 mg/m3
	Daily average
	Continuous
	BS EN 15267-3(1)

	A13
As shown on drawing number CL(50)01/B Ref4
	Carbon Monoxide
	Vent from holding furnace
	150 mg/m3
	-
	Annual
	BS EN 15058

	
	Oxides of nitrogen (as NO2)
	
	60 mg/m3
	4 hour
	Annual
	BS EN 14792

	
	Particulate
	
	10 mg/m3
	Daily average
	Continuous
	BS EN 15267-3(1)

	
	Particulate
	
	For calibration purposes – no limit
	4 hours
	Annual
	BS EN 13284-1

	A15
As shown on drawing number CL(50)01/B Ref3
	N/A
	Vent from casting pit
	N/A
	N/A
	N/A
	N/A

	A16  
(NGR SJ 376 492)
	N/A
	Continuous homogeniser
	N/A
	N/A
	N/A
	N/A



Note 1: certification to the MCERTS performance standards indicates compliance with BS EN 15267-3



Schedule 3 – conditions to be added
None
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