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Tata Steel Strip Products UK

Port Talbot Steelworks

Environment Department

Response to Improvement Condition (IC6): 

For emission points A51, A53 and A62 the Operator shall submit for written approval by NRW emission limit values in accordance with Article 30 (Emission Limit Values) of the Industrial Emissions Directive post 30th June 2020.
Date 30th December 2015

Tata Steel and the NRW have been discussing the proposed emission limit values IED Post 30th June 2020 and have previously submitted proposals and submitted to the NRW in September 2014 with agreed daily limits 0f 121% ELV

The table below gives the proposed Emission Limit Values

	Boiler
	A51 Boiler 5
	A53 Mitchell Boiler
	A62 Boiler 3

	Parameter
	Parts

mg/Nm3
	SO2

mg/Nm3
	NOx

mg/Nm3
	Parts

mg/Nm3
	SO2

mg/Nm3
	NOx

mg/Nm3
	Parts

mg/Nm3
	SO2

mg/Nm3
	NOx

mg/Nm3

	LCPD Fuel-waited ELV
	15
	500
	250
	15
	300
	250
	15
	300
	200

	Daily Limit 

121% ELV
	18.2
	605
	302.5
	18.2
	605
	302.5
	18.2
	605
	242

	Annual 95% hourly mean

200% ELV
	30
	1,000
	500
	30
	1,000
	500
	30
	600
	400


