Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V012

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	24/08/15  15:10


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	23/08/15  19:50

	Reference or description of the location of the event 
	Kiln feed/Pre-Heater Tower

	Description of where any release into the environment took place
	A damper due to a short term build-up of positive pressure in PHT/Filter system

	Substances(s) potentially released
	Raw meal and gases.

	Best estimate of the quantity or rate of  release of substances
	Short term event estimated at 25-50Kg of material and fumes

	Measures taken, or intended to be taken, to stop any emission
	Kiln conditions bought under control and negative pressure restored

	Description of the failure or accident.
	Unstable kiln conditions


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	The area of from which the emission was found is a slide damper (SD01)  in ducting that carries hot gasses (circa 300-400oC) from the kiln through to the raw mill,  where it is used to dry the raw materials in the mill, rather than a dedicated material transfer line.
The Kiln Operator was trying to balance the negative pressures through the kiln system but the position of this hole is not obvious from the trends available in the control room. 

Whilst going through the process of stabilising the system there was a short period of positive pressure which forced the gas stream to exit through the damaged damper.

Further investigations were undertaken as to how the gas stream had been able to exit the ducting and damper system. This revealed that the damper casing had been holed. 


	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	As this is not directly in the gas flow it isn’t considered a high risk maintenance area and therefore is only inspected in shut downs when access to this area can be carried out when the system is cool.
Hole in the damper was patched we have not experienced issues with its operation since, however additional work is scheduled for the full January 2016 shutdown as a preventative measure.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	Emission of dust was short lived and dissipated rapidly with minimal environmental effect.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	19/09/13

13/04/14

06/02/15

17/07/15

27/09/13

02/09/14

01/04/15

23/08/15

10/10/13

06/09/14

06/07/15

16/11/13

21/01/15

15/07/15




	Name* 
	Victoria Smith

	Post  
	Quality and Environment Manager

	Signature 
	

	Date 
	27/08/15


* authorised to sign on behalf of Castle Cement Limited
