Schedule 5 - Notification 

This page outlines the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	CB3432AA

	Name of operator
	3C Waste Ltd

	Location of Installation
	Llanddulas Composting Facility

	Time and date of the detection 
	23rd June  2016


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	N/A

	Reference or description of the location of the event 
	N/A

	Description of where any release into the environment took place
	N/A

	Substances(s) potentially released
	N/A

	Best estimate of the quantity or rate of  release of substances
	N/A

	Measures taken, or intended to be taken, to stop any emission
	N/A

	Description of the failure or accident.
	N/A


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	100 – 150m South of the pad boundary on the track that surrounds the quarry surface. Grid reference SH 90287 77018

	Parameter(s)
	Mesophilic Bacteria

	Limit
	Total Bacteria = 1000 cfu/m3 (Table S3.2 of Permit)

	Measured value and uncertainty
	SP2 Mesophilic Bacteria = 2333 cfu/m3

	Date and time of monitoring
	23rd June2016

	Measures taken, or intended to be taken, to stop the emission
	All samples and locations were below the permit thresholds apart from SP2 which had a slightly elevated result for Mesophilic Bacteria but mean results for Asperigillus Fumigatus were within acceptable levels.

We plan to undertake the next quarterly monitoring in September


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	N/A

	Substances(s) detected
	N/A

	Concentrations of substances detected
	N/A

	Date of monitoring/sampling
	N/A


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	N/A

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	 The composting process will continue to be operated in accordance with the sites working plan, odour management plan and site specific bioaerosol risk assessment

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	N/A

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	12/12/14, 09/06/15,  08/09/2015 and 17/03/16

	Name*
	Chris Bennion

	Post
	Site Business Manager

	Signature
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	Date
	4th July 2016


*authorised to sign on behalf of 3C Waste Ltd
