Permit Reference Number: BR7321





Operator: Tata Steel Colors
Installation: Tata Steel Colors Shotton Works




Form Number: E1

Reporting of Energy Usage for the year ……2014

	Energy Source
	Energy Usage
	CO2
Produced

(tonnes)
	
	Trends in Energy Usage

	
	Quantity
	Primary Energy

(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy usage
	CO2

produced
	CO2 per

MWh

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	2005
	662658 MWh
	127741 Tonnes
	0.193 T/MWh

	Electricity *
	MWh
	174,143
	28,734
	
	2006
	728829 MWh
	134225 Tonnes
	0.184 T/MWh

	Natural Gas
	GJ
	1,104,366
	62,688
	
	2007
	662742 MWh
	121571 Tonnes
	0.183 T/MWh

	Gas Oil
	Tonnes
	
	
	
	2008
	583065 MWh
	113566 Tonnes
	0.194 T/MWh

	
	
	
	
	
	2009
	487,380 MWh
	93480 Tonnes
	0.191 T/MWh

	TOTAL
	-
	483,365
	91,422
	
	2010
	494,226 MWh
	94789 Tonnes
	0.191 T/MWh

	
	
	
	
	
	2011
	478,530 MWh
	91472 Tonnes
	0.191 T/MWh

	
	
	
	
	
	2012
	422,833 MWh
	76,541 Tonnes
	0.181 T/MWh

	
	
	
	
	
	2013
	478,857 MWh
	90,552 Tonnes
	0.189 T/MWh

	
	
	
	
	
	2014
	483,365 MWh
	91,422 Tonnes
	0.189 T/MWh


* Conversion factor for delivered electricity to primary energy = 2.6

	Operator’s comments :

Gas and Electricity emission factors taken from Environment Agency’s IPPC H2 – Energy Efficiency Horizontal guidance Note.

Oil emission factors taken from EU ETS Emissions factors




Signed ………………P. Shephard…………………………………………….  

Date……31/01/15…………………..




(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Tata Steel Colors
Installation: Tata Steel Colors Shotton Works




Form Number: WU1

Reporting of Water Usage for the year - 2014

	Water Source
	Usage

(m3)
	Specific Usage 

(m3/t)
	
	Trends in Water Usage

	
	
	
	
	Year
	Parameter

	
	
	
	
	
	Potable 

Water 
	Non-Potable 

Water  
	Water per unit output

	Mains water
	484538
	0.54
	
	
	
	
	

	Site borehole
	0
	0
	
	2004
	263,427
	1,642,412
	1.69

	River abstraction
	
	
	
	2005
	206,477
	1,191,544
	1.30

	
	
	
	
	2006
	333,940
	1,013,508
	1.17

	
	
	
	
	2007
	120,066
	881,258 (FWD)

12,341 (Boreholes)
	1.04

	TOTAL WATER USAGE
	484538
	
	
	2008
	155,875
	736,049 (FWD)

32,572 (Boreholes)
	0.91

	
	
	
	
	2009
	117,015
	494,822 (FWD)

122,823 (boreholes)
	1.10

	
	
	
	
	2010
	98791
	539,728 (FWD)

42,786 (borehole)
	0.89

	
	
	
	
	2011
	159408
	548670 (FWD)
	0.93

	
	
	
	
	2012
	218611
	448102 (FWD)
	0.92

	
	
	
	
	2013
	134807
	323765 (FWD)
	0.53

	
	
	
	
	2014
	132222
	352316 (FWD)
	0.54


	Operator’s comments :

Note: 


Signed ………… P. Shephard ………………………………………………….  

Date………31/01/15………………..




(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Tata Steel Colors
Installation: Tata Steel Colors Shotton Works




Form Number: R1

Reporting of Waste Disposal and Recovery for the year 2014

	Waste

Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes
	Tonnes
	
	Year
	Parameter

	
	
	
	
	
	
	Total Hazardous 

Waste
	Total Non-Hazardous

Waste
	Waste per unit output

	1) Hazardous Wastes
	
	
	
	
	2004
	1041.02
	6096.01
	0.006

	Chromate
	licenced contractor
	326.9
	
	
	2005
	1356.52
	3800.49
	0.0049

	Oil
	licenced contractor
	6.92
	6.92
	
	2006
	1513.74
	4321.23
	0.0051

	Dry Oily Waste
	licenced contractor
	0.96
	
	
	2007
	1247.52
	4003.59
	0.0049

	Solvent/paint
	licenced contractor
	1050.42
	997.73
	
	2008
	1367.9
	4182.34
	0.0055

	Clinical waste
	licenced contractor
	0.252
	
	
	2009
	1250.569
	7380.59
	0.013

	Batteries
	licenced contractor
	2.31
	
	
	2010
	1428.36
	10325
	0.015

	WEEE
	licenced contractor
	9.4
	9.4
	
	2011
	1952.83
	11273
	0.015

	Other hazardous wastes
	licenced contractor
	73.63
	52.66
	
	2012
	1422.88
	10215.212
	0.016

	Total hazardous waste
	
	1470.79
	
	
	2013
	1176.11
	13091.69
	0.016

	2) Non-Hazardous Wastes
	
	
	
	
	2014
	1470.79
	12464.967
	0.016

	Filtercake
	Landfill
	725.52
	410.36
	
	
	
	
	

	Office waste/ General Skip Waste
	Internal Landfill
	447.16
	
	
	
	
	
	

	Construction / demolition waste
	Internal Landfill
	42.82
	
	
	
	
	
	

	Paper/cardboard/plastic
	licenced contractor
	43.54
	43.54
	
	
	
	
	

	Zinc Dross
	licenced contractor
	971.64
	971.64
	
	
	
	
	

	Waste Drums
	licenced contractor
	0
	
	
	
	
	
	

	Metals
	licenced contractor
	9727.86
	9727.86
	
	
	
	
	

	Other non-hazardous wastes
	licenced contractor
	506.43
	429.62
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	Total non-hazardous waste
	
	12464.967
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	TOTAL WASTE
	
	13935.76
	
	
	
	
	
	


Signed ……………… P. Shephard …………………………………………….  

Date………31/01/15………………..




(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Tata Steel Colors
Installation: Tata Steel Colors Shotton Works




Form Number: PI1

Reporting of Performance Indicators for the year  2014

	Annual Production/Treatment

	Production of galvanised steel product
	609849 tonnes

	Production of colour coated steel product 
	277163  tonnes

	Total Production of coated steel products
	887012  tonnes


Environmental Performance Indicators

	Parameter
	Annual Average
	Units
	
	Trends in Environmental Performance

	
	
	
	
	Year
	Parameter

	
	
	
	
	
	Total VOC / tonne 
	% VOC Fugitives
	Primary Energy / tonne

	Primary Energy Use 
	483,365
	MW-hr /  tonne
	
	
	
	
	

	Total VOC Emission to Air (as Carbon)
	0.24
	Kg /  tonne
	
	2004
	0.13
	2.75
	0.66

	VOC Fugitive Emission Value
	4.87
	%
	
	2005
	0.145
	2.83
	0.615

	Potable Water Use
	0.14
	m3 / tonne
	
	2006
	0.137
	2.87
	0.635

	Non-Potable Water Use
	0.39
	m3 / tonne
	
	2007
	0.15
	2.92
	0.620

	Quantity of Hazardous Waste
	1.65
	Kg / tonne
	
	2008
	0.05
	2.43
	0.65

	Quantity of Non-Hazardous Waste
	14.0
	Kg / tonne
	
	2009
	0.157
	9.11
	0.73

	
	
	
	
	2010
	0.159
	10.2
	0.65

	
	
	
	
	2011
	0.07
	4.86
	0.61

	
	
	
	
	2012
	0.05
	3.13
	0.59

	
	
	
	
	2013
	0.05
	3.57
	0.561

	
	
	
	
	2014
	0.07
	4.87
	0.54


	Operator’s comments :




Signed …………… P. Shephard ……………………………………………….  

Date………31/01/15………………..

(authorised to sign as representative of the Operator)

